{"text_format":"3","workbook":"xlsx","n_sheets":24,"sheets":["LCM List 2026","Capacitive Touch Display","Resistive Touch Display","High-brightness TFT","Wide Temp TFT","Square TFT","Round TFT","Bartype TFT","Transflective TFT","Reflective TFT","Blanview TFT","Flexible AM-OLED Display","AM-OLED Display","PM-OLED Display","Mini-LED","HDMI TFT","HDMI AMOLED","Type-C TFT","UART TFT","E-Paper Display","LTPS TFT","Curved Monitor","Display Monitor","OLED Monitor"],"not_rendered":{"images":3,"defined_names":22},"read":"whole","date_system":"1900"}

{"sheet":"LCM List 2026","index":0,"n_rows":1463,"n_cols":13,"rows_kept":1463}
["STARTEK LCM Product List 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.91”","KD0091SQOIN001","PDF","128x32","i2C","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","38.00*12.00*3.80","22.38*5.58","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["0.95”","KD0095OLEDN010","PDF","120x240","SPI","RM69310","Free V.A","No TP","-20℃~70℃","450 nits","12.80*27.35*0.74","10.80*21.60","AMOLED Display,Bartype TFT,LTPS Display"]
["0.96”","KD0096SHFSD006-02","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["0.96”","KD0096SQOSN009","PDF","128x64","SPI","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","27.30*27.80*4.10","21.74*10.86","PMOLED Display,Wide Temp TFT"]
["0.96”","KD0096FM-1","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","500 nits","13.50*27.95*1.50","10.80*21.70"]
["0.96”","KD0096SQOSN012","PDF","128x64","SPI/IIC","SSD1315","Free V.A","No TP","-40℃~85℃","80 nits","24.70*16.60*1.30","21.74*11.18","PMOLED Display,Wide Temp TFT"]
["0.96”","KD0096SHFSD006-a","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["1.0”","KD010LQOSN001-C0000","PDF","340x340","QSPI","SH8601","Free V.A","CTP","-10℃~60℃","630 nits","29.25*30.00*0.68","26.35*26.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.1”","KD011SQOSN002","PDF","64x128","SPI","CH1115","Free V.A","No TP","-40℃~70℃","180 nits","24.00*33.00*3.80","10.86*25.58","PMOLED Display,Wide Temp TFT"]
["1.3”","KD013QVFMD010","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","26.16*29.22*1.79","23.40*23.40","Square TFT"]
["1.3”","KD013QVFMD002-01","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","450 nits","35.90*39.70*1.39","32.40*32.40","Round TFT"]
["1.3”","KD013QCFSN015","PDF","144x200","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","24.69*36.64*0.95","19.44*27.00","E-Paper Display"]
["1.3”","KD013SQOIN012","PDF","128x64","i2C","SH1106","Free V.A","No TP","-40℃~70℃","150 nits","35.40*33.50*4.00","29.42*14.70","PMOLED Display,Wide Temp TFT"]
["1.3”","KD013QVFMD007A","PDF","240x240","SPI&MCU&RGB","GC9A01","Free V.A","No TP","-20℃~70℃","500 nits","35.60*37.74*1.48","32.40*32.40","Round TFT"]
["1.3”","KD013QVFMD002-03","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","450 nits","35.90*39.70*1.39","32.40*32.40","Round TFT"]
["1.3”","KD013QVFMD010A","PDF","240x240","SPI&MCU&RGB","ST7789T3-G4-1","Free V.A","No TP","-20℃~70℃","550 nits","26.16*29.22*1.79","23.40*23.40","Square TFT"]
["1.4”","KD014VGOSN001-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","650 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.4”","KD014HVOIN011-C0000","PDF","320x360","MIPI","FT2390","Free V.A","CTP","-20℃~60℃","450 nits","25.74*29.87*0.79","23.84*26.82","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.44”","KD014QQTBN002","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","No TP","-20℃~70℃","800 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.44”","KD014QQTBN002-TP","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","RTP","-20℃~70℃","640 nits","32.36*38.00*4.20","25.50*26.50","Resistive Touch Display,Square TFT"]
["1.44”","KD014QQFBN006","PDF","128x128","SPI&MCU","ST7735S","Free V.A","No TP","-20℃~70℃","950 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.44”","KD014QQTBN001-01","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","No TP","-20℃~70℃","200 nits","32.36*38.00*2.60","25.50*26.50","Square TFT"]
["1.5”","KD015QVFMN002-C001B","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","320 nits","37.52*41.10*4.45","27.72*27.72","Capacitive Touch Display,Square TFT"]
["1.5”","KD015QVFMN002","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","33.32*36.06*2.25","27.72*27.72","Square TFT"]
["1.5”","KD015SQOSN013","PDF","128x128","SPI","SH1107","Free V.A","No TP","-40℃~70℃","100 nits","34.00*49.30*5.00","26.86*26.86","PMOLED Display,Wide Temp TFT"]
["1.5”","KD015QVFMD020-C001D","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","800 nits","37.52*41.10*3.82","27.72*27.72","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["1.54”","KD0154WEOLN006","PDF","128x64","Parallel/SPI/I2C","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","42.04*27.22*1.46","35.04*17.51","PMOLED Display,Wide Temp TFT"]
["1.54”","KD015QVFSN012","PDF","152x152","SPI","SSD1681","Free V.A","No TP","0℃~50℃","0 nit","31.80*37.32*1.14","27.51*27.51","Square TFT,E-Paper Display"]
["1.54”","KD015QVFSN015","PDF","200x200","SPI","SSD1681","Free V.A","No TP","0℃~40℃","0 nit","31.80*37.32*1.00","27.00*27.00","Square TFT,E-Paper Display"]
["1.6”","KD016WVFID001","PDF","400x400","MIPI","ST7797","Free V.A","No TP","-20℃~70℃","350 nits","42.94*45.89*1.94","39.84*39.84","Round TFT"]
["1.6”","KD016HVOMN002-C001A","PDF","320x360","MIPI&SPI","RM69092","Free V.A","CTP","-20℃~70℃","320 nits","31.32*36.05*2.05","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016WVFID001-C002A","PDF","400x400","MIPI","ST7797","Free V.A","CTP","-20℃~70℃","350 nits","51.94*52.94*3.09","39.84*39.84","Capacitive Touch Display,Round TFT"]
["1.6”","KD016HVOQN006-C000O","PDF","320x360","QSPI","RM69092","Free V.A","CTP","-20℃~70℃","450 nits","28.92*33.35*0.76","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.7”","KD017SQOIN003","PDF","128x32","i2C","SSD1312","Free V.A","No TP","-40℃~70℃","120 nits","60.50*18.75*4.95","42.22*10.54","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["1.75”","KD018LQRMN029","PDF","296x222","MCU","ILI9342C","Free V.A","No TP","-20℃~70℃","350 nits","42.07*39.71*2.50","35.52*26.64","Transflective TFT"]
["1.75”","KD018LQRBD028","PDF","296x222","MCU","ILI9342C","Free V.A","No TP","-20℃~70℃","320 nits","40.80*36.20*2.26","35.52*26.64","Transflective TFT"]
["1.77”","KD018C-2","PDF","128x160","SPI&MCU","ILI9163V","V.A 12H","No TP","-20℃~70℃","300 nits","34.00*47.00*2.40","28.03*35.04"]
["1.77”","KD018C-2-TP","PDF","128x160","SPI&MCU&RGB","ILI9163V","V.A 12H","RTP","-20℃~70℃","280 nits","34.00*47.00*3.60","28.03*35.04","Resistive Touch Display"]
["1.77”","KD018QQTBN009","PDF","128x160","SPI&MCU","ST7735S","V.A 12H","No TP","-20℃~70℃","450 nits","34.70*46.70*2.50","28.03*35.04"]
["1.77”","KD018QQTBN009-RT","PDF","128x160","SPI&MCU","ST7735S","V.A 12H","RTP","-20℃~70℃","330 nits","34.70*46.70*3.55","28.03*35.04","Resistive Touch Display"]
["1.77”","KD018QVFIN016","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","500 nits","34.70*46.70*2.50","26.64*35.52"]
["1.77”","KD018QVFIN016-C001A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","450 nits","39.70*52.50*4.85","26.64*35.52","Capacitive Touch Display"]
["1.77”","KD018QVFMN010-02-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","300 nits","34.70*46.70*3.55","26.64*35.52","Resistive Touch Display"]
["1.77”","KD018QVFPN013","PDF","240x320","SPI+RGB","ST7789V","Free V.A","No TP","-20℃~70℃","430 nits","34.70*46.70*2.50","26.64*35.52"]
["1.77”","KD018QQTBN009-C002A","PDF","128x160","SPI&MCU","ST7735S","V.A 12H","CTP","-20℃~70℃","400 nits","39.70*52.50*4.25","28.03*35.04","Capacitive Touch Display"]
["1.77”","KD018QVFMN010-02","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","34.70*46.70*3.55","26.64*35.52"]
["1.77”","KD018QVFMN010-02-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","200 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*4.85","26.64*35.52","Capacitive Touch Display"]
["1.78”","KD017HVOSN005-C000","PDF","368x448","QSPI/SPI","CO5300","Free V.A","CTP","-20℃~60℃","450 nits","33.50*40.89*2.58","28.70*34.94","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.8”","KD018HVFMD042","PDF","360x360","MCU/SPI/QSPI","ST77916","Free V.A","No TP","-20℃~70℃","800 nits","48.08*49.95*1.94","45.68*45.68","High-brightness TFT,Round TFT"]
["1.96”","KD019HVOSN001-C001A","PDF","410x502","QSPI","CO5300AF-46","Free V.A","CTP","-10℃~60℃","600 nits","35.37*42.40*2.76","31.37*38.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.0”","KD020QVRMA028","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","260 nits","35.80*52.10*2.65","30.60*40.80","Transflective TFT"]
["2.0”","KD020QVTMA008-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","400 nits","35.80*52.10*3.75","30.60*40.80","Resistive Touch Display"]
["2.0”","KD020LQFMA014","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","No TP","-20℃~70℃","600 nits","46.50*41.56*2.50","40.80*30.60"]
["2.0”","KD020LQFMA014-C003A","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","CTP","-20℃~70℃","550 nits","54.50*47.56*4.15","40.80*30.60","Capacitive Touch Display"]
["2.0”","KD019QQFBN002-C001A","PDF","128x160","SPI&MCU","ST7735","Free V.A","CTP","-20℃~70℃","900 nits","47.47*59.04*3.20","31.87*39.84","Capacitive Touch Display,High-brightness TFT"]
["2.0”","KD020LQFMA014-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","RTP","-20℃~70℃","540 nits","46.50*41.56*3.70","40.80*30.60","Resistive Touch Display"]
["2.0”","KD020QVFIA013","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","600 nits","35.80*52.10*2.65","30.60*40.80"]
["2.0”","KD020QVFMA009","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","480 nits","35.80*52.10*2.65","30.60*40.80"]
["2.0”","KD020QVFMA009-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","400 nits","35.80*52.10*3.77","30.60*40.80","Resistive Touch Display"]
["2.0”","KD020QVFIA013-C001A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","550 nits","35.80*52.10*4.40","30.60*40.80","Capacitive Touch Display"]
["2.0”","KD019QQFBN002","PDF","128x160","SPI&MCU","ST7735","Free V.A","No TP","-20℃~70℃","1000 nits","37.47*49.04*2.02","31.87*39.84","High-brightness TFT"]
["2.0”","KD020QCTBN019","PDF","176x220","MCU","ST7775R","V.A 12H","No TP","-20℃~70℃","530 nits","38.40*51.40*2.35","31.68*39.60"]
["2.0”","KD020QCTBN019-TP","PDF","176x220","MCU","ST7775R","V.A 12H","RTP","-20℃~70℃","480 nits","38.40*51.40*3.56","31.68*39.60","Resistive Touch Display"]
["2.0”","KD020QCTBN020","PDF","176x220","SPI&MCU&RGB","ST7775R","V.A 12H","No TP","-20℃~70℃","400 nits","38.40*51.40*2.35","31.68*39.60"]
["2.0”","KD020QCTBN020-TP","PDF","176x220","SPI&MCU&RGB","ST7775R","V.A 12H","RTP","-20℃~70℃","380 nits","38.40*51.40*3.56","31.68*39.60","Resistive Touch Display"]
["2.0”","KD020LQRMA017","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","No TP","-20℃~70℃","350 nits","46.50*41.56*2.70","40.80*30.60","Transflective TFT"]
["2.0”","KD020LQRMA017-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","RTP","-20℃~70℃","280 nits","46.50*41.56*3.90","40.80*30.60","Resistive Touch Display,Transflective TFT"]
["2.0”","KD020LQRMA017-C003A","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","CTP","-20℃~70℃","300 nits","54.50*47.56*4.35","40.80*30.60","Capacitive Touch Display,Transflective TFT"]
["2.0”","KD020WQFPA023-RT","PDF","480x360","SPI+RGB","ST7701S","Free V.A","RTP","-30℃~85℃","900 nits","46.50*41.56*3.70","40.82*30.62","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023","PDF","480x360","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024","PDF","480x360","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","900 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023-C003B","PDF","480x360","SPI+RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024-C003B","PDF","480x360","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","820 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD019QQFBN002-RT","PDF","128x160","SPI&MCU","ST7735","Free V.A","RTP","-20℃~70℃","800 nits","37.47*49.04*3.22","31.87*39.84","Resistive Touch Display,High-brightness TFT"]
["2.0”","KD020QVTMA008","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","500 nits","35.80*52.10*2.65","30.60*40.80"]
["2.0”","KD020QVRMA028-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","200 nits","35.80*52.10*3.85","30.60*40.80","Resistive Touch Display,Transflective TFT"]
["2.0”","KD020LQFMA014-C003A-RS232","PDF","320x240","RS232","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-RS485","PDF","320x240","RS485","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-TTL","PDF","320x240","TTL","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020VGFPA038","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","No TP","-30℃~85℃","700 nits","35.80*52.10*2.65","30.60*40.80","Wide Temp TFT"]
["2.0”","KD020VGFIA039","PDF","480x640","MIPI","ST7701SI","Free V.A","No TP","-30℃~85℃","700 nits","35.80*52.10*2.65","30.60*40.80","Wide Temp TFT"]
["2.0”","KD020WQFPA023-C003B-RS232","PDF","480x360","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS485","PDF","480x360","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020WQFPA023-C003B-TTL","PDF","480x360","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020QVFMA009-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020QVFMA009-C008A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","420 nits","35.80*52.10*2.65","30.60*40.80","Capacitive Touch Display"]
["2.06”","KD020HVOSN001","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","34.79*43.14*0.78","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001-C001A","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","36.70*44.21*2.55","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002-C002B","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","550 nits","37.35*45.15*2.31","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","600 nits","34.79*43.14*0.83","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.1”","KD021WVFID002-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFPD003-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFID002","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021WVFPD003","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021SCOIN007","PDF","256x64","i2C","SH1122","Free V.A","No TP","-40℃~70℃","150 nits","72.50*27.24*5.10","51.18*12.78","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.1”","KD021WVFPD003-02","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","56.18*59.71*2.24","53.28*53.28","High-brightness TFT,Round TFT"]
["2.1”","KD021WVFPD011","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","650 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021WVFPD011-C001A","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVOSN009-C003B","PDF","480x480","QSPI","CO5300AF","Free V.A","CTP","-20℃~60℃","600 nits","42.39*42.39*2.55","38.39*38.39","Capacitive Touch Display,AMOLED Display,Square TFT,LTPS Display"]
["2.13”","KD021QVFSN006","PDF","122x250","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","29.20*59.20*1.00","23.70*48.55","E-Paper Display"]
["2.13”","KD021QVFSN005","PDF","122x250","SPI","UC8251","Free V.A","No TP","0℃~50℃","0 nit","29.20*59.20*1.14","23.70*48.55","E-Paper Display"]
["2.2”","KD022QVTID022","PDF","240x320","MIPI","JD9852","V.A 6H","No TP","-20℃~70℃","450 nits","41.70*56.16*2.60","33.84*45.12"]
["2.2”","KD022QVTBD032","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","280 nits","41.70*56.16*2.60","33.48*45.64"]
["2.2”","KD022QVTBD032-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","220 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVTPD005","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","280 nits","41.70*56.16*2.60","33.84*45.12"]
["2.2”","KD022QVTPD005-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","220 nits","41.70*56.16*3.80","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTPD006","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","220 nits","41.70*56.16*2.60","33.84*45.12"]
["2.2”","KD022QVTPD006-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","170 nits","41.70*56.16*3.80","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVFBD014","PDF","240x320","MCU","R61516","Free V.A","No TP","-20℃~70℃","450 nits","41.70*56.16*2.60","33.84*45.12"]
["2.2”","KD022QVFMD018","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","700 nits","41.70*56.16*2.60","33.84*45.12"]
["2.2”","KD022SQOSN037","PDF","128x32","SPI/IIC","SSD1305","Free V.A","No TP","-40℃~70℃","120 nits","74.00*30.00*8.20","55.02*13.10","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.2”","KD022QVTBD031","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","400 nits","41.70*56.16*2.60","33.48*44.64"]
["2.2”","KD022QVTBD033","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","280 nits","41.70*56.16*2.60","33.48*44.64"]
["2.2”","KD022QVTBD024A","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","1000 nits","41.70*56.16*2.72","33.48*44.64","High-brightness TFT"]
["2.2”","KD022QVTBD031-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","400 nits","41.70*56.16*3.70","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVTBD024A-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","900 nits","41.70*56.16*3.70","33.48*44.64","Resistive Touch Display,High-brightness TFT"]
["2.2”","KD022QVTBD032-C002A","PDF","240x320","MCU","ST7789V","V.A 6H","CTP","-20℃~70℃","240 nits","41.70*56.16*4.63","33.48*44.64","Capacitive Touch Display"]
["2.2”","KD022QVFBD014-RT","PDF","240x320","MCU","ER61516","Free V.A","RTP","-20℃~70℃","450 nits","41.70*56.16*3.85","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVFMD018-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVTPD039","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","300 nits","41.70*56.16*2.60","33.48*44.64"]
["2.2”","KD022QVTPD040","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","220 nits","41.70*56.16*2.60","33.48*44.64"]
["2.2”","KD022QVTPD040-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","170 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVFMD018-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","510 nits","41.70*56.16*3.85","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTPD039-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","240 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.3”","KD023C-1","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","No TP","-20℃~70℃","350 nits","52.35*46.35*2.60","46.75*35.06"]
["2.3”","KD023C-1-TP","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","RTP","-20℃~70℃","350 nits","52.35*46.35*3.80","46.75*35.06","Resistive Touch Display"]
["2.3”","KD023C-1-C004A","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","CTP","-20℃~70℃","280 nits","55.20*51.60*4.18","46.75*35.06","Capacitive Touch Display"]
["2.4”","KD024QVFIA073","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","550 nits","42.92*60.26*2.50","36.72*48.96"]
["2.4”","KD024B-3C","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-20℃~70℃","400 nits","42.72*60.26*2.10","36.72*48.96"]
["2.4”","KD024B-3C-TP","PDF","240x320","MCU","ST7789V","Free V.A","RTP","-20℃~70℃","350 nits","42.72*60.26*3.50","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024C-1H","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","550 nits","42.72*60.26*2.60","36.72*48.96"]
["2.4”","KD024C-1H-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","500 nits","42.72*60.26*3.80","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFIA073-02-C021B","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","48.72*70.26*3.95","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","42.92*60.26*2.50","36.72*48.96"]
["2.4”","KD024HVFID078-01","PDF","320x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","600 nits","39.52*60.68*2.30","33.12*49.68"]
["2.4”","KD024HVFPD079-01","PDF","320x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","700 nits","39.52*60.68*2.30","33.12*49.68"]
["2.4”","KD024QVFIA073-C009A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*4.25","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFIA073-C021A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","48.72*70.26*4.25","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits","42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","450 nits","42.92*60.26*3.78","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFMA021","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","42.92*60.26*2.50","36.72*48.96"]
["2.4”","KD024QVFMA021-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","450 nits","42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA021-RT","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","480 nits","42.92*60.26*3.78","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFMD012","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","42.72*60.26*2.10","36.72*48.96"]
["2.4”","KD024QVFMD012-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","400 nits","42.72*60.26*3.30","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVRBA050","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-20℃~70℃","170 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA041A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","300 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA041A-C012A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","300 nits","42.92*60.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024QVRMA041A-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","290 nits","42.92*60.26*3.55","36.72*48.96","Resistive Touch Display,Transflective TFT"]
["2.4”","KD024HVFID078-01-C029A","PDF","320x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","44.52*69.88*4.38","33.12*49.68","Capacitive Touch Display"]
["2.4”","KD024HVFPD079-01-C029A","PDF","320x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","700 nits","44.52*69.88*4.38","33.12*49.68","Capacitive Touch Display"]
["2.4”","KD024HVFMA089","PDF","320x426","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","650 nits","42.92*60.26*2.50","36.72*48.88"]
["2.4”","KD024WVFLD101","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024VGFPD094","PDF","480x640","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFPD094A-RT","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","RTP","-30℃~80℃","680 nits","42.92*60.26*3.30","36.72*48.96","Resistive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFPD094-C021D","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFID095","PDF","480x640","MIPI","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFID095-C021D","PDF","480x640","MIPI","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024SQOSN132","PDF","128x64","SPI","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","72.00*43.00*7.00","55.01*27.49","PMOLED Display,Wide Temp TFT"]
["2.4”","KD024VGFPD094-C021D-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA021-C003B","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","350 nits","48.72*70.26*4.03","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVRMD137","PDF","240x320","SPI&MCU&RGB","ST7789T3-G4-1","V.A 6H","No TP","-20℃~70℃","250 nits","42.72*60.26*2.63","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVFMA020-06-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits"," 42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-C009A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVRMA038A-C015A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","220 nits","48.72*70.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024QVRMA138","PDF","240x320","SPI&MCU&RGB","ST7789T3-G4-1","V.A 3H","No TP","-20℃~70℃","350 nits","42.92*60.26*2.46","36.72*48.96","Transflective TFT"]
["2.4”","KD024WQFID142","PDF","272x480","MIPI","ST7797","Free V.A","No TP","-20℃~70℃","600 nits","33.89*60.32*2.06","30.19*53.28"]
["2.4”","KD024VGFPD094-C042A","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","900 nits","42.92*60.26*3.95","36.72*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024WQFMD146","PDF","222x480","SPI&MCU&RGB","ST7797","Free V.A","No TP","-20℃~70℃","550 nits","30.3*63.11*2.11","25.51*55.15"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.4”","KD024HVFMA089-TP","PDF","320x426","SPI&MCU&RGB","ST7796","Free V.A","RTP","-20℃~70℃","550 nits","42.92*60.26*3.78","36.72*48.88","Resistive Touch Display"]
["2.4”","KD024WVFPD102-C001A-RS232","PDF","800x480","RS232","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-RS485","PDF","800x480","RS485","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-TTL","PDF","800x480","TTL","HX8283-A","Free V.A","CTP","-20℃~70℃","670 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,UART TFT"]
["2.4”","KD024HVFMA090","PDF","320x426","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","450 nits","42.92*60.26*2.50","36.72*48.88"]
["2.4”","KD024QVFIA073-03-C009B","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","550 nits","42.92*60.26*3.53","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024WVFLD101A","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101A-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024VGFPD094-C021D-SP002A-HDMI","PDF","480x640","HDMI","ST7701SI","Free V.A","CTP","-20℃~70℃","700 nits","48.72*70.26*20.00","36.72*48.96","Capacitive Touch Display,HDMI TFT"]
["2.4”","KD024WVFPD102A","PDF","800x480","RGB","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102A-C001A","PDF","800x480","RGB","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024QVRMA038A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","250 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.4”","KD024EGOIN152-01","PDF","450x600","MCU/MIPI","RM690B0","Free V.A","No TP","-20℃~80℃","800 nits","38.72*51.56*1.00","36.72*48.96","AMOLED Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024QVFPA077","PDF","240x320","SPI+RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","42.92*60.26*2.50","36.72*48.96"]
["2.47”","KD024HVFID076","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-10℃~60℃","430 nits","69.19*71.74*2.50","62.64*62.64","Round TFT"]
["2.47”","KD024HVFPD088","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~70℃","480 nits","69.19*71.74*2.50","62.64*62.64","Round TFT"]
["2.5”","KD025EGOIN002-C000","PDF","400x712","MIPI","RM690C0","Free V.A","CTP","-20℃~70℃","800 nits","32.90*58.56*2.00","31.10*55.36","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["2.6”","KD026QVFID015","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","430 nits","46.00*64.00*2.60","39.60*52.80"]
["2.6”","KD026HVRMA010-TP","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","RTP","-30℃~85℃","430 nits","46.76*65.85*3.91","39.84*53.78","Resistive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026QVFBD001","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-20℃~70℃","300 nits","46.00*64.00*2.60","39.60*52.80"]
["2.6”","KD026HVRIA009","PDF","320x432","MIPI","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRMA010","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026LQTMA008","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","No TP","-20℃~70℃","300 nits","60.30*51.15*2.60","52.80*39.60"]
["2.6”","KD026LQTMA008-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","RTP","-20℃~70℃","240 nits","60.30*51.15*3.80","52.80*39.60","Resistive Touch Display"]
["2.6”","KD026QVFMD007","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","300 nits","46.00*64.00*2.60","39.60*52.80"]
["2.6”","KD026QVFMD007-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","240 nits","46.00*64.00*3.80","39.60*52.80","Resistive Touch Display"]
["2.6”","KD026QVFMD007-C006A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits","46.00*64.00*4.08","39.60*52.80","Capacitive Touch Display"]
["2.6”","KD026LQTMA008-C001A","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","CTP","-20℃~70℃","270 nits","60.30*51.15*4.05","52.80*39.60","Capacitive Touch Display"]
["2.6”","KD026WXFLD022","PDF","1280x720","LVDS","SC5014","Free V.A","No TP","-20℃~70℃","1300 nits","63.88*43.46*2.74","57.60*32.40","High-brightness TFT"]
["2.6”","KD026WXFLD022-C008A","PDF","1280x720","LVDS","SC5014","Free V.A","CTP","-20℃~70℃","1200 nits","73.88*53.46*4.37","57.60*32.40","Capacitive Touch Display,High-brightness TFT"]
["2.6”","KD026HVRMA010-C004B","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","CTP","-30℃~85℃","420 nits","46.76*65.85*4.26","39.84*53.78","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026WXFLD022-C008A-RS232","PDF","1280x720","RS232","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-TTL","PDF","1280x720","TTL","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-RS485","PDF","1280x720","RS485","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.7”","KD027QVFSN007","PDF","152x296","SPI","UC8251","Free V.A","No TP","0℃~50℃","0 nit","36.30*71.82*1.14","30.70*60.09","E-Paper Display"]
["2.7”","KD027QVFSN008","PDF","152x296","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","36.30*71.82*0.90","30.70*60.09","E-Paper Display"]
["2.7”","KD027HVFMD010","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009-C004A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A-RS232","PDF","320x320","RS232","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-RS485","PDF","320x320","RS485","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-TTL","PDF","320x320","TTL","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027WVOIN011","PDF","800x600","MIPI","RM69700","Free V.A","No TP","-40℃~85℃","400 nits","56.60*47.25*1.50","54.60*40.95","AMOLED Display,Wide Temp TFT,LTPS Display"]
["2.8”","KD028QVFIA038","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","710 nits","50.50*69.70*2.60","43.20*57.60"]
["2.8”","KD028FM-1","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","850 nits","50.50*69.70*2.60","43.20*57.60","High-brightness TFT"]
["2.8”","KD028FM-1-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","650 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["2.8”","KD028FM-1-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","50.50*69.70*3.85","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-C004A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","56.10*77.29*4.10","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-CTP-001","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","430 nits","56.10*77.29*4.38","44.20*58.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA005","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","No TP","-20℃~80℃","480 nits","50.20*69.70*2.60","43.20*57.60"]
["2.8”","KD028QVTMA005-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","RTP","-20℃~70℃","450 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["2.8”","KD028QVTMA005-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","410 nits","50.20*69.70*3.85","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-01-C019A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","56.10*77.29*3.69","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA013-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFMA011-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA005-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.20*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028WQRMD039-01","PDF","240x400","SPI&MCU&RGB","ILI9327","V.A 5H","No TP","-20℃~70℃","120 nits","44.00*72.50*2.54","36.72*61.20","Transflective TFT"]
["2.8”","KD028QVFMA027","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","700 nits","49.40*67.60*2.35","43.20*57.60"]
["2.8”","KD028QVFIA038-C018A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","610 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028VGFID048","PDF","480x640","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","47.00*66.25*1.83","43.20*57.60"]
["2.8”","KD028VGFPD047","PDF","480x640","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","47.00*66.25*1.83","43.20*57.60"]
["2.8”","KD028VGFID048-C026A","PDF","480x640","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028VGFPD047-C026A","PDF","480x640","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFID051","PDF","240x320","MIPI","JD9852","Free V.A","No TP","-20℃~70℃","710 nits","50.50*69.70*2.35","43.20*57.60"]
["2.8”","KD028QVFID051-C028A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","610 nits","50.50*69.70*4.14","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028WXFPD057","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","73.03*76.48*2.24","70.13*70.13","Round TFT"]
["2.8”","KD028WXFID056","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","73.03*76.48*2.24","70.13*70.13","Round TFT"]
["2.8”","KD028VGFPD047-SP001A-HDMI","PDF","480x640","HDMI","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","47.00*66.25*1.83","43.20*57.60","HDMI TFT"]
["2.8”","KD028VGFPD047-C026A-SP001A-HDMI","PDF","480x640","HDMI","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,HDMI TFT"]
["2.8”","KD028WXFPD057-C040A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028WXFID056-C040A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028VGFID048-C026A-SP002A-TypeC","PDF","480x640","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*15.00","43.20*57.60","Capacitive Touch Display,Type-C TFT"]
["2.8”","KD028QVFMA058","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-30℃~85℃","700 nits","50.50*69.70*2.60","43.20*57.60","Wide Temp TFT"]
["2.8”","KD028QVRMD073","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-30℃~80℃","160 nits","50.50*69.70*2.50","43.20*57.60","Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVTMA005-C020A-RS232","PDF","240x320","RS232","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-RS485","PDF","240x320","RS485","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-TTL","PDF","240x320","TTL","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*19.00","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028WXFID076","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["2.8”","KD028WXFPD075","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["2.8”","KD028QVRMD073-C050A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~80℃","150 nits","52.90*79.30*3.95","43.20*57.60","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVFMA011","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","50.50*69.70*2.60","43.20*57.60"]
["2.8”","KD028QVFMA011-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","500 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["2.8”","KD028QVFMA011-02","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","50.50*69.70*2.63","43.20*57.60"]
["2.8”","KD028QVFMA011-02-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFMA058-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~85℃","630 nits","50.50*69.70*3.85","43.20*57.60","Capacitive Touch Display,Wide Temp TFT"]
["2.9”","KD029QHFID001","PDF","376x960","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","31.20*76.60*2.13","26.51*67.68","Bartype TFT"]
["2.9”","KD029QHFPD002","PDF","376x960","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","31.20*76.60*2.13","26.51*67.68","Bartype TFT"]
["2.9”","KD029QHFPD002-C001A","PDF","376x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QVFSN005","PDF","128x296","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","36.70*79.00*1.20","29.06*66.90","E-Paper Display"]
["2.9”","KD029QHFID001-C004A","PDF","376x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFPD002-C004A","PDF","376x960","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QVFSN006","PDF","128x296","SPI","TBD","Free V.A","No TP","0℃~35℃","0 nit","36.70*79.00*1.14","29.06*66.90","E-Paper Display"]
["2.9”","KD029QHFID001-C001A-SP001A-HDMI","PDF","376x960","HDMI","SC7283","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,HDMI TFT"]
["2.9”","KD029FHOIN010","PDF","1080x1200","MIPI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*0.65","50.11*55.68","AMOLED Display,LTPS Display"]
["2.9”","KD029FHOIN010-HDMI","PDF","1080x1200","HDMI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*11.00","50.11*55.68","AMOLED Display,LTPS Display,HDMI AMOLED"]
["3.0”","KD030FWFIN021A","PDF","480x854","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","550 nits","42.04*73.67*2.17","36.72*65.28","Wide Temp TFT"]
["3.0”","KD030FWFPN022A","PDF","480x854","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","550 nits","42.04*73.67*2.17","36.72*65.28","Wide Temp TFT"]
["3.0”","KD030NHFIN015","PDF","360x640","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","340 nits","42.04*73.67*2.17","36.72*65.28"]
["3.0”","KD030NHFPN017","PDF","360x640","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","340 nits","42.04*73.67*2.17","36.72*65.28"]
["3.0”","KD030WQFMD019-RT","PDF","240x400","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*3.89","38.88*64.80","Resistive Touch Display"]
["3.0”","KD030WQFMD019-C020B","PDF","240x400","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*4.30","38.88*64.80","Capacitive Touch Display"]
["3.0”","KD030NHFIN015B-C008A","PDF","360x640","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","300 nits","48.14*83.50*3.82","36.72*65.28","Capacitive Touch Display"]
["3.0”","KD030NHFPN017-C015A","PDF","360x640","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","300 nits","52.57*83.28*4.22","36.72*65.28","Capacitive Touch Display"]
["3.0”","KD030FWFPN022A-C018A","PDF","480x854","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030FWFIN021A-C018A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030WQFMD019","PDF","240x400","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","400 nits","45.04*77.00*2.60","38.88*64.80"]
["3.0”","KD030WVFID029","PDF","268x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","400 nits","26.96*80.08*1.66","24.12*72.00","Bartype TFT"]
["3.0”","KD030WVFID029-C028A","PDF","268x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030WVFPD030","PDF","268x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","26.96*80.08*1.66","24.12*72.00","Bartype TFT"]
["3.0”","KD030WVFPD030-C028A","PDF","268x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","650 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030WQFMD036A","PDF","240x400","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","400 nits","45.04*77.00*2.60","38.88*64.80"]
["3.0”","KD030WQTBD013","PDF","240x400","MCU","ILI9327","V.A 12H","No TP","-20℃~70℃","250 nits","45.04*77.00*2.50","38.88*64.80"]
["3.0”","KD030C-2-TP","PDF","240x400","MCU&RGB","ILI9327","V.A 12H","RTP","-20℃~70℃","300 nits","45.40*77.00*3.70","38.88*64.80","Resistive Touch Display"]
["3.0”","KD030C-2-C003A","PDF","240x400","MCU&RGB","ILI9327","V.A 12H","CTP","-20℃~70℃","270 nits","45.04*77.00*3.85","38.88*64.80","Capacitive Touch Display"]
["3.0”","KD030WQFMD036A-C020B","PDF","240x400","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*4.30","38.88*64.80","Capacitive Touch Display"]
["3.1”","KD031WVFID001","PDF","480x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","350 nits","46.28*77.00*2.20","40.32*67.20"]
["3.1”","KD031WVFPD002","PDF","480x800","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","350 nits","46.28*77.00*2.20","40.32*67.20"]
["3.1”","KD031WVFPD002-C001A","PDF","480x800","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display"]
["3.1”","KD031WVFID001-C001A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","320 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display"]
["3.1”","KD031SCOSN004","PDF","256x64","SPI","SSD1322","Free V.A","No TP","-40℃~70℃","80 nits","102.00*35.00*6.60","76.78*19.18","PMOLED Display"]
["3.1”","KD031WVFPD002-C001A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*19.50","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVTIA018","PDF","240x320","MIPI","JD9852","V.A 6H","No TP","-20℃~70℃","450 nits","55.00*77.20*2.60","48.60*64.80"]
["3.2”","KD032FM-1","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","530 nits","57.04*78.95*3.00","48.60*64.80"]
["3.2”","KD032FM-1-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","430 nits","57.04*78.95*4.20","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTMA011","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","430 nits","55.00*77.20*2.60","48.60*64.80"]
["3.2”","KD032QVTMA011-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","350 nits","55.00*77.20*3.80","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTMA011-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","370 nits","55.00*77.20*3.85","48.60*64.80","Capacitive Touch Display"]
["3.2”","KD032QVTMA015","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","No TP","-20℃~70℃","400 nits","55.00*77.20*2.60","48.60*64.80"]
["3.2”","KD032QVTMA015-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","320 nits","55.00*77.20*3.80","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTMA015-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","350 nits","55.00*77.20*3.85","48.60*64.80","Capacitive Touch Display"]
["3.2”","KD032QVFMD028","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-30℃~85℃","500 nits","54.99*77.20*2.40","48.60*64.80","Wide Temp TFT"]
["3.2”","KD032QVFMD028-TTL","PDF","240x320","TTL","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*2.40","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-RS232","PDF","240x320","RS232","ST7789V2","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*2.40","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-RS485","PDF","240x320","RS485","ST7789V2","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*15.10","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-C002A-RS485","PDF","240x320","RS485","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*15.10","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-C002A-TTL","PDF","240x320","TTL","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVTBN008","PDF","240x320","MCU","ST7789V","V.A 12H","No TP","-20℃~70℃","250 nits","57.04*78.70*3.10","48.60*64.80"]
["3.2”","KD032QVTBN008-TP","PDF","240x320","MCU","ST7789V","V.A 12H","RTP","-20℃~70℃","220 nits","57.04*78.70*4.20","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032VGFPD035-C008A","PDF","480x640","SPI+RGB","ST7701SN","Free V.A","CTP","-20℃~70℃","700 nits","66.85*85.51*4.25","49.25*65.66","Capacitive Touch Display"]
["3.2”","KD032VGFPD035-RTP","PDF","480x640","SPI+RGB","ST7701SN","Free V.A","RTP","-20℃~70℃","800 nits","54.35*73.51*4.09","49.25*65.66","Resistive Touch Display,High-brightness TFT"]
["3.2”","KD032VGFID034-C008A","PDF","480x640","MIPI","ST7701SN","Free V.A","CTP","-20℃~70℃","850 nits","66.85*85.51*4.25","49.25*65.66","Capacitive Touch Display,High-brightness TFT"]
["3.2”","KD032QVTPN013","PDF","240x320","SPI+RGB","ST7789V","V.A 12H","No TP","-20℃~70℃","250 nits","57.04*78.70*3.10","48.60*64.80"]
["3.2”","KD032QVTBN009","PDF","240x320","MCU","ST7789V","V.A 12H","No TP","-20℃~70℃","250 nits","57.04*78.70*3.10","48.60*64.80"]
["3.2”","KD032HDFLD038","PDF","1024x768","LVDS","JD9168","Free V.A","No TP","-20℃~70℃","550 nits","69.41*57.19*4.79","64.51*48.38"]
["3.2”","KD032HDFLD038-C009A","PDF","1024x768","LVDS","JD9168","Free V.A","CTP","-20℃~70℃","500 nits","79.41*67.19*6.82","64.51*48.38","Capacitive Touch Display"]
["3.2”","KD032HDFID037","PDF","1024x768","MIPI","JD9168S","Free V.A","No TP","-20℃~70℃","600 nits","69.41*57.19*2.06","64.51*48.38"]
["3.2”","KD032HDFID037-C009A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-20℃~70℃","550 nits","79.41*67.19*4.09","64.51*48.38","Capacitive Touch Display"]
["3.4”","KD034WXFID001","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","No TP","-30℃~70℃","950 nits","65.72*69.64*14.00","60.48*60.48","High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFID001-C001A-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*16.00","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFLD005","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*4.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WVFID003","PDF","800x800","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","430 nits","94.90*96.95*2.18","87.60*87.60","Round TFT"]
["3.4”","KD034WXFLD005-C001A","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","800 nits","65.72*69.64*6.34","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WVFLD004","PDF","800x800","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","420 nits","94.90*96.95*2.18","87.60*87.60","Round TFT"]
["3.4”","KD034WXFPD002-RS232","PDF","480x480","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-RS485","PDF","480x480","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-TTL","PDF","480x480","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WVFID003-SP001A-HDMI","PDF","800x800","HDMI","ILI9881C","Free V.A","No TP","-20℃~70℃","600 nits","94.89*96.95*17.08","87.60*87.60","Round TFT,HDMI TFT"]
["3.4”","KD034WVFID003-C008A","PDF","800x800","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","111.20*113.20*3.41","87.60*87.60","Capacitive Touch Display,Round TFT"]
["3.5”","KD035LQFPA093-C051A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.85","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPD093-02-C037B","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.51","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVTBA032","PDF","320x480","MCU","ILI9488","V.A 6H","No TP","-20℃~70℃","250 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035WVFPD107","PDF","340x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","400 nits","37.27*89.00*1.60","33.97*81.00","Bartype TFT"]
["3.5”","KD035HVTIA067","PDF","320x480","MIPI","ILI9488","V.A 6H","No TP","-20℃~70℃","380 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVTIA067-C022A","PDF","320x480","MIPI","ILI9488","V.A 6H","CTP","-20℃~70℃","350 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA026","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","No TP","-20℃~70℃","300 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVTMA026-C009A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","270 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-TP","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","RTP","-20℃~70℃","250 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVTMA027","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","No TP","-20℃~70℃","390 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVTMA027-C009A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","360 nits","55.50*84.96*4.05","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA027-TP","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","RTP","-20℃~70℃","320 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035LQFPA093","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","560 nits","76.90*63.90*3.17","70.08*52.56"]
["3.5”","KD035LQFPA093-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-TP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","450 nits","76.90*63.90*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064","PDF","240x320","MCU","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*3.00","53.28*71.04","Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-C021A","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*4.73","53.28*71.04","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-TP","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","RTP","-30℃~85℃","360 nits","63.00*85.00*4.05","53.28*71.04","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035VGFIA111","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","420 nits","64.00*85.00*3.10","53.28*71.04"]
["3.5”","KD035VGFIA111-C041A","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035VGFPA094","PDF","480x640","RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*3.10","53.28*71.04","Blanview TFT"]
["3.5”","KD035VGFPA094-C035A","PDF","480x640","RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","540 nits","64.00*85.00*4.55","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035WVFPD122","PDF","480x800","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*2.30","45.36*75.60"]
["3.5”","KD035WVFPD122-C047A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","60.16*96.30*4.46","45.36*75.60","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C052A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA027-C053A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C052A-RS232","PDF","320x480","RS232","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD094-01-C055A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","570 nits","69.96*92.96*4.93","53.28*71.04","Capacitive Touch Display,Blanview TFT"]
["3.5”","KD035VGFIA111A-01-C041A","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","1250 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFIA111A-01","PDF","480x640","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","1600 nits","64.00*85.00*3.10","53.28*71.04","High-brightness TFT"]
["3.5”","KD035VGFPA094-02","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","1550 nits","64.00*85.00*3.10","53.28*71.04","High-brightness TFT,Blanview TFT"]
["3.5”","KD035VGFPA094-02-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","1300 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT,Blanview TFT"]
["3.5”","KD035HVFBA140","PDF","320x480","MCU","ST7796S","Free V.A","No TP","-20℃~70℃","600 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVFMD143","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","630 nits","55.58*84.72*2.30","48.96*73.44"]
["3.5”","KD035HVFID144","PDF","320x480","MIPI","ILI9488","Free V.A","No TP","-20℃~70℃","550 nits","55.58*84.72*2.30","48.96*73.44"]
["3.5”","KD035HVFMD145","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","550 nits","54.58*83.57*2.20","48.96*73.44"]
["3.5”","KD035HVFMD145-01-C005C","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","61.90*96.04*3.90","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035HVFMD137","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","600 nits","54.58*83.57*2.18","48.96*73.44"]
["3.5”","KD035HVFMD137-C009A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","550 nits","55.30*84.76*3.31","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMD137-CTP-005","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","550 nits","61.90*96.04*3.96","48.96*73.44"]
["3.5”","KD035HVFMD137-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","500 nits","54.58*83.57*3.38","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFMA138-C009A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","340 nits","55.50*84.96*3.75"," 48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA138-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","330 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFMA139","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","600 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVFMA139-C030A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA139-C031A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","61.90*96.04*4.27","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA139-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","510 nits","55.50*94.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFIA141","PDF","320x480","MIPI","ILI9488","Free V.A","No TP","-20℃~70℃","550 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035HVFIA141-C009A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","450 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFIA141-C048A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","500 nits","61.90*96.04*4.43","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMD143-C047A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","61.90*96.04*4.32","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFID144-C048A","PDF","320x432","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","480 nits","61.90*96.04*4.32","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMD145-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","460 nits","54.58*83.57*3.40","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035VGFPD158","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","No TP","-20℃~70℃","750 nits","74.38*62.35*2.43","70.08*52.56"]
["3.5”","KD035VGFPD158-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-20℃~70℃","660 nits","85.80*85.80*4.46","70.00*52.56","Capacitive Touch Display"]
["3.5”","KD035HVFMD145-01","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","54.58*83.57*2.20","48.96*73.44","High-brightness TFT"]
["3.5”","KD035QHFID161","PDF","640x960","MIPI","ST7703","Free V.A","No TP","-30℃~85℃","500 nits","54.98*85.02*2.55","49.92*74.88","Wide Temp TFT"]
["3.5”","KD035QHFPD154","PDF","640x960","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","500 nits","54.98*84.42*2.55","49.92*74.88","Wide Temp TFT"]
["3.5”","KD035VGFID162","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-20℃~70℃","740 nits","74.38*62.35*2.43","70.08*52.56"]
["3.5”","KD035VGFID162-C061B","PDF","640x480","MIPI","ST7703","Free V.A","CTP","-20℃~70℃","670 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display"]
["3.5”","KD035HVFMA138","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","No TP","-20℃~70℃","420 nits","55.50*84.96*2.50","48.96*73.44"]
["3.5”","KD035QHFPD154-C062B","PDF","640x960","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQTMN182","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-20℃~70℃","370 nits","78.10*64.90*3.35","70.08*52.56"]
["3.5”","KD035LQTMN184","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-20℃~70℃","370 nits","78.10*64.90*3.05","70.08*52.56"]
["3.5”","KD035LQTMU190","PDF","320x240","SPI+RGB","ST7796","V.A 12H","No TP","-20℃~70℃","370 nits","78.10*64.90*3.35","70.08*52.56"]
["3.5”","KD035LQTMD188","PDF","320x240","SPI&MCU&RGB","ST7796","V.A 12H","No TP","-20℃~70℃","480 nits","77.30*64.00*2.92","70.08*52.56"]
["3.5”","KD035QVFBN212","PDF","240x360","SPI&MCU","UC8253","Free V.A","No TP","-20℃~60℃","0 nit","54.41*84.70*1.14","49.67*74.51","E-Paper Display"]
["3.5”","KD035QVRMA223","PDF","240x320","SPI&MCU&RGB","ILI9341","V.A 6H","No TP","-20℃~70℃","120 nits","60.00*82.90*2.78","53.64*71.52","Transflective TFT"]
["3.5”","KD035VGFIA111-C041A-SP007A-TypeC","PDF","480x640","Type C","TBD","Free V.A","CTP","-20℃~70℃","360 nits","64.00*85.00*17.00","53.28*71.04","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035VGFIA111-SP007A-TypeC","PDF","480x640","Type C","TBD","Free V.A","No TP","-20℃~70℃","460 nits","64.00*85.00*14.60","53.28*71.04","Type-C TFT"]
["3.5”","KD035VGFID162-C061B-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","CTP","-20℃~70℃","660 nits","85.80*85.80*16.00","70.08*52.56","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035VGFID162-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","No TP","-20℃~70℃","740 nits","74.38*62.35*14.00","70.08*52.56","Square TFT,Type-C TFT"]
["3.5”","KD035WVFLD237","PDF","480x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","500 nits","50.16*86.30*4.30","45.36*75.60"]
["3.5”","KD035WVFLD237-C047A","PDF","480x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","480 nits","60.16*96.30*6.76","45.36*75.60","Capacitive Touch Display"]
["3.5”","KD035HVTMA241","PDF","320x480","SPI&MCU&RGB","ST7365P","V.A 6H","No TP","-20℃~70℃","450 nits","54.50*83.00*2.30","48.96*73.44"]
["3.5”","KD035QHFID161-C062B","PDF","640x960","MIPI","ST7703","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035VGFPD249","PDF","640x480","RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035QVFID225-C086A","PDF","320x480","MIPI","AXS15231","Free V.A","CTP","-20℃~70℃","800 nits","61.90*96.04*3.24","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFPD249-C061B","PDF","640x480","RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFID251","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-20℃~70℃","1100 nits","74.38*62.35*2.43","70.08*52.56","High-brightness TFT"]
["3.5”","KD035LQFPA252","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","850 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA252-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035QVRMD223-C102A","PDF","240x320","SPI&MCU&RGB","ILI9341","V.A 6H","CTP","-20℃~70℃","120 nits","66.24*87.12*6.16","53.64*71.52","Capacitive Touch Display,Transflective TFT"]
["3.5”","KD035QVFSN268","PDF","240x360","SPI","TBD","Free V.A","No TP","0℃~40℃","0 nit","54.41*84.70*0.85","49.67*74.51","E-Paper Display"]
["3.5”","KD035VGFPA094A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","No TP","-30℃~70℃","700 nits","64.00*85.00*3.10","53.28*71.04"]
["3.5”","KD035VGFPA094A-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-30℃~70℃","600 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035QVFMA064-RS232","PDF","240x320","RS232","HX8347A","Free V.A","No TP","-30℃~80℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-RS485","PDF","240x320","RS485","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-TTL","PDF","240x320","TTL","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035HVTMA026-C052A-TTL","PDF","320x480","TTL","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035HVTMA026-C052A-RS485","PDF","320x480","RS485","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035HVFMA155-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS232","PDF","240x320","RS232","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS485","PDF","240x320","RS485","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-TTL","PDF","240x320","TTL","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS232","PDF","320x240","RS232","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS485","PDF","320x240","RS485","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-TTL","PDF","320x240","TTL","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-CAN","PDF","320x240","CAN","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS232","PDF","320x240","RS232","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS485","PDF","320x240","RS485","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-TTL","PDF","320x240","TTL","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-CAN","PDF","320x240","CAN","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVTMA026-RS232","PDF","320x480","RS232","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035HVTMA026-RS485","PDF","320x480","RS485","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035HVTMA026-TTL","PDF","320x480","TTL","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035VGFPA094-RS232","PDF","480x640","RS232","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-RS485","PDF","480x640","RS485","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-TTL","PDF","480x640","TTL","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-CAN","PDF","480x640","CAN","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS232","PDF","480x640","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS485","PDF","480x640","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-TTL","PDF","480x640","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-CAN","PDF","480x640","CAN","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD250-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-RS232","PDF","480x800","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.5”","KD035WVFPD122-RS485","PDF","480x800","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.5”","KD035WVFPD122-TTL","PDF","480x800","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.5”","KD035LQTMN196-04","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-30℃~85℃","1500 nits","78.10*64.90*3.10","70.08*52.56","High-brightness TFT"]
["3.5”","KD035VGFPD167-C061B-SP004A-HDMI","PDF","640x480","HDMI","NV3052CGRB","Free V.A","CTP","-10℃~60℃","500 nits","85.80*85.80*21.36","70.08*52.56","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["3.5”","KD035VGFIA281","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-30℃~85℃","1100 nits","76.91*63.90*3.15","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035HVRPD288","PDF","320x480","SPI&MCU","ST7365","TBD","No TP","-20℃~70℃","150 nits","52.26*80.60*2.21","48.96*75.60","Transflective TFT"]
["3.5”","KD035VGFLD285","PDF","640x480","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*4.85","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFLD285-C061B","PDF","640x480","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","85.80*85.80*6.88","70.08*52.56","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035LQFPA093-04","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","900 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-RTP-A","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","850 nits","76.90*63.90*4.35","70.08*52.56","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQTMN089-TP","PDF","320x240","SPI&MCU&RGB","SSD2119","V.A 12H","RTP","-20℃~70℃","330 nits","78.10*64.90*4.45","70.08*52.56","Resistive Touch Display"]
["3.5”","KD035LQTMD188-RT","PDF","320x240","SPI&MCU&RGB","ST7796","V.A 12H","RTP","-20℃~70℃","400 nits","77.80*64.50*4.30","70.08*52.56","Resistive Touch Display"]
["3.5”","KD035HVFMA155A","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","No TP","-30℃~85℃","700 nits","55.50*84.96*2.50","48.96*73.44","Wide Temp TFT"]
["3.5”","KD035HVFMA155A-C055A","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQTMD188-C037B","PDF","320x240","SPI&MCU&RGB","ST7796","V.A 12H","CTP","-20℃~70℃","430 nits","86.84*74.84*4.42","70.08*52.56","Capacitive Touch Display"]
["3.5”","KD035HVFMA155A-C005C","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","61.90*96.04*4.30","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFMA155A-RT","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","RTP","-30℃~85℃","610 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFBA062-01-C009A","PDF","320x480","MCU","ILI9488","Free V.A","CTP","-20℃~70℃","340 nits","55.50*84.96*3.62","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035LQTMU184A","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-20℃~70℃","370 nits","78.10*64.90*3.35","70.08*52.56"]
["3.5”","KD035LQTMA184B","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-20℃~70℃","400 nits","78.10*64.90*3.55","70.08*52.56"]
["3.5”","KD035HVFIA141-C055A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","500 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035LQTMN196","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-20℃~70℃","370 nits","78.10*64.90*3.05","70.08*52.56"]
["3.5”","KD035LQFPA093-05-RTP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","550 nits","76.95*64.00*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035C-1A","PDF","320x240","SPI&MCU&RGB","SSD2119","V.A 6H","No TP","-20℃~70℃","250 nits","78.02*64.85*3.10","70.08*52.56"]
["3.5”","KD035HVFMD129","PDF","320x480","SPI&MCU&RGB","ILI9488","Free V.A","No TP","-20℃~70℃","650 nits","54.58*83.57*2.30","48.96*73.44"]
["3.5”","KD035LQFPA093-04-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","76.95*64.00*4.35","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035WVFID121A","PDF","480x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","50.16*86.30*2.30","45.36*75.60"]
["3.5”","KD035WVFID121A-C043A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","420 nits","60.16*96.30*4.46","45.36*75.60","Capacitive Touch Display"]
["3.5”","KD035VGFIA111A","PDF","480x640","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","420 nits","64.00*85.00*3.10","53.28*71.04"]
["3.6”","KD036AUFPA002","PDF","544x506","RGB","ST72566","Free V.A","No TP","-35℃~85℃","900 nits","99.88*94.12*7.71","89.76*83.49","Wide Temp TFT,High-brightness TFT,Round TFT"]
["3.7”","KD037WQFSN002","PDF","240x416","SPI","UC8253","Free V.A","No TP","0℃~50℃","0 nit","53.00*92.99*1.14","47.04*81.54","E-Paper Display"]
["3.7”","KD037WQFSN003","PDF","240x416","SPI","UC8253","Free V.A","No TP","0℃~40℃","0 nit","53.00*92.99*0.90","47.04*81.54","E-Paper Display"]
["3.7”","KD037WVOPD004","PDF","480x800","RGB","TL2796","Free V.A","No TP","-30℃~80℃","250 nits","53.94*90.00*1.50","48.24*80.40","AMOLED Display,Wide Temp TFT,LTPS Display"]
["3.8”","KD038HDFPD002","PDF","1024x600","RGB","JD9168","Free V.A","No TP","-20℃~70℃","900 nits","89.92*59.93*2.78","82.64*48.42","High-brightness TFT"]
["3.8”","KD038HDFLD001","PDF","1024x600","LVDS","JD9168","Free V.A","No TP","-20℃~70℃","900 nits","89.92*59.93*2.78","82.64*48.42","High-brightness TFT"]
["3.8”","KD038HDFPD002-C001A","PDF","1024x600","RGB","JD9168","Free V.A","CTP","-20℃~70℃","810 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFLD001-C001A","PDF","1024x600","LVDS","JD9168","Free V.A","CTP","-20℃~70℃","800 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFPD002-C001A-RS232","PDF","1024x600","RS232","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-RS485","PDF","1024x600","RS485","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-TTL","PDF","1024x600","TTL","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.9”","KD39QWQ01HS","PDF","480x128","RGB","ILI6480","V.A 12H","No TP","-20℃~70℃","500 nits","105.50*40.64*2.95","95.04*25.34","Bartype TFT"]
["3.9”","KD039WQFPN002","PDF","480x128","RGB","ST7282","Free V.A","No TP","-20℃~70℃","2000 nits","102.46*34.40*3.58","95.04*25.34","High-brightness TFT,Bartype TFT"]
["3.9”","KD039WQFPN002-C001A","PDF","480x128","RGB","ST7282","Free V.A","CTP","-30℃~85℃","1900 nits","112.46*44.40*5.61","95.04*25.34","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["3.9”","KD039FHOIN003-01-C0000","PDF","1080x1240","MIPI","SD5302","Free V.A","CTP","-20℃~70℃","500 nits","67.25*79.87*0.80","65.45*75.14","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040WVFPA027","PDF","480x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","480 nits","58.26*98.10*2.50","51.84*86.40"]
["4.0”","KD040WVFPA027-RT","PDF","480x800","SPI+RGB","ST7701S","Free V.A","RTP","-20℃~70℃","400 nits","58.26*98.10*3.60","51.84*86.40","Resistive Touch Display"]
["4.0”","KD040WVFPD025","PDF","480x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","520 nits","58.26*98.10*2.75","51.84*86.40"]
["4.0”","KD040WXFID017","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-01-RTP","PDF","480x480","RGB","ST7701S","Free V.A","RTP","-30℃~85℃","800 nits","77.00*80.00*3.50","71.86*70.18","Resistive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFID026-C008B","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.25","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFID026-C009B","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFMD022-C021A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","480 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFPD025-C008B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","440 nits","58.26*98.10*4.25","51.84*87.40","Capacitive Touch Display"]
["4.0”","KD040WVFPD025-C009B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","440 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFID017-C015A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","950 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","850 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFID026-01","PDF","480x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","58.26*98.10*2.55","51.84*86.40"]
["4.0”","KD040WVFID026-01-C025A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.10","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040HDFID032","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID032-C026C","PDF","720x720","MIPI","ST7703","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*3.76","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID035","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*4.23","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040QHFID049","PDF","400x960","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","42.50*102.08*2.02","39.18*94.03","Bartype TFT"]
["4.0”","KD040QHFPD047","PDF","400x960","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","500 nits","42.50*102.08*2.02","39.18*94.03","Wide Temp TFT,Bartype TFT"]
["4.0”","KD040QHFID049-C039A","PDF","400x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["4.0”","KD040QHFPD047-C039A","PDF","400x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["4.0”","KD040WVFID026","PDF","480x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","480 nits","58.26*98.10*2.75","51.84*86.40"]
["4.0”","KD040WVFPA027-C022A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.05","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFLD071","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-30℃~85℃","950 nits","77.00*80.00*2.35","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFLD070","PDF","480x800","LVDS","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","58.26*98.10*4.70","51.84*86.40"]
["4.0”","KD040WXFLD071-C015C","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","77.00*80.00*4.51","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFLD070-C008B","PDF","480x800","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","480 nits","57.86*97.70*6.21","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040HDFID032-C026C-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","CTP","-20℃~70℃","650 nits","84.00*85.99*15.50","71.93*71.93","Capacitive Touch Display,Square TFT,Type-C TFT"]
["4.0”","KD040HDFID032-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","No TP","-20℃~70℃","700 nits","77.00*80.00*14.00","71.93*71.93","Square TFT,Type-C TFT"]
["4.0”","KD040WVFID026-01-C025A-SP005A-TypeC","PDF","480x800","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*16.00","51.84*86.40","Capacitive Touch Display,Type-C TFT"]
["4.0”","KD040WXFID017-C015C-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","77.00*80.00*16.00","71.86*70.18","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["4.0”","KD040HDFLD072","PDF","720x720","LVDS","NV3051F-L","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040WVFSN077","PDF","480x800","SPI","SD8385","Free V.A","No TP","0℃~40℃","0 nit","56.24*96.62*0.81","51.84*86.40","E-Paper Display"]
["4.0”","KD040HVFID080","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFID080-C050A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081-C050A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A-RS232","PDF","720x720","RS232","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS485","PDF","720x720","RS485","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-TTL","PDF","720x720","TTL","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-SP002A-HDMI","PDF","480x800","HDMI","ST7701S","Free V.A","No TP","-10℃~60℃","480 nits","58.26*98.10*13.78","51.84*86.40","HDMI TFT"]
["4.0”","KD040WXFPD014-C015C-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-CAN","PDF","720x720","CAN","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040QHFID049-SP004A-TypeC","PDF","400x960","Type C","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","42.50*102.08*13.50","39.18*94.03","Type-C TFT"]
["4.0”","KD040QHFID049-C039A-SP004A-TypeC","PDF","400x960","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*15.00","39.18*94.03","Capacitive Touch Display,Type-C TFT"]
["4.0”","KD040HDFID088","PDF","720x720","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","900 nits","105.60*109.87*2.16","101.52*101.52","High-brightness TFT,Round TFT"]
["4.0”","KD040WVTPD090","PDF","480x800","RGB","ST7701SI","V.A 6H","No TP","-20℃~70℃","150 nits","57.14*96.85*2.60","51.84*86.40","Transflective TFT"]
["4.0”","KD040WVTPD090-C008B","PDF","480x800","RGB","ST7701SI","V.A 6H","CTP","-10℃~60℃","150 nits","57.86*97.70*4.08","51.84*86.40","Capacitive Touch Display,Transflective TFT"]
["4.0”","KD040FHFLD058-C041A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","1000 nits","104.87*72.22*4.76","88.59*49.83","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["4.0”","KD040FHFLD058","PDF","1920x1080","LVDS","SC5010","Free V.A","No TP","-20℃~70℃","1100 nits","94.87*62.22*2.73","88.59*49.83","High-brightness TFT,LTPS Display"]
["4.0”","KD040WVFBD056","PDF","480x800","MCU","ILI9806","Free V.A","No TP","-20℃~70℃","500 nits","58.34*97.50*2.55","51.84*86.40"]
["4.0”","KD040HDFID088-C054A","PDF","720x720","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","800 nits","125.29*127.29*3.41","101.52*101.52","Capacitive Touch Display,High-brightness TFT,Round TFT"]
["4.0”","KD040WVFPD027-02-C008B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*3.85","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFPD014-C046B","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","82.80*82.80*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040UXOIN109-C073A","PDF","1080x1200","MIPI","VTDR6130A","Free V.A","CTP","-20℃~70℃","600 nits","72.93*80.53*1.12","68.43*76.03","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040WXFPD014-a","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.1”","KD041HDOIN002-C000","PDF","2480x1860","MIPI","RM69A10","Free V.A","CTP","-20℃~70℃","280 nits","48.24*100.84*2.64","43.55*94.47","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043WVFID083-02-C048A","PDF","480x800","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","69.16*120.05*4.58","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WQFPA042","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-01-RT","PDF","480x272","RGB","SC7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFIA083","PDF","480x800","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","450 nits","62.50*105.55*2.65","56.16*93.60"]
["4.3”","KD043WQTPA097A-04","PDF","480x272","RGB","NV3047E","V.A 12H","No TP","-20℃~70℃","600 nits","105.40*67.15*3.16","95.04*53.86"]
["4.3”","KD043WQTPA097A-01-RT","PDF","480x272","RGB","NV3047E","V.A 12H","RTP","-20℃~70℃","400 nits","105.40*67.15*4.06","95.04*53.86","Resistive Touch Display"]
["4.3”","KD043WQTPA097A-01","PDF","480x272","RGB","NV3047E","V.A 12H","No TP","-20℃~70℃","500 nits","105.40*67.15*3.16","95.04*53.86"]
["4.3”","KD043WVFBD082","PDF","480x800","MCU","ILI9806","Free V.A","No TP","-20℃~70℃","480 nits","62.66*105.95*2.25","56.16*93.60"]
["4.3”","KD043WVFBD082-RT","PDF","480x800","MCU","ILI9806","Free V.A","RTP","-20℃~70℃","380 nits","62.66*105.95*3.85","56.16*93.60","Resistive Touch Display"]
["4.3”","KD043WVFPA084","PDF","480x800","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","450 nits","62.50*105.55*2.65","56.16*93.60"]
["4.3”","KD043WVFPA084-01-RT","PDF","480x800","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","370 nits","62.50*105.55*3.70","56.16*93.60","Resistive Touch Display"]
["4.3”","KD043WQFPA042-01-C037C","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-C038A","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","115.40*79.15*4.80","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQTPA097A-01-C009A","PDF","480x272","RGB","NV3047E","V.A 12H","CTP","-20℃~70℃","450 nits","105.40*67.15*4.41","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WQTPA097A-01-C017A","PDF","480x272","RGB","NV3047E","V.A 12H","CTP","-20℃~70℃","450 nits","115.40*79.15*4.79","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WVFBD082-C010A","PDF","480x800","MCU","ILI9806","Free V.A","CTP","-20℃~70℃","430 nits","62.66*105.95*3.68","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFIA083-01-C064A","PDF","480x800","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*4.20","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFPA084-01-C015B","PDF","480x800","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*4.20","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFLA096-03-C049A-ZJB-HDMI","PDF","800x480","HDMI","ST7262","Free V.A","CTP","-10℃~60℃","450 nits","105.40*79.15*21.96","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFPD051-01-C050A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*4.25","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFLA096-02","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPD049-C038B","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","740 nits","115.40*79.15*4.63","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFPA084-02-SP001A-HDMI","PDF","480x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","730 nits","62.50*105.55*19.75","56.16*93.60","HDMI TFT"]
["4.3”","KD043WVFPA051-02","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","1250 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","1000 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C049A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","115.40*79.15*4.86","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQTPA097A-04-C017A-SP003A-HDMI","PDF","480x272","HDMI","TBD","V.A 12H","CTP","-20℃~70℃","500 nits","115.40*79.15*21.89","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFLA096-02A-RT","PDF","800x480","LVDS","ST7262","Free V.A","RTP","-30℃~85℃","950 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPD042-07-C017C-SP004A-HDMI","PDF","480x272","HDMI","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","115.40*79.15*20.40","95.04*53.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["4.3”","KD043WVFPA084-05-C015B-SP001A-HDMI","PDF","480x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","62.50*105.55*21.30","56.16*93.60","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS232","PDF","480x800","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS485","PDF","480x800","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-TTL","PDF","480x800","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS232","PDF","480x272","RS232","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS485","PDF","480x272","RS485","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-TTL","PDF","480x272","TTL","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS232","PDF","800x480","RS232","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS485","PDF","800x480","RS485","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-TTL","PDF","800x480","TTL","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-CAN","PDF","480x272","CAN","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFMD134","PDF","480x272","MCU","NV3041A-01","Free V.A","No TP","-30℃~85℃","950 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-03","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","650 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142","PDF","480x272","RGB","ST7282A","Free V.A","No TP","-30℃~80℃","700 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA137","PDF","480x272","RGB","ILI6485","Free V.A","No TP","-30℃~80℃","600 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFPA051-05","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFPA051-05-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFLA096","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFLA096-02A","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-03","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFLA096-03-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043OLEDN001","PDF","568x1210","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","600 nits","49.13*103.55*0.75","47.37*100.91","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043WQFMD134-01-RT","PDF","480x272","MCU","NV3041A-01","Free V.A","RTP","-20℃~70℃","950 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,High-brightness TFT"]
["4.3”","KD043WQFMD134-01-C037A","PDF","480x272","MCU","NV3041A-01","Free V.A","CTP","-30℃~85℃","900 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-C037D","PDF","480x272","RGB","ST7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-RT","PDF","480x272","RGB","ST7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA042-01","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVTBD116","PDF","480x800","MCU","ILI9806","V.A 12H","No TP","-20℃~70℃","300 nits","62.66*105.95*2.35","56.16*93.60"]
["4.3”","KD043WVFLD117","PDF","480x800","LVDS","ILI9806E","Free V.A","No TP","-20℃~70℃","450 nits","62.54*105.59*2.53","56.16*93.60"]
["4.3”","KD043WVFLD117-C048A","PDF","480x800","LVDS","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","69.16*120.05*4.58","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WQTPA115","PDF","480x272","RGB","ST7282","V.A 12H","No TP","-30℃~85℃","500 nits","105.50*67.20*3.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQTPA115-01-C090A","PDF","480x272","RGB","ST7282","V.A 12H","CTP","-20℃~70℃","440 nits","105.50*67.20*5.40","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WQTPA115-01-RT","PDF","480x272","RGB","ST7282","V.A 12H","RTP","-30℃~85℃","400 nits","105.50*67.20*5.10","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA147","PDF","480x272","RGB","IL5230A","Free V.A","No TP","-20℃~70℃","230 nits","105.50*67.20*2.95","95.04*53.86"]
["4.3”","KD043WQFPA142-01","PDF","480x272","RGB","ST7282A","Free V.A","No TP","-30℃~80℃","700 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142-01-RT","PDF","480x272","RGB","ST7282A","Free V.A","RTP","-30℃~80℃","550 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQRPA140","PDF","480x272","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","650 nits","105.50*67.20*3.80","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142-01-C037D","PDF","480x272","RGB","ST7282A","Free V.A","CTP","-30℃~80℃","650 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQTPA097B","PDF","480x272","RGB","ST7282A","V.A 6H","No TP","-20℃~70℃","350 nits","105.40*67.15*3.16","95.04*53.86"]
["4.5”","KD045FWFPA010-01-RT","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","400 nits","61.54*110.09*3.80","55.44*98.64","Resistive Touch Display"]
["4.5”","KD045FWFIA011","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","500 nits","61.54*110.09*2.60","55.44*98.64"]
["4.5”","KD045FWFPA010-01-C001B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWTPA001-02-SP001A-HDMI","PDF","480x854","HDMI","ILI9806E","V.A 12H","No TP","-20℃~70℃","350 nits","61.54*110.09*17.45","55.44*98.64","HDMI TFT"]
["4.5”","KD045FWTPA001-02-C001B-SP001A-HDMI","PDF","480x854","HDMI","ILI9806E","V.A 12H","CTP","-20℃~70℃","350 nits","61.54*110.09*19.00","55.44*98.64","Capacitive Touch Display,HDMI TFT"]
["4.5”","KD045FWFPA010","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","500 nits","61.54*110.09*2.60","55.44*98.64"]
["4.5”","KD045FWFLA012-01-C001B","PDF","480x854","LVDS","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFIA011-01-C001B","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFPA010-01-C001B-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFID015","PDF","480x854","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","60.00*109.00*2.13","55.44*98.64"]
["4.5”","KD045FWFID015-C005A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","72.00*121.00*3.85","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFID016","PDF","480x854","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","60.00*109.00*2.13","55.44*98.64"]
["4.5”","KD045FWFID016-C005A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","72.00*121.00*3.85","55.44*98.64","Capacitive Touch Display"]
["4.7”","KD047HDFID001","PDF","720x1280","MIPI","ST7703","Free V.A","No TP","-20℃~70℃","450 nits","61.00*110.60*1.80","58.10*103.30"]
["5.0”","KD050SXFID039","PDF","1080x1080","MIPI","HX8399","Free V.A","No TP","-20℃~60℃","300 nits","136.53*132.21*1.98","127.01*127.01","Round TFT"]
["5.0”","KD050FWFID042-C010B","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPD041-C010B","PDF","480x854","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA029-02-C045A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","120.70*75.90*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","650 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFIA019","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","550 nits","67.56*122.35*2.60","61.63*109.65"]
["5.0”","KD050FWFIA019-C019A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","520 nits","67.56*122.35*2.60","61.63*109.65"]
["5.0”","KD050FWFPA011-C009A","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*4.03","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-LVDS","PDF","480x854","LVDS","ILI9806E","Free V.A","No TP","-20℃~70℃","450 nits","67.56*122.35*2.60","61.63*109.65"]
["5.0”","KD050FWFPA011-TP","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","430 nits","67.56*122.35*3.80","61.63*109.65","Resistive Touch Display"]
["5.0”","KD050HDFIA020","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","500 nits","67.56*122.35*2.60","62.10*110.40"]
["5.0”","KD050HDFID040-C020B","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","440 nits","78.56*135.65*4.13","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050HDFPA054-RT","PDF","720x1280","RGB","NV3052CGRB","Free V.A","RTP","-20℃~70℃","320 nits","67.56*122.35*3.80","62.10*110.40","Resistive Touch Display"]
["5.0”","KD050SXFID039-C045A","PDF","1080x1080","MIPI","HX8399","Free V.A","CTP","-20℃~60℃","270 nits","208.00*208.00*4.16","127.01*127.01","Capacitive Touch Display,Round TFT"]
["5.0”","KD050WVTPA045-01","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","No TP","-20℃~70℃","400 nits","120.70*75.90*2.95","108.00*64.80"]
["5.0”","KD050HDFIA020-SP003A-TYPE C","PDF","720x1280","Type C","ILI9881C","Free V.A","No TP","-20℃~70℃","500 nits","67.56*122.35*13.75","62.10*110.40","Type-C TFT"]
["5.0”","KD050HDFIA020-06-C020E-SP003A-TYPE C","PDF","720x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*15.35","62.10*110.40","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050HDFIA061-RT","PDF","720x1280","MIPI","ILI9881C","Free V.A","RTP","-20℃~70℃","320 nits","67.56*122.35*3.80","62.10*110.40","Resistive Touch Display"]
["5.0”","KD050WVTPA045","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","No TP","-20℃~70℃","350 nits","120.70*75.80*3.10","108.00*64.80"]
["5.0”","KD050HDFIA020-06-C020E","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*4.03","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050HDFPA054","PDF","720x1280","RGB","NV3052CGRB","Free V.A","No TP","-20℃~70℃","400 nits","67.56*122.35*2.60","62.10*110.40"]
["5.0”","KD050HDFPA054-C020A","PDF","720x1280","RGB","NV3052CGRB","Free V.A","CTP","-20℃~70℃","350 nits","78.56*135.65*4.20","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050HDFIA014","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","500 nits","67.56*122.35*2.60","62.10*110.40"]
["5.0”","KD050HDFIA020-06-C020D","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","78.56*135.65*4.20","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050FHFLD102","PDF","1920x1080","LVDS","SC5010B","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.76*2.77","110.59*62.21","High-brightness TFT,LTPS Display"]
["5.0”","KD050WVTPA045-C005A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","310 nits","120.70*75.80*4.48","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-RT","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","RTP","-20℃~70℃","280 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display"]
["5.0”","KD050WVTPA045-C005A-SP001A-HDMI","PDF","800x480","HDMI","ILI5960/ILI6122","V.A 12H","CTP","-10℃~60℃","310 nits","120.70*75.80*19.81","108.00*64.80","Capacitive Touch Display,HDMI TFT"]
["5.0”","KD050HDFLD091-C020C","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","400 nits","67.56*122.35*4.05","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-010","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","950 nits","67.56*122.35*2.60","61.63*109.65","High-brightness TFT"]
["5.0”","KD050FWFIA019-SP004-TYPE C","PDF","480x854","Type C","ILI9806E","Free V.A","No TP","-20℃~70℃","610 nits","67.56*122.35*13.70","61.63*109.65","Type-C TFT"]
["5.0”","KD050FWFIA019-02-C009E-SP004A-TYPE C","PDF","480x854","Type C","ILI9806E","Free V.A","CTP","-20℃~70℃","540 nits","67.56*122.35*15.25","61.63*109.65","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050FWFLD099-C010B","PDF","480x854","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFLD099","PDF","480x854","LVDS","ST7701S","Free V.A","No TP","-20℃~70℃","650 nits","67.06*121.85*2.90","61.63*109.65"]
["5.0”","KD050FWFBA002-TP","PDF","480x854","MCU","ILI9806E","Free V.A","RTP","-20℃~70℃","450 nits","67.56*122.35*3.80","61.56*109.53","Resistive Touch Display"]
["5.0”","KD050FWFBA002","PDF","480x854","MCU","ILI9806E","Free V.A","No TP","-20℃~70℃","500 nits","67.56*122.35*2.60","61.56*109.53"]
["5.0”","KD050FWFPA011-CTP-002","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-C010B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.00","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FHFID103","PDF","1920x1080","MIPI","SC5010E","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.67*2.77","110.59*62.20","High-brightness TFT,LTPS Display"]
["5.0”","KD050WVFPA107","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","950 nits","118.50*77.80*3.85","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA107-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","760 nits","118.50*77.80*5.10","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA107-C104A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","900 nits","118.50*77.80*6.34","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109","PDF","480x272","RGB","ST7282","Free V.A","No TP","-30℃~85℃","1000 nits","120.16*75.36*2.53","110.88*62.83","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109-C107A","PDF","480x272","RGB","ST7282","Free V.A","CTP","-30℃~85℃","900 nits","120.16*75.36*4.56","110.88*62.83","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050HDOIN116-C000","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FWFPA011-09-C009E-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS232","PDF","720x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS485","PDF","720x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-TTL","PDF","720x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS232","PDF","800x480","RS232","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS485","PDF","800x480","RS485","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-TTL","PDF","800x480","TTL","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDOIN116-C116B","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","70.52*123.12*1.67","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050WVRPA092","PDF","800x480","RGB","HX8264+HX8664","V.A 12H","No TP","-20℃~70℃","180 nits","120.70*75.90*2.96","108.00*64.80","Transflective TFT"]
["5.0”","KD050HDFPA118","PDF","720x1280","RGB","GC9704C","Free V.A","No TP","-20℃~70℃","400 nits","67.56*122.35*2.60","62.10*110.40"]
["5.0”","KD050WVRPD092-03-C045A","PDF","800x480","RGB","HX8264+HX8664","V.A 12H","CTP","-20℃~70℃","150 nits","132.72*87.80*4.99","108.00*64.80","Capacitive Touch Display,Transflective TFT"]
["5.0”","KD050FWFPA121","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","580 nits","67.56*122.35*2.60","61.56*109.53"]
["5.0”","KD050WVFPA124A","PDF","800x480","RGB","TBD","Free V.A","No TP","-30℃~85℃","700 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050HDOIN116-C000-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","64.12*116.72*10.80","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C116B-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","70.52*123.12*12.37","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050FWFIA019-01-C019A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","67.26*122.00*3.98","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-01","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","400 nits","67.06*121.85*2.50","61.63*109.65"]
["5.0”","KD050FWFIA019-02","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","490 nits","67.56*122.35*2.60","61.63*109.65"]
["5.0”","KD050FWFIA019-02-C002A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-02-C009F","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA029-06-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","120.70*75.90*4.48","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","700 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVTPA045-C003A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","310 nits","132.72*87.80*5.00","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-02A-C003A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","650 nits","132.72*87.80*4.88","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-02A-C005A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","650 nits","120.70*75.90*4.60","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-02A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","No TP","-20℃~70℃","800 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT"]
["5.0”","KD050WVTPA045-02A-TP","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","RTP","-20℃~70℃","650 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display"]
["5.0”","KD050WVFPA029-06","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","850 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050FHFLD102-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","116.59*72.76*18.67","110.59*62.21","High-brightness TFT,HDMI TFT"]
["5.0”","KD050FHFLD102-01-C085B","PDF","1920x1080","LVDS","SC5010B","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["5.0”","KD050HDFID040-02-C020B","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","430 nits","78.56*135.65*4.33","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050WVFLA033-01-C045A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","750 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFLA037-01-C045A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-20℃~70℃","600 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050HDOIN132-C001","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FWFIA019-02-C009E","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050HDFIA020-06","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","450 nits","67.56*122.35*2.65","62.10*110.40"]
["5.0”","KD050WVFLA022","PDF","800x480","LVDS","HX8678C/HX8249A","Free V.A","No TP","-30℃~85℃","700 nits","124.90*78.10*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050WVFLA033","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA018","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","No TP","-30℃~85℃","700 nits","124.90*78.10*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050WVFPA018-C020A","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","CTP","-30℃~85℃","630 nits","124.90*78.10*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA018-RTP","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","RTP","-30℃~85℃","560 nits","124.90*78.10*4.05","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFPA041-03-C002A","PDF","480x854","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","520 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFBA002-02-C009E","PDF","480x854","MCU","ILI9806","Free V.A","CTP","-20℃~70℃","550 nits","67.56*122.35*4.03","61.56*109.53"]
["5.0”","KD050FHFLD079-C085A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050HDFIA020-04","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","750 nits","67.56*122.35*2.60","62.10*110.40"]
["5.0”","KD050FWFPA011-09-C002A","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-C009B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","67.56*122.35*3.88","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050HDFID040-C020C","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*4.05","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-09-TP","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","410 nits","67.56*122.35*3.70","61.63*109.65","Resistive Touch Display"]
["5.0”","KD050FWFPA011-09-C009E","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*4.03","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-004","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","950 nits","67.56*122.35*2.60","61.63*109.65","High-brightness TFT"]
["5.0”","KD050HDOIN116-C000-a","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FHFID103-01-C085B","PDF","1920x1080","MIPI","SC5010E","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050WVFLA146","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-01","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.16*75.36*2.70","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02-C039A","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","950 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-02-C045A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","850 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C039A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C040C","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","120.70*75.90*4.38","108.50*65.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFID042-C009B","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","67.56*122.35*4.38","61.63*109.65","Capacitive Touch Display"]
["5.5”","KD055FHFID018","PDF","1080x1920","MIPI","HX8399-A","Free V.A","No TP","-20℃~70℃","400 nits","71.04*129.67*1.45","68.04*120.96"]
["5.5”","KD055HDFIA001-C001A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","360 nits","86.04*144.96*4.75","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055FHFID018B-01-C017C","PDF","1080x1920","MIPI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*2.64","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055HDFLD023-C026A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","650 nits","79.04*137.67*4.39","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055HDFIA001-C001A-SP002A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","500 nits","86.04*144.96*21.85","68.04*120.96","Capacitive Touch Display,HDMI TFT"]
["5.5”","KD055FHFID018-01-C017A-SP003A-HDMI","PDF","1080x1920","HDMI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*19.74","68.04*120.96","Capacitive Touch Display,HDMI TFT,LTPS Display"]
["5.5”","KD055SCOSN025","PDF","256x64","SPI","SSD1322","Free V.A","No TP","-40℃~70℃","80 nits","160.00*50.00*6.60","135.65*33.89","PMOLED Display"]
["5.5”","KD055FHFID010","PDF","1080x1920","MIPI","XM91080","Free V.A","No TP","-20℃~70℃","360 nits","71.04*129.67*1.69","68.04*120.96"]
["5.5”","KD055FHFID010-C017A","PDF","1080x1920","MIPI","XM91080","Free V.A","CTP","-20℃~70℃","340 nits","79.04*137.67*2.84","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055FHFID018-C017A","PDF","1080x1920","MIPI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*2.60","68.04*120.96","Capacitive Touch Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001","PDF","1080x1920","MIPI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*0.82","67.82*120.58","Capacitive Touch Display,AMOLED Display"]
["5.5”","KD055FHOIN031-C0000","PDF","1080x1920","MIPI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.82","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001-SP005A-HDMI","PDF","1080x1920","HDMI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*10.80","67.82*120.58","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN031-C0000-HDMI","PDF","1080x1920","HDMI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.83","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055HDFID028-C001A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","430 nits","86.04*144.96*4.75","67.93*120.77","Capacitive Touch Display"]
["5.5”","KD055HDFID028","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","450 nits","74.28*133.21*2.64","67.93*120.77"]
["5.6”","KD056VGTPA003","PDF","640x480","RGB","TBD","V.A 12H","No TP","-20℃~70℃","450 nits","126.50*100.00*4.50","112.90*84.67"]
["5.6”","KD056VGTPA003-C002A","PDF","640x480","RGB","TBD","V.A 12H","CTP","-20℃~70℃","380 nits","126.50*100.00*6.08","112.90*84.67","Capacitive Touch Display"]
["5.6”","KD056VGTPA004","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*5.70","115.20*86.40","High-brightness TFT"]
["5.6”","KD056VGTPA004-RT","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","RTP","-20℃~70℃","700 nits","126.50*100.00*7.30","115.00*86.40","Resistive Touch Display"]
["5.6”","KD056VGTPA004-C004A","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","CTP","-20℃~70℃","750 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display"]
["5.6”","KD056VGTPA004-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*13.08","115.20*86.40","High-brightness TFT,HDMI TFT"]
["5.6”","KD056VGTPA004-C004A-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","CTP","-20℃~70℃","750 nits","126.50*100.00*23.60","115.50*86.40","Capacitive Touch Display,HDMI TFT"]
["5.6”","KD056VGTPA003-RT","PDF","640x480","RGB","TBD","V.A 12H","RTP","-20℃~70℃","350 nits","126.50*100.00*5.50","112.90*84.67","Resistive Touch Display"]
["5.6”","KD056VGTPA006","PDF","640x480","RGB","ILI6192A-01/ ILI5481A","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*5.70","112.90*84.68","High-brightness TFT"]
["5.7”","KD057VGFPA011-C004A","PDF","640x480","RGB","JD9186S","Free V.A","CTP","-30℃~80℃","550 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA011","PDF","640x480","RGB","JD9186S","Free V.A","No TP","-30℃~80℃","600 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","600 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015-RT","PDF","640x480","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","480 nits","126.50*100.00*7.40","115.20*86.40","Resistive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGTPA003-TP","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","RTP","-20℃~70℃","600 nits","144.00*104.60*14.60","115.20*86.40","Resistive Touch Display"]
["5.7”","KD057VGFPA015A","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015A-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFLA012A","PDF","640x480","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFLA012A-C004A","PDF","640x480","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFIA014A","PDF","640x480","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFIA014A-C004A","PDF","640x480","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA018","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","700 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA018-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","650 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.8”","KD058UXFLA003-C001A","PDF","1920x1080","LVDS","ST5892B","Free V.A","CTP","-20℃~70℃","950 nits","144.56*87.40*7.65","126.72*71.28","Capacitive Touch Display,High-brightness TFT"]
["5.8”","KD058UXFLA003","PDF","1920x1080","LVDS","ST5892B","Free V.A","No TP","-20℃~70℃","950 nits","144.56*87.40*5.50","126.72*71.28","High-brightness TFT"]
["5.8”","KD058UXFLA003-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","No TP","-10℃~60℃","950 nits","144.56*87.40*20.40","126.72*71.28","High-brightness TFT,HDMI TFT"]
["5.8”","KD058UXFLA003-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","CTP","-20℃~70℃","900 nits","144.56*87.40*21.26","126.72*71.28","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["5.8”","KD058VGFSN005","PDF","640x480","SPI","TBD","Free V.A","No TP","0℃~50℃","0 nit","125.40*99.50*1.26","118.78*88.22","E-Paper Display"]
["5.9”","KD059WVFPD001","PDF","840x512","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.16*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-C001A","PDF","840x512","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.16*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-RTP","PDF","840x512","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.16*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003","PDF","840x512","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003-C001A","PDF","840x512","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002","PDF","840x512","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-C001A","PDF","840x512","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-RTP","PDF","840x512","LVDS","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.76*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.0”","KD060HDFID001","PDF","720x1440","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","500 nits","75.04*147.63*2.35","68.04*136.08"]
["6.0”","KD060HDFID001-C001A","PDF","720x1440","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","480 nits","95.04*167.63*4.33","68.04*136.08","Capacitive Touch Display"]
["6.0”","KD060HDFID001-SP001A-HDMI","PDF","720x1440","HDMI","ILI9881C","Free V.A","No TP","-20℃~70℃","450 nits","75.04*147.63*17.25","68.04*136.08","HDMI TFT"]
["6.0”","KD060HDFID001-C001A-SP001A-HDMI","PDF","720x1440","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","95.04*167.63*19.23","68.04*136.08","Capacitive Touch Display,HDMI TFT"]
["6.0”","KD060HDFLD007","PDF","720x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","400 nits","77.52*141.50*2.01","73.98*131.52"]
["6.0”","KD060HDFID001-C001A-SP002A-TYPEC","PDF","720x1440","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","480 nits","95.04*167.63*15.55","68.04*136.08","Capacitive Touch Display,Type-C TFT"]
["6.0”","KD060HDFLD007-C005A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.0”","KD060HDFID006-C005A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.0”","KD060HDFSN009","PDF","758x1024","Parallel","TBD","Free V.A","No TP","0℃~50℃","0 nit","101.80*138.40*0.93","90.58*122.37","E-Paper Display"]
["6.0”","KD060FPOIN011-C0000","PDF","1080x2160","MIPI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.0”","KD060FPOIN011-C0000-HDMI","PDF","1080x2160","HDMI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.0”","KD060HDFID006","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","400 nits","77.52*141.50*2.01","73.98*131.52"]
["6.0”","KD060HDFID006-C005A-SP001A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","80.58*146.12*18.21","73.98*131.52","Capacitive Touch Display,HDMI TFT"]
["6.0”","KD060HDFLD007A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","400 nits","77.52*141.50*2.01","73.98*131.52"]
["6.0”","KD060HDFLD007A-C005A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.0”","KD060FHFID014","PDF","1080x1920","MIPI","NT35532","Free V.A","No TP","-20℃~70℃","250 nits","76.72*139.62*1.21","74.52*132.48"]
["6.2”","KD062VGFPA003-01-SP001A-HDMI","PDF","640x240","HDMI","ST5043AA/ST5894AA","Free V.A","No TP","-20℃~70℃","900 nits","163.60*67.60*17.77","148.80*53.76","High-brightness TFT,Bartype TFT,HDMI TFT"]
["6.2”","KD062VGFPD003-C002A","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","800 nits","173.80*82.76*4.76","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-RTP","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","RTP","-30℃~85℃","750 nits","163.10*67.10*4.21","148.80*53.76","Resistive Touch Display,Wide Temp TFT"]
["6.2”","KD062VGFPD003","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.10*67.10*2.71","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-C002A-TTL","PDF","640x240","TTL","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS485","PDF","640x240","RS485","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS232","PDF","640x240","RS232","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPA003-01","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.60*67.60*2.87","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062HDFLD005-01-C007A","PDF","1024x600","LVDS","JD9168S","Free V.A","CTP","-20℃~70℃","1350 nits","155.40*88.40*6.68","137.47*77.23","Capacitive Touch Display,High-brightness TFT"]
["6.4”","KD064FPOIN001-C0000","PDF","1080x2340","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.4”","KD064FPOIN001-C0000-HDMI","PDF","1080x2340","HDMI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.5”","KD065FPOIN003","PDF","1080x2400","MIPI","RM692E5","Free V.A","No TP","-20℃~70℃","500 nits","71.45*156.64*0.29","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.5”","KD065FPOIN003-HDMI","PDF","1080x2400","HDMI","TBD","Free V.A","No TP","-20℃~70℃","450 nits","71.45*156.64*11.00","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["6.6”","KD066FHFID010-C011A","PDF","1080x2400","MIPI","FT8725","Free V.A","CTP","-25℃~70℃","550 nits","74.88*167.48*2.19","68.43*152.57","Capacitive Touch Display"]
["6.67”","KD067FPOIN004-C0000","PDF","1080x2400","MIPI","VTDR6130","Free V.A","CTP","-20℃~70℃","500 nits","71.53*200.59*0.33","69.55*154.56","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.7”","KD067WSFLA001","PDF","1920x1080","LVDS","HX8249/HX8678","Free V.A","No TP","-20℃~70℃","1300 nits","161.12*97.68*4.77","148.32*83.43","High-brightness TFT"]
["6.7”","KD067WSFLA001-C001A","PDF","1920x1080","LVDS+eDP","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1300 nits","161.12*97.68*7.12","148.32*84.43","Capacitive Touch Display,High-brightness TFT"]
["6.7”","KD067WSFLA001-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1500 nits","161.12*97.68*23.02","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1100 nits","161.12*97.68*20.67","148.32*83.43","High-brightness TFT,HDMI TFT"]
["6.7”","KD067FHFID002-C003A","PDF","1080x2400","MIPI","ICNL9922CAC-01","Free V.A","CTP","-20℃~70℃","400 nits","74.31*164.56*2.13","70.08*155.74","Capacitive Touch Display"]
["6.7”","KD067WSFLA001-C001A-SP002A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1000 nits","161.12*97.68*23.10","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068HDFLD004","PDF","480x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1650 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005","PDF","480x1280","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","2350 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005-C001A","PDF","480x1280","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","2250 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFLD004-C001A","PDF","480x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1450 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068WVFPA007","PDF","800x480","RGB","TBD","Free V.A","No TP","-30℃~85℃","800 nits","156.10*100.91*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPA007-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","No TP","-20℃~70℃","800 nits","156.10*100.91*21.40","140.10*88.86","High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPD007-01-C003A","PDF","800x480","RGB","TBD","Free V.A","CTP","-30℃~85℃","800 nits","155.96*100.77*7.29","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","CTP","-20℃~70℃","800 nits","155.96*100.77*23.19","148.10*88.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPA001","PDF","800x480","RGB","ST72658","Free V.A","No TP","-30℃~85℃","800 nits","165.00*100.00*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS232","PDF","800x480","RS232","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS485","PDF","800x480","RS485","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-TTL","PDF","800x480","TTL","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-CAN","PDF","800x480","CAN","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068HDFPD011","PDF","480x1280","RGB","GC9704","Free V.A","No TP","-20℃~70℃","2000 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009","PDF","480x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","2100 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009-C009A","PDF","480x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","2000 nits","78.20*191.10*6.42","60.19*160.51","High-brightness TFT,Bartype TFT"]
["7.0”","7.0 inch Andriod Tablet","PDF","800*1280","2G+16G","Andriod","Free V.A","CTP","-20 ℃~70℃","350 nits"]
["7.0”","KD070WVTPA077","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","No TP","-20℃~70℃","1300 nits","165.00*100.00*5.80","154.08*85.92","High-brightness TFT"]
["7.0”","KD070WVTPA077-C004A","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","1100 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFPA010-02","PDF","800x480","RGB","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","800 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","400 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT"]
["7.0”","KD070HDTLA020","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","No TP","-20℃~70℃","620 nits","165.00*100.00*5.80","154.21*85.92"]
["7.0”","KD070HDFPA019","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","780 nits","165.00*100.00*5.80","154.21*85.92"]
["7.0”","KD070C-4","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","No TP","-20℃~70℃","500 nits","165.00*100.00*5.80","154.08*85.92"]
["7.0”","KD070WVFPA065","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","600 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT"]
["7.0”","KD070WVTPA006","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","No TP","-20℃~70℃","500 nits","165.00*100.00*5.80","154.08*85.92"]
["7.0”","KD070HDFPA012","PDF","1024x600","RGB","JD79001HF & JD73215","Free V.A","No TP","-20℃~70℃","240 nits","164.90*100.00*3.50","154.08*85.92"]
["7.0”","KD070WVFLA035","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WXFID050","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~60℃","450 nits","103.56*162.38*2.70","94.20*150.72"]
["7.0”","KD070HDFIA030","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","No TP","-20℃~70℃","900 nits","165.00*100.00*5.80","154.21*85.92"]
["7.0”","KD070HDFLA028","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","650 nits","165.00*100.00*5.80","154.21*85.92"]
["7.0”","KD070HDFID067","PDF","720x1440","MIPI","GC9702P","Free V.A","No TP","-20℃~70℃","400 nits","81.71*163.34*2.35","78.02*156.04"]
["7.0”","KD070HDFLD070","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-30℃~85℃","1100 nits","166.90*108.65*7.40","152.45*91.47","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-C010A","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","350 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA011-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","300 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDTLA020-C030A","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","CTP","-20℃~70℃","550 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDTLA020-C031A","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","CTP","-20℃~70℃","550 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDTLA020-TP","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","RTP","-20℃~70℃","490 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFPA019-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA019-C002A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA019-RT","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","630 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFLA013-01-C018A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","450 nits","182.07*117.60*7.55","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-C004A","PDF","800x480","LVDS","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","380 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-C007A-LVDS","PDF","800x480","LVDS","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","400 nits","182.07*117.60*13.75","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-TP","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","RTP","-20℃~70℃","430 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display"]
["7.0”","KD070WVTPA006-C005A","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","400 nits","165.0*100.00*8.18","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070WVTPA006-TP","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","RTP","-20℃~70℃","400 nits","165.00*100.00*7.19","154.08*85.92","Resistive Touch Display"]
["7.0”","KD070WVFPA065-C010A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","550 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA065-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","480 nits","165.40*104.59*7.00","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA043-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1100 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-C049A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-RT","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1000 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA028-C014A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","600 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA028-C015A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","600 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA028-RT","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","580 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFIA030-04-C026B","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","850 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFIA030-04-C027B","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","850 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-RT","PDF","1024x600","MIPI","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","480 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFIA030-C027A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD","Free V.A","CTP","-20℃~70℃","520 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLD070-C085A","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","CTP","-30℃~85℃","980 nits","182.45*121.47*9.38","152.45*91.47","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WXFID050-C065A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","103.56*162.38*4.73","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070HDFID067-C080A","PDF","720x1440","MIPI","GC9702P","Free V.A","CTP","-20℃~70℃","350 nits","101.73*186.34*3.53","78.02*156.04","Capacitive Touch Display"]
["7.0”","KD070WVTPA088","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","No TP","-30℃~85℃","500 nits","165.00*100.00*5.80","154.08*85.92","Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-RT","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-C004A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-C101A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","182.07*117.60*8.15","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA035A-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","Free V.A","No TP","-10℃~60℃","1100 nits","65.40*104.59*22.90","152.40*91.44","High-brightness TFT,HDMI TFT"]
["7.0”","KD070WVFLA035A-C049C-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","V.A 12H","CTP","-10℃~60℃","1000 nits","165.40*104.59*24.83","152.40*91.44","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["7.0”","KD070WXFID050-C038A-SP001A-TYPEC","PDF","800x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","119.46*176.78*15.80","94.20*150.72","Capacitive Touch Display,Type-C TFT"]
["7.0”","KD070WXFID093","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","1200 nits","103.46*162.28*7.63","94.20*150.72","High-brightness TFT"]
["7.0”","KD070HDFLA044","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1600 nits","165.10*100.10*5.50","154.21*85.92","High-brightness TFT"]
["7.0”","KD070HDFID086-C102A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID093A-C107A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1200 nits","119.46*176.78*7.27","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFLD083","PDF","800x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1200 nits","103.46*162.28*5.18","94.20*150.72","High-brightness TFT"]
["7.0”","KD070WVTLA095","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","No TP","-30℃~85℃","500 nits","165.00*100.00*5.80","154.08*85.92","Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-RT","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-C004A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-C101A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","450 nits","182.07*117.60*10.55","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLD092-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.62","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA044-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1600 nits","165.10*100.10*6.81","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID094","PDF","280x1424","MIPI","OTA7290N","Free V.A","No TP","-20℃~70℃","650 nits","38.20*181.47*3.40","33.60*170.88","Bartype TFT"]
["7.0”","KD070WXFID094-C074A","PDF","280x1424","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","600 nits","50.20*193.47*5.20","33.60*170.88","Capacitive Touch Display,Bartype TFT"]
["7.0”","KD070C-4-SP003A-HDMI","PDF","800x480","HDMI","TBD","V.A 12H","No TP","-10℃~60℃","450 nits","165.00*100.00*22.90","154.08*85.92","HDMI TFT"]
["7.0”","KD070HDFLD089","PDF","720x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1150 nits","96.30*167.70*5.22","86.94*154.56","High-brightness TFT"]
["7.0”","KD070HDFLD089-C102A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD092-C113A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.67","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099","PDF","800x480","RGB","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.10*100.10*5.10","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","850 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","1000 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WUFID085-C021A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-20℃~70℃","410 nits","119.46*176.78*19.30","94.50*151.20","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070WVFPA010-02-RTP","PDF","800x480","RGB","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","640 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLD092-C050B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","182.07*117.60*7.22","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVTPA006-02","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","No TP","-20℃~70℃","1000 nits","165.00*100.00*5.80","154.08*85.92","High-brightness TFT"]
["7.0”","KD070WXFID050-02","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~60℃","850 nits","103.56*162.38*2.70","94.20*150.72","High-brightness TFT"]
["7.0”","KD070WVFPA010-02-C010A","PDF","800x480","RGB","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","720 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLA116-CTP-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","550 nits","169.20*104.00*38.26","154.21*85.92","Capacitive Touch Display,Display Monitor"]
["7.0”","KD070FHFID078-01-C021A","PDF","1200x1920","MIPI","HX8279","Free V.A","CTP","-20℃~80℃","400 nits","119.46*176.78*3.98","94.50*151.20","Capacitive Touch Display"]
["7.0”","KD070FHFID078-01","PDF","1200x1920","MIPI","HX8279","Free V.A","No TP","-20℃~80℃","450 nits","98.70*160.80*1.96","94.50*151.20"]
["7.0”","KD070C-4-05-C004A-RS232","PDF","800x480","RS232","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070HDFIA030-C026A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD","Free V.A","CTP","-20℃~70℃","520 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070WVFPA043A-C049A-RS232","PDF","800x480","RS232","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-RS485","PDF","800x480","RS485","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-TTL","PDF","800x480","TTL","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-RS485","PDF","800x480","RS485","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070C-4-05-C004A-TTL","PDF","800x480","TTL","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070HDFLA028-02-C027B-SP001A-HDMI","PDF","1024x600","HDMI","EK73215&EK79001","Free V.A","CTP","-10℃~60℃","550 nits","165.00*100.00*22.27","154.21*85.92","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFIA030-02","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","No TP","-20℃~70℃","1700 nits","165.00*100.00*5.80","154.21*85.92","High-brightness TFT"]
["7.0”","KD070HDFIA030-02-C028A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-02-C029A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-02-RT","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","RTP","-20℃~70℃","1500 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLD106-C114A","PDF","800x480","LVDS","ST7277-G6-K","Free V.A","CTP","-20℃~70℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD110","PDF","720x1440","MIPI","GC9704","Free V.A","No TP","-20℃~70℃","400 nits","81.71*163.34*2.35","78.02*156.04"]
["7.0”","KD070HDFPA126","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","500 nits","164.90*100.00*2.80","154.21*85.92"]
["7.0”","KD070HDFPA126-C125A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","450 nits","164.90*100.00*4.40","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070WUFID123-C123A","PDF","1200x1920","MIPI","FT7250","Free V.A","CTP","-20℃~70℃","950 nits","109.80*173.00*5.00","94.50*151.20","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID094-CP001A-HDMI","PDF","280x1424","HDMI","OTA7290N","Free V.A","No TP","-20℃~70℃","900 nits","38.20*181.47*3.44","33.60*170.88","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.0”","KD070HDFPA127-C128A","PDF","1024x600","RGB","JD9165","Free V.A","CTP","-10℃~60℃","450 nits","164.86*99.96*5.28","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA051-01","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","780 nits","165.00*100.00*5.80","154.21*85.92"]
["7.0”","KD070HDFPA051-01-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","182.07*117.60*8.05","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070WVFLA125","PDF","800x480","LVDS","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA096","PDF","1024x600","LVDS","JD9165","Free V.A","No TP","-20℃~60℃","600 nits","164.90*100.00*2.80","154.21*85.92"]
["7.0”","KD070FHOIN128-C0000","PDF","1080x1920","MIPI","ICNA3512","Free V.A","CTP","-20℃~70℃","950 nits","89.13*160.91*1.01","87.13*154.91","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["7.0”","KD070HDFLD070-SP001A-HDMI","PDF","1280x768","HDMI","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-10℃~60℃","1200 nits","166.90*108.65*21.23","152.45*91.47","High-brightness TFT,HDMI TFT"]
["7.0”","KD070HDFPA038-C024A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-SP002A-HDMI","PDF","800x480","HDMI","EK9713/EK73002","V.A 12H","CTP","-10℃~60℃","400 nits","165.00*100.00*24.43","154.08*85.92","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFLA028-06-C014C","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLA028-06-RT","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","580 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFLA028-06","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","650 nits","165.00*100.00*5.75","154.21*85.92"]
["7.0”","KD070HDFLA028-06-C014A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLD106","PDF","800x480","LVDS","ST7277-G6-K","Free V.A","No TP","-20℃~70℃","950 nits","165.10*100.10*5.10","153.84*85.63","High-brightness TFT"]
["7.0”","KD070WVFPA043A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043A-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A-C049C","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WXFID050-C038A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-10℃~60℃","400 nits","119.46*176.78*4.75","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070WXFID050-02-C038A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","780 nits","119.46*176.78*4.75","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070HDFID086","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","1200 nits","96.30*167.70*5.22","86.94*154.56","High-brightness TFT"]
["7.0”","KD070C-4-05-CTP-002","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","182.07*117.60*8.13","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-05-C004A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA028-06-C015B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFPA136","PDF","1024x600","RGB","JD9168DA","Free V.A","No TP","-20℃~70℃","300 nits","164.86*99.96*3.50","154.21*85.92"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["7.0”","KD070WVFPA140","PDF","800x480","RGB","ST7277-G6-K","Free V.A","No TP","-30℃~85℃","1200 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD140-01-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","1050 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["7.0”","KD070WXFID138-C038B","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","119.46*176.78*6.46","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD092","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-30℃~85℃","1600 nits","165.10*100.10*5.12","154.21*85.92","High-brightness TFT,Wide Temp TFT"]
["7.3”","KD073WVFSN001","PDF","800x480","SPI","0110-53000018","Free V.A","No TP","15℃~35℃","0 nit","170.20*111.20*1.00","160.00*96.00","E-Paper Display"]
["7.3”","KD073WVFSN002","PDF","800x480","SPI","TBD","Free V.A","No TP","0℃~40℃","0 nit","170.20*111.20*0.85","160.00*96.00","E-Paper Display"]
["7.5”","KD075WVFSN001","PDF","800x480","SPI","JD79686","Free V.A","No TP","0℃~40℃","0 nit","170.20*111.20*1.25","163.20*97.92","E-Paper Display"]
["7.8”","KD078FHFBN003","PDF","1404x1872","MCU","HH7163 T-Con","Free V.A","No TP","0℃~50℃","0 nit","127.60*173.80*0.86","118.64*158.18","E-Paper Display"]
["7.84”","KD078HDFID004","PDF","400x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","1100 nits","67.60*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002","PDF","400x1280","RGB","GC9704C","Free V.A","No TP","-20℃~70℃","1000 nits","67.90*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFID006","PDF","400x1280","MIPI","OTA7290B","Free V.A","No TP","-20℃~70℃","480 nits","67.80*205.78*4.60","59.40*190.08","Bartype TFT"]
["7.84”","KD078HDFID004-C004A","PDF","400x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","950 nits","67.60*206.28*6.27","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002-C003A-RS232","PDF","400x1280","RS232","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS485","PDF","400x1280","RS485","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-TTL","PDF","400x1280","TTL","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFID004-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","No TP","-20℃~70℃","800 nits","67.60*206.28*19.29","59.40*190.08","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078HDFID004-C004A-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","CTP","-20℃~70℃","800 nits","67.60*206.28*21.12","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078FHFBN009","PDF","1404x1872","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","127.60*173.80*0.81","118.64*158.18","E-Paper Display"]
["8.0”","KD080WXFLD023-C015A-SP002A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","400 nits","130.70*200.10*22.15","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","8.0 inch Andriod Tablet","PDF","1200x1920","3G+32G","Andriod","Free V.A","CTP","-20 ℃~70℃","600 nits"]
["8.0”","KD080WXFID015","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~60℃","450 nits","114.50*184.00*2.85","107.64*172.22"]
["8.0”","KD080FM-8","PDF","1600x480","LVDS","HX8249/HX8678","Free V.A","No TP","-20℃~70℃","500 nits","208.00*73.00*5.50","194.40*58.32","Bartype TFT"]
["8.0”","KD080WXFID012","PDF","800x1280","MIPI","TBD","Free V.A","No TP","-20℃~60℃","230 nits","114.70*184.10*2.60","107.64*172.22"]
["8.0”","KD080C-4","PDF","800x600","RGB","TBD","V.A 6H","No TP","-20℃~70℃","350 nits","183.00*141.00*5.60","162.00*121.50"]
["8.0”","KD080WXFID015-C015A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*5.04","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080FM-8-C008A","PDF","1600x480","LVDS","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","420 nits","249.20*87.00*6.86","194.40*58.32","Capacitive Touch Display,Bartype TFT"]
["8.0”","KD080WXFID012-C008A","PDF","800x1280","MIPI","TBD","Free V.A","CTP","-20℃~60℃","200 nits","130.70*200.10*4.65","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080C-4-CTP-001","PDF","800x600","RGB","EK9713/EK7330","V.A 6H","CTP","-20℃~70℃","250 nits","199.00*157.00*7.93","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WXFLD023","PDF","800x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~60℃","450 nits","114.50*184.00*2.85","107.64*172.22"]
["8.0”","KD080WXFID015-C015A-SP004A-TYPEC","PDF","800x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*16.15","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080FHFID017-C016A-SP001A-TYPEC","PDF","1200x1920","Type C","NT51021","Free V.A","CTP","-10℃~50℃","250 nits","124.60*190.80*15.01","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080WXFID015-C015A-SP003A-HDMI","PDF","800x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~60℃","500 nits","130.70*200.10*22.09","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080C-5-01-C006B-CP001A-HDMI","PDF","1024x768","HDMI","TBD","V.A 12H","CTP","-10℃~60℃","300 nits","174.00*136.00*13.92","162.05*121.54","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080C-5-01-CP001A-HDMI","PDF","1024x768","HDMI","TBD","V.A 12H","No TP","-10℃~60℃","450 nits","174.00*136.00*11.53","162.05*121.54","HDMI TFT"]
["8.0”","KD080WUFLD027","PDF","1920x1200","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1500 nits","179.96*119.92*4.20","172.22*107.64","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080C-4-TP","PDF","800x600","RGB","TBD","V.A 6H","RTP","-20℃~70℃","270 nits","183.00*141.00*7.11","162.00*121.50","Resistive Touch Display"]
["8.0”","KD080WVTPA029","PDF","800x480","RGB","TBD","V.A 6H","No TP","-30℃~80℃","900 nits","192.80*116.90*6.40","176.64*99.36","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080WVFPA032","PDF","800x600","RGB","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WXFID015-C015A-RS232","PDF","800x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-RS485","PDF","800x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-TTL","PDF","800x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-02","PDF","800x1280","MIPI","ILI9881","Free V.A","No TP","-20℃~60℃","850 nits","114.70*184.20*2.70","107.64*172.22","High-brightness TFT"]
["8.0”","KD080WXFID015-02-C015A","PDF","800x1280","MIPI","ILI9881","Free V.A","CTP","-20℃~60℃","800 nits","130.70*200.10*4.90","107.64*172.22","Capacitive Touch Display,High-brightness TFT"]
["8.0”","KD080WVFLA034","PDF","800x600","LVDS","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WVFLA034-RT","PDF","800x600","LVDS","JD9165BA","Free V.A","RTP","-20℃~70℃","730 nits","182.90*141.00*7.20","162.00*121.50","Resistive Touch Display"]
["8.0”","KD080WVFLA034-C030A","PDF","800x600","LVDS","JD9165BA","Free V.A","CTP","-20℃~70℃","730 nits","199.00*157.00*7.87","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WVFPA032-RT","PDF","800x600","RGB","JD9165BA","Free V.A","RTP","-20℃~70℃","730 nits","182.90*141.00*7.20","162.00*121.50","Resistive Touch Display"]
["8.0”","KD080WVFPA032-C029A","PDF","800x600","RGB","JD9165BA","Free V.A","CTP","-20℃~70℃","730 nits","199.00*157.00*7.87","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WQOIN035","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WVFIA033","PDF","800x600","MIPI","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WXFID015-C008A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*4.84","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080WXFLD023-C015A","PDF","800x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*5.05","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080C-5-01-C006B","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-10℃~60℃","310 nits","174.00*136.00*4.83","162.05*121.54","Capacitive Touch Display"]
["8.0”","KD080WUFLD040","PDF","1920x1200","LVDS","FL5893DA","Free V.A","No TP","-20℃~70℃","1800 nits","181.80*119.85*5.35","172.22*107.64","High-brightness TFT"]
["8.0”","KD080WUFLD040-C034A","PDF","1920x1200","LVDS","FL5893DA","Free V.A","CTP","-20℃~70℃","1750 nits","181.80*119.85*7.40","172.22*107.64","Capacitive Touch Display,High-brightness TFT"]
["8.0”","KD080WQOIN035-C000-a","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["8.6”","KD086UXFLD001","PDF","600x1600","LVDS","GC9704","Free V.A","No TP","-20℃~70℃","350 nits","82.18*212.85*2.57","76.36*203.62","Bartype TFT"]
["8.6”","KD086UXFLD001-C001A","PDF","600x1600","LVDS","GC9704","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.6”","KD086UXFID002","PDF","600x1600","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","350 nits","82.18*212.85*2.57","76.36*203.62","Bartype TFT"]
["8.6”","KD086UXFID002-C001A","PDF","600x1600","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.9”","KD089FHFID004","PDF","480x1920","MIPI","OTA7290N","Free V.A","No TP","-20℃~70℃","950 nits","64.10*231.20*4.73","54.72*218.88","High-brightness TFT,Bartype TFT"]
["8.9”","KD089FHFID004-C001A","PDF","480x1920","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","850 nits","76.00*243.10*6.75","54.72*218.88","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["9.0”","KD090C-1-RT","PDF","800x480","RGB","TBD","V.A 6H","RTP","-20℃~70℃","300 nits","210.70*126.50*6.90","198.00*111.70","Resistive Touch Display"]
["9.0”","KD090C-1","PDF","800x480","RGB","TBD","V.A 6H","No TP","-20℃~70℃","300 nits","210.70*126.50*5.50","198.00*111.70"]
["9.0”","KD090HWFLA004","PDF","1280x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1000 nits","210.70*124.15*6.20","198.91*111.89","Wide Temp TFT,High-brightness TFT"]
["9.0”","KD090HDFLA006","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFLA006-SP001A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*22.50","196.61*114.15","High-brightness TFT,HDMI TFT"]
["9.0”","KD090HDFPA007","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFLA006-C001A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFLA006-RTP","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-RTP","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008-RTP","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFIA008-C001A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFLA006-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.7”","KD097HDFLD001-C001A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","0℃~50℃","240 nits","228.10*187.90*8.12","196.60*147.46","Capacitive Touch Display"]
["9.7”","KD097HDFLD001","PDF","1024x768","LVDS","TBD","Free V.A","No TP","0℃~50℃","240 nits","217.58*167.95*5.25","196.60*147.46"]
["9.8”","KD098WXTIA-001","PDF","1280x320","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1300 nits","252.75*73.17*11.00","241.15*60.29","Wide Temp TFT,High-brightness TFT"]
["10.0”","KD100UXFIN002","PDF","1200x1600","MIPI","HX8279","Free V.A","No TP","-20℃~70℃","0 nit","157.86*211.88*0.72","152.46*203.28","Reflective TFT"]
["10.1”","KD101HDFLA010","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","252.70*175.55*6.44","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA010-C016A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","252.70*175.55*9.25","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101UXFID008","PDF","1200x1920","MIPI","NT51021","Free V.A","No TP","-10℃~50℃","320 nits","159.00*244.60*2.30","135.36*216.58"]
["10.1”","KD101UXFID008-C014A","PDF","1200x1920","MIPI","NT51021","Free V.A","CTP","-10℃~50℃","300 nits","159.00*244.60*4.33","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101UXFLD009","PDF","1920x1200","LVDS","4*HX8255+2*HX8678","Free V.A","No TP","-30℃~80℃","400 nits","237.92*157.88*13.00","217.44*135.90","Wide Temp TFT"]
["10.1”","KD101WXFID018","PDF","800x1280","MIPI","JD9365AA","Free V.A","No TP","-20℃~60℃","380 nits","159.00*244.60*2.76","135.36*216.58"]
["10.1”","KD101WXFID018-C012A","PDF","800x1280","MIPI","JD9365AA","Free V.A","CTP","-20℃~60℃","300 nits","159.00*244.60*4.96","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID018-C012B","PDF","800x1280","MIPI","JD9365AA","Free V.A","CTP","-20℃~60℃","300 nits","159.00*244.60*4.96","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID018-01","PDF","800x1280","MIPI","JD9365AA","Free V.A","No TP","-20℃~60℃","650 nits","159.00*244.60*2.76","135.36*216.58"]
["10.1”","KD101UXFLD024-C035A","PDF","1920x1200","LVDS","HX8290-B","Free V.A","CTP","-20℃~70℃","500 nits","246.31*168.75*4.87","216.81*135.50","Capacitive Touch Display"]
["10.1”","KD101WXFID027","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~60℃","400 nits","143.00*228.60*2.66","135.36*216.58"]
["10.1”","KD101WXFID027-C012A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*4.86","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID027-C012B","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*4.86","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFLD021-01","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","550 nits","229.06*148.70*2.56","216.96*135.60"]
["10.1”","KD101FHFIA026","PDF","440x1920","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","750 nits","64.98*266.44*4.60","57.95*252.86","Bartype TFT"]
["10.1”","KD101WSFLD028-C040A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WXFLD035","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","500 nits","228.20*148.85*2.60","216.96*135.60"]
["10.1”","KD101WSFID033","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","No TP","-20℃~70℃","550 nits","235.10*143.20*2.80","222.72*125.28"]
["10.1”","KD101HDFLA034-01","PDF","1280x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","650 nits","238.60*148.00*6.50","223.68*125.82","Wide Temp TFT"]
["10.1”","KD101FHFID031","PDF","440x1920","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","1000 nits","65.08*266.19*4.48","57.95*252.86","High-brightness TFT,Bartype TFT"]
["10.1”","KD101FHFID031-C037A","PDF","440x1920","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*6.23","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["10.1”","KD101WSFID033-C040A","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFPD036","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","550 nits","235.10*143.20*2.80","222.72*125.28"]
["10.1”","KD101WSFPD036-C040A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101FHFID030-01","PDF","1200x1920","MIPI","HX8279D","Free V.A","No TP","-10℃~50℃","380 nits","143.00*228.60*2.60","135.36*216.58"]
["10.1”","KD101FHFID030-01-C014A","PDF","1200x1920","MIPI","HX8279D","Free V.A","CTP","-10℃~50℃","350 nits","159.00*244.60*4.81","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101FHFID030-C036A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","280 nits","174.37*255.12*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101FHFID030-C014A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101WXFID027-C012B-SP001A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*19.76","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101FHFID030-C014A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*19.40","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WXFLD021","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","450 nits","229.06*148.70*2.56","216.96*135.60","Wide Temp TFT"]
["10.1”","KD101WXFLD021-01-C009B","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~85℃","590 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101WXFLD021-C009B","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101WXFID045","PDF","1280x800","MIPI","EK79202DA","Free V.A","No TP","-30℃~85℃","550 nits","229.06*148.70*2.56","216.96*135.60","Wide Temp TFT"]
["10.1”","KD101WXFID045-C009B","PDF","1280x800","MIPI","EK79202D","Free V.A","CTP","-30℃~85℃","500 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101HDFLA020","PDF","1280x800","LVDS","EK79202B1","Free V.A","No TP","-20℃~70℃","1000 nits","232.70*155.55*5.00","216.96*135.60","High-brightness TFT"]
["10.1”","KD101WXFLD047-01-C001B","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","750 nits","229.06*148.70*4.71","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101WSFID033-C040A-SP001A-HDMI","PDF","1024x600","HDMI","EK73217& EK79007","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.76","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101HDFLD020-01-C045C-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","900 nits","232.70*155.56*24.50","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFLD051-01-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","700 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101HDFLD053-C064A-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","293.00*194.00*62.00","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD051-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","350 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFLD028-C040A-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","0℃~50℃","320 nits","258.10*166.10*43.23","222.72*125.28","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFPD036-C040A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101HDFLD054","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","1000 nits","228.60*149.10*4.38","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WSFLD028A-C040A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFID033A-C040A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFID033A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","No TP","-20℃~70℃","550 nits","235.10*143.20*2.80","222.72*125.28"]
["10.1”","KD101WSFPD036A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","550 nits","235.10*143.20*2.80","222.72*125.28"]
["10.1”","KD101WSFPD036A-C040A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101UXFLD024D","PDF","1920x1200","LVDS","HX8290-B","Free V.A","No TP","-20℃~70℃","1300 nits","229.46*149.10*7.65","216.81*135.50","High-brightness TFT"]
["10.1”","KD101HDFLA060-CTP-Monitor","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","500 nits","259.96*177.96*29.40","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD021-02-C045C-SP007A-HDMI","PDF","1280x800","HDMI","EK79202D_A","Free V.A","CTP","-20℃~70℃","700 nits","229.06*148.70*22.84","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WSFLA058","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.25","High-brightness TFT"]
["10.1”","KD101WSFLA058-C065A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101WSFPA055","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.28","High-brightness TFT"]
["10.1”","KD101WSFPA055-C065A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLD056A","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~80℃","1350 nits","228.80*147.90*4.66","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLD056A-C045E","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~80℃","1250 nits","252.96*171.60*6.91","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WSFIA057","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.28","High-brightness TFT"]
["10.1”","KD101WSFIA057-C065A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLD020-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","232.70*155.55*22.50","216.96*135.60","High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFLD047-01-SP001A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","600 nits","229.06*148.70*12.41","216.96*135.60","HDMI TFT"]
["10.1”","KD101HDFLA020-C016A","PDF","1280x800","LVDS","EK79202B1","Free V.A","CTP","-20℃~70℃","1100 nits","252.70*175.55*10.31","216.96*135.60","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101WXFLD021-C045C-RS232","PDF","1280x800","RS232","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-RS485","PDF","1280x800","RS485","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-TTL","PDF","1280x800","TTL","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101FHFID031-C037A-CP001A-HDMI","PDF","440x1920","HDMI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*12.29","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["10.1”","KD101WSFLA058-C065A-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","254.50*162.50*23.15","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101UXFLD024A-SP003A-HDMI","PDF","1920x1200","HDMI","TBD","Free V.A","No TP","-10℃~60℃","550 nits","226.37*148.81*19.04","216.81*135.50","HDMI TFT"]
["10.1”","KD101UXFLD024D-SP001A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1000 nits","229.46*149.10*22.73","216.81*135.50","High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLD069","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~60℃","1000 nits","229.30*149.10*2.60","216.96*135.60","High-brightness TFT"]
["10.1”","KD101WXFLD021A-C072A-Monitor","PDF","1280x800","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","258.25*176.05*26.68","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFLA058-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","235.00*143.00*20.90","222.72*125.28","High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLA059","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~85℃","1300 nits","229.46*149.10*7.06","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WXFID071","PDF","800x1280","MIPI","JD9365DA","Free V.A","No TP","-20℃~70℃","300 nits","143.00*228.60*2.60","135.36*216.58"]
["10.1”","KD101UXFLD024","PDF","1920x1200","LVDS","HX8290-B","Free V.A","No TP","-20℃~70℃","550 nits","226.37*148.81*2.67","216.81*135.50"]
["10.1”","KD101WXFLD047-01","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","850 nits","229.06*148.70*2.51","216.96*135.60","High-brightness TFT"]
["10.1”","KD101UXFLD024A-C035A","PDF","1920x1200","LVDS","ST5892B","Free V.A","CTP","-20℃~70℃","500 nits","246.31*168.75*4.87","216.81*135.50","Capacitive Touch Display"]
["10.1”","KD101FM-1-10-C032C-SP005A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","254.50*162.50*21.24","216.96*135.60","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WXFLD021-C045C","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*4.79","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101FHFID063-C070A","PDF","1200x1920","MIPI","OTA7290B","Free V.A","CTP","-10℃~50℃","450 nits","159.00*244.60*4.25","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101UXFLD024D-01-C035A-SP002A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1100 nits","246.31*168.75*23.98","216.81*135.50","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.3”","KD103WUFLD001","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","258.60*107.00*6.37","243.65*91.37","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["10.3”","KD103HDFMN005","PDF","2240x1680","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","216.70*174.40*0.71","209.67*157.25","E-Paper Display"]
["10.4”","KD104C-1","PDF","800x600","RGB","TBD","V.A 6H","No TP","-10℃~50℃","250 nits","228.40*175.40*5.90","211.20*158.40"]
["10.4”","KD104C-1-C002A","PDF","800x600","RGB","TBD","V.A 6H","CTP","-10℃~50℃","200 nits","228.40*175.40*8.28","211.20*158.40","Capacitive Touch Display"]
["10.4”","KD104C-1-CTP-001","PDF","800x600","RGB","TBD","V.A 6H","CTP","-10℃~50℃","250 nits","248.40*195.40*8.23","211.20*158.40","Capacitive Touch Display"]
["10.4”","KD104WSTPA003","PDF","1024x100","RGB","HX8282，HX8678","V.A 12H","No TP","-20℃~70℃","1000 nits","288.92*41.50*6.89","264.19*25.80","High-brightness TFT,Bartype TFT"]
["10.4”","KD104WSTPA-001","PDF","1024x100","RGB","HX8282-A*1, HX8678-C*1","V.A 12H","No TP","0℃~50℃","450 nits","288.92*41.50*7.12","264.19*25.80","Bartype TFT"]
["10.4”","KD104HDFLD006-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","No TP","-10℃~60℃","680 nits","236.00*174.34*18.95","211.20*158.40","HDMI TFT"]
["10.4”","KD104WVTLA009-CTP-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","750 nits","261.60*208.80*43.00","213.20*160.40","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104XGFLA011","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","238.60*175.80*9.20","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104WVTLA008","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","900 nits","228.40*175.40*5.90","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104HDFLA0018-C009A-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","350 nits","283.00*225.20*64.00","211.20*158.48","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104XGFLD022","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1200 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA011-C009A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1300 nits","266.13*221.29*12.54","210.43*157.82","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA022-01","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1050 nits","225.80*174.35*5.92","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104WVTPA028","PDF","800x600","RGB","TBD","V.A 6H","No TP","-20℃~60℃","400 nits","228.50*175.50*6.00","211.20*158.40"]
["10.4”","KD104XGFID025-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027-C011A","PDF","1024x768","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026","PDF","1024x768","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["11.6”","KD116WSFEA002","PDF","1920x1080","eDP","TBD","Free V.A","No TP","-20℃~70℃","1100 nits","268.00*158.00*4.87","256.32*144.18","High-brightness TFT"]
["11.6”","KD116FHFEA001-C001A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","800 nits","291.52*179.38*8.59","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["11.6”","KD116WSFEA003-CTP-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","1000 nits","298.22*186.10*44.00","257.32*145.18","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["11.6”","KD116UHFED004","PDF","3840x2160","eDP","TBD","Free V.A","No TP","-15℃~60℃","550 nits","265.90*158.20*3.00","256.90*144.50"]
["11.6”","KD116WSFEA002-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","268.00*158.00*21.56","256.32*144.18","High-brightness TFT,HDMI TFT"]
["11.6”","KD116WSFEA002-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","291.52*179.38*24.28","256.32*144.18","Capacitive Touch Display,HDMI TFT"]
["11.6”","KD116WSFEA002-C002A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","256.92*144.78","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFPA001","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~85℃","600 nits","260.50*204.00*8.80","245.76*184.32","Wide Temp TFT"]
["12.1”","KD121HDFPA001-C001B","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~85℃","600 nits","281.80*220.70*11.20","245.76*184.32","Capacitive Touch Display,Wide Temp TFT"]
["12.1”","KD121HDFLA007","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","278.00*184.00*10.00","261.12*163.20","High-brightness TFT"]
["12.1”","KD121HDFLA011","PDF","1280x800","LVDS","HX8245-J+HX8695-E","Free V.A","No TP","-30℃~80℃","400 nits","278.00*184.00*9.20","261.12*163.20","Wide Temp TFT"]
["12.1”","KD121HDFLA011-SP001A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","350 nits","278.00*184.00*15.60","261.12*163.20","HDMI TFT"]
["12.1”","KD121HDFLA009","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","283.00*185.10*9.40","261.12*163.20","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA013","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","800 nits","260.50*204.00*8.60","245.76*184.32","High-brightness TFT"]
["12.1”","KD121HDFLA014","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~85℃","800 nits","260.50*204.00*8.60","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA015-CTP-Monitor","PDF","1024x768","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","850 nits","294.50*233.00*44.00","247.00*185.50","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["12.1”","KD121HDFLA013-C007A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-20℃~70℃","700 nits","290.00*228.50*10.90","245.76*184.32","Capacitive Touch Display"]
["12.1”","KD121HDFLA013-C007A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","750 nits","290.00*228.50*31.94","245.76*184.32","Capacitive Touch Display,HDMI TFT"]
["12.1”","KD121HDFLD010-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1100 nits","306.50*196.20*14.50","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLD009-01-C006A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1350 nits","306.50*196.20*15.42","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121WVTLA029","PDF","800x600","LVDS","TBD","V.A 12H","No TP","-20℃~60℃","350 nits","276.00*209.00*9.00","246.00*184.50"]
["12.1”","KD121HDFLA030","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","450 nits","260.50*204.00*8.70","245.76*184.32"]
["12.1”","KD121HDFLA032","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","450 nits","260.50*204.00*8.70","245.76*184.32"]
["12.1”","KD121XGFLD024","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1250 nits","260.49*203.45*6.88","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFPA001-C001C","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-10℃~60℃","600 nits","281.80*220.70*11.00","245.76*184.32","Capacitive Touch Display"]
["12.1”","KD121HDFLA026","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","277.70*180.60*6.00","261.12*163.20","High-brightness TFT"]
["12.1”","KD121HDFLA026-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","294.10*196.20*8.10","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFLA042","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","400 nits","278.00*184.09*9.29","261.12*163.20","Wide Temp TFT"]
["12.1”","KD121UXFLA037","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1200 nits","276.60*179.50*5.70","262.83*164.27","High-brightness TFT"]
["12.1”","KD121UXFLA037-C014B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","305.00*200.00*8.65","262.83*164.27","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFLA035-C012B","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1200 nits","294.10*196.20*9.33","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.2”","KD122WXFLA001","PDF","1280x800","LVDS","HX8245","Free V.A","No TP","-20℃~70℃","400 nits","278.00*184.00*6.76","262.66*164.16"]
["12.3”","KD123WUFLA003","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","308.10*130.00*15.10","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD005","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.63*123.61*6.55","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD006","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.10*125.50*6.35","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLA002","PDF","1920x720","LVDS","HX8255A*4, HX8695H*1","Free V.A","No TP","-30℃~85℃","700 nits","312.90*132.20*13.20","292.03*109.51","Wide Temp TFT,Bartype TFT"]
["12.3”","KD123WUFLD006-C002A","PDF","1920x720","LVDS","TBD","Free V.A","CTP","-30℃~85℃","950 nits","311.02*132.60*9.15","292.03*109.51","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.8”","KD128FHFLD001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~85℃","700 nits","294.40*175.01*6.50","283.39*159.41","Wide Temp TFT"]
["12.8”","KD128FHFLD001-01","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~70℃","1000 nits","294.40*175.00*5.00","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["12.8”","KD128FHFLA002","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-40℃~85℃","800 nits","321.46*181.08*13.29","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["12.8”","KD128FHFLD003-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","650 nits","325.09*201.11*44.00","284.59*160.61","Display Monitor"]
["12.8”","KD128FHFLD001-01-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-30℃~85℃","650 nits","294.40*175.00*26.20","283.39*159.41","Wide Temp TFT,HDMI TFT"]
["12.8”","KD128OLED004","PDF","1728x1888","LVDS","HX8160-G01","Free V.A","No TP","-40℃~85℃","600 nits","224.96*248.22*5.80","218.76*239.02","AMOLED Display"]
["12.8”","KD128FHFLD001-01-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-30℃~85℃","550 nits","320.59*196.61*29.45","283.39*159.41","Capacitive Touch Display,Wide Temp TFT,HDMI TFT"]
["13.0”","KD130UXOEN001-C001A","PDF","2560x1440","eDP","RM98120","Free V.A","CTP","-40℃~85℃","800 nits","292.69*168.27*2.10","286.69*161.27","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["13.3”","KD133FHFED012","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","1250 nits","298.76*177.04*3.80","293.76*165.24","High-brightness TFT"]
["13.3”","KD133FHFED012-C008A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","750 nits","325.20*199.80*4.90","293.76*165.24","Capacitive Touch Display"]
["13.3”","KD133FHFLA013","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","800 nits","309.70*184.10*9.60","293.47*165.08","High-brightness TFT"]
["13.3”","KD133FHFLA013-C009A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","800 nits","325.20*199.80*9.65","293.47*165.08","Capacitive Touch Display,High-brightness TFT"]
["13.3”","KD133QHFSN014","PDF","960x680","SPI","SSD1677","Free V.A","No TP","0℃~40℃","0 nit","286.32*212.26*1.20","275.52*195.16","E-Paper Display"]
["13.3”","KD133FHFLA013-C009A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-20℃~70℃","900 nits","325.20*199.80*22.55","293.47*165.08","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["13.3”","KD133FHFLA013-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-20℃~70℃","950 nits","309.70*184.10*19.35","293.47*165.08","High-brightness TFT,HDMI TFT"]
["13.3”","KD133FHFLA013-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","300 nits","325.00*205.00*35.00","296.00*164.00","Display Monitor"]
["13.3”","KD133FHFLA015-C010A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","332.40*206.40*56.80","293.76*165.24","Capacitive Touch Display,Display Monitor"]
["13.3”","KD133FHFEA019","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","280 nits","300.36*177.54*2.50","293.76*165.24"]
["13.3”","KD133QXFEN020","PDF","1536x2048","eDP","TBD","Free V.A","No TP","0℃~50℃","300 nits","213.80*284.80*0.53","202.75*270.34","AMOLED Display,Flexible AMOLED,LTPS Display"]
["13.3”","KD133FHFED022","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","280 nits","300.26*177.39*2.60","293.76*165.24"]
["13.3”","KD133FHFED023","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","280 nits","300.26*177.39*2.80","293.76*165.24"]
["13.3”","KD133FHFED021","PDF","1920x1080","eDP","TBD","V.A 6H","No TP","0℃~50℃","200 nits","300.00*187.50*2.50","293.76*165.24"]
["13.3”","KD133FHFED023-C011A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","280 nits","325.20*199.80*6.00","293.76*165.24","Capacitive Touch Display"]
["13.3”","KD133FHFEA024","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","350 nits","300.26*187.50*2.50","293.76*165.24"]
["13.3”","KD133UXFMN026","PDF","2200x1650","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","287.00*215.50*0.86","270.60*202.95","E-Paper Display"]
["13.5”","KD135HDFLA001","PDF","1280x235","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","360.00*83.00*15.90","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.5”","KD135HDFLA001-C001A","PDF","1280x235","LVDS","TBD","Free V.A","CTP","0℃~50℃","800 nits","380.00*106.00*18.95","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.9”","KD139HDFLD001","PDF","1280x400","LVDS","HX8249/HX8678","Free V.A","No TP","0℃~50℃","1400 nits","358.50*135.00*13.30","337.92*105.14","High-brightness TFT,Bartype TFT"]
["14.0”","KD140C-1","PDF","1600x900","eDP","TBD","V.A 6H","No TP","0℃~50℃","250 nits","320.40*205.10*3.00","309.60*174.15"]
["14.0”","KD140FHFLD003","PDF","1920x1080","eDP","TBD","Free V.A","No TP","-20℃~70℃","800 nits","317.52*186.73*4.80","308.16*173.34","High-brightness TFT,LTPS Display"]
["14.0”","KD140FHFLD003-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","650 nits","317.52*186.73*27.77","308.16*173.34","HDMI TFT"]
["14.0”","KD140FHFLD003-C003A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","700 nits","337.49*206.76*7.58","308.16*173.34","Capacitive Touch Display,LTPS Display"]
["14.0”","KD140FHFEA010-C003B","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","450 nits","337.49*206.76*7.95","308.16*173.34","Capacitive Touch Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["14.5”","KD145OLEDN003-C003A","PDF","3000x1876","MIPI","HX5318","Free V.A","CTP","-20℃~70℃","400 nits","316.56*201.06*1.62","312.30*192.29","Capacitive Touch Display,AMOLED Display"]
["15.0”","KD150XGFLD002-C001A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","385.50*312.50*30.92","304.10*228.10","Capacitive Touch Display,HDMI TFT"]
["15.0”","KD150HDFLA007","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1200 nits","403.30*98.10*11.00","374.78*70.86","High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA007-C006B","PDF","1280x242","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","423.30*118.10*14.20","374.78*71.10","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["15.0”","KD150XGFLA009","PDF","1024x768","LVDS","TBD","V.A 12H","No TP","-20℃~70℃","300 nits","326.50*253.50*10.00","304.13*228.10"]
["15.0”","KD150HDFLA008","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","403.30*98.10*14.00","374.79*70.86","High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA015","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","350 nits","326.50*253.50*9.60","304.13*228.10"]
["15.0”","KD150HDFLA013","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","500 nits","326.50*253.50*9.60","304.13*228.10"]
["15.0”","KD150HDFLD014","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-10℃~50℃","350 nits","312.70*241.00*3.20","304.13*228.10"]
["15.0”","KD150HDFLD016","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","400 nits","314.25*245.42*3.25","304.13*228.10"]
["15.0”","KD150XGFLD002","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","450 nits","326.50*253.50*9.00","304.10*228.10","Wide Temp TFT"]
["15.1”","KD151WQOEN001-C0000","PDF","2560x1600","eDP","RM98121","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*1.30","324.10*202.56","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["15.1”","KD151WQOEN001-SP001A-HDMI","PDF","2560x1600","HDMI","TBD","Free V.A","No TP","-40℃~85℃","550 nits","328.90*210.46*5.80","324.10*202.56","AMOLED Display,Wide Temp TFT,LTPS Display,HDMI AMOLED"]
["15.6”","KD156FM-1","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","220 nits","359.50*223.80*3.20","344.16*193.59"]
["15.6”","KD156FM-1-01-C003A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","220 nits","425.76*275.19*6.90","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156FHFEA005","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","450 nits","350.72*216.40*2.94","344.16*193.59"]
["15.6”","KD156FHFLA007","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","310 nits","351.86*206.33*6.50","344.16*193.59"]
["15.6”","KD156FHFLA007-C004A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","280 nits","373.58*228.33*11.05","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156FHFLD010","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","450 nits","350.92*206.30*3.00","344.16*193.59"]
["15.6”","KD156FHFLA011","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","360.00*212.30*5.70","344.16*193.59","High-brightness TFT"]
["15.6”","KD156FHFLA012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","363.80*215.90*9.30","344.16*193.59","Wide Temp TFT,High-brightness TFT"]
["15.6”","KD156WSFED019","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","350 nits","350.66*205.78*4.98","344.16*193.59"]
["15.6”","KD156FHFLA014","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","700 nits","363.80*215.90*12.60","344.16*193.59"]
["15.6”","KD156WSFED020","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","350 nits","350.76*204.96*4.80","344.16*193.59"]
["15.6”","KD156WSFEA016-01-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","300 nits","398.00*248.00*46.50","343.54*192.83","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFED015","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","500 nits","350.72*216.40*2.90","344.16*193.59"]
["15.6”","KD156FHFED015-C010A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","400 nits","385.70*235.70*5.20","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156UHOEN018","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*1.05","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156FHFLA021-C011A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","376.40*236.40*43.20","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFED024-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","300 nits","388.55*240.98*41.00","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFLA022-C008A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~80℃","750 nits","392.00*242.00*15.55","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156FHFLA022-01","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","1200 nits","363.80*215.90*9.50","344.16*193.59","High-brightness TFT"]
["15.6”","KD156FHFLA022-02","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","800 nits","363.80*215.90*9.50","344.16*193.59","High-brightness TFT"]
["15.6”","KD156UHOEN025","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.22*201.62*1.10","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN018-C014A","PDF","3840x2160","eDP","RM98110","Free V.A","CTP","-20℃~70℃","320 nits","357.22*208.27*3.35","344.22*193.62","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["15.6”","KD156UHFED040","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","600 nits","350.66*216.23*2.45","344.22*193.62"]
["15.6”","KD156FHFED030","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","350 nits","359.50*223.75*3.10","344.16*193.59"]
["15.6”","KD156FHFLA035","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","500 nits","363.80*215.90*8.80","344.16*193.59"]
["15.6”","KD156UHOEN018-SP001A-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*15.00","344.22*193.62","AMOLED Display,LTPS Display,HDMI AMOLED"]
["16.7”","KD167FHFLA001","PDF","1920x540","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1200 nits","439.00*144.00*14.00","408.96*115.02","High-brightness TFT,Bartype TFT"]
["17.0”","KD170SXFLA001","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","-20℃~70℃","500 nits","358.50*296.50*10.30","337.92*270.34"]
["17.0”","KD170SXFLA002","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","0℃~50℃","900 nits","358.50*296.50*10.30","337.92*270.34","High-brightness TFT"]
["17.0”","KD170SXTLA003","PDF","1280x1024","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1400 nits","358.50*296.50*10.50","337.92*270.34","Wide Temp TFT,High-brightness TFT"]
["17.0”","KD170UVFLA004","PDF","1280x960","LVDS","TBD","Free V.A","No TP","0℃~50℃","240 nits","359.00*284.70*8.60","345.41*259.06"]
["18.5”","KD185FHFLA003","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","350 nits","430.40*254.60*12.00","408.96*230.04","Wide Temp TFT"]
["18.5”","KD185FHFLA004","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","800 nits","430.37*254.60*11.50","408.96*230.04","High-brightness TFT"]
["18.5”","KD185FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1000 nits","430.40*254.60*12.00","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["18.5”","KD185FHFLA010","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","430.37*254.60*11.50","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["18.5”","KD185FHFLD013","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","430.37*254.60*9.30","408.96*230.04"]
["19.0”","KD190SGFLA003","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","0℃~50℃","240 nits","396.00*324.00*10.90","376.32*301.06"]
["19.0”","KD190SXTLA004","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","-30℃~85℃","450 nits","396.00*324.00*12.88","376.32*301.06","Wide Temp TFT"]
["19.0”","KD190SGFLA005","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","-20℃~70℃","900 nits","395.60*323.80*15.00","376.32*301.06","High-brightness TFT"]
["19.0”","KD190SGFLA005-C002A-SP001A-HDMI","PDF","1280x1024","HDMI","TBD","Free V.A","CTP","-10℃~60℃","720 nits","423.00*347.70*37.00","376.32*301.06","HDMI TFT"]
["19.0”","KD190SGFLA005-C002A","PDF","1280x1024","LVDS","TBD","Free V.A","CTP","-20℃~70℃","750 nits","423.00*347.70*19.00","376.32*301.06","Capacitive Touch Display"]
["19.0”","KD190SXFLA007-01-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","710 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["19.0”","KD190SXFLA007-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","270 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["20.8”","KD208FHFLA001","PDF","1920x184","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","592.00*75.00*12.30","527.04*50.60","Bartype TFT"]
["21.5”","KD215FHFLA004","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","350 nits","495.60*292.20*10.70","476.64*268.11"]
["21.5”","KD215FHFLD006","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","487.86*276.25*12.89","478.66*260.28"]
["21.5”","KD215FHFLD007","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","495.60*292.20*10.57","476.06*267.79","High-brightness TFT"]
["21.5”","KD215WSFVA009F-Monitor","PDF","1920x1080","HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","510 nits","523.64*315.11*59.30","475.64*267.11","Display Monitor"]
["21.5”","KD215WSFVA009E-Monitor","PDF","1920x1080","HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","500 nits","523.64*315.11*59.30","475.64*267.11","Display Monitor"]
["21.5”","KD215WSFVA017-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~45℃","550 nits","493.26*284.13*35.59","478.67*260.28","Display Monitor"]
["21.5”","KD215WSFVA018-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~45℃","710 nits","493.26*284.13*35.59","478.67*260.28","Display Monitor"]
["21.5”","KD215WSFVA011-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","400 nits","510.00*306.60*56.20","475.64*268.11","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215WSFLA012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","495.60*292.20*10.62","476.05*267.79","High-brightness TFT"]
["21.5”","KD215WSFLA013","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","700 nits","484.56*284.49*12.50","476.05*267.79"]
["21.5”","KD215WSFLA014","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","850 nits","484.56*284.49*12.50","476.05*267.79"]
["21.5”","KD215WSFLA015","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","650 nits","484.56*284.49*12.50","476.05*267.79"]
["21.5”","KD215WSFVA009-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","750 nits","532.20*319.40*46.50","479.60*270.90","Display Monitor"]
["21.5”","KD215WSFVA017A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","492.70*283.90*44.40","478.66*260.28","Display Monitor"]
["21.5”","KD215FHFLA023-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLD007-C005A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","505.60*302.20*13.97","476.06*267.79","Capacitive Touch Display,High-brightness TFT"]
["21.5”","KD215FHFLA022","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~85℃","1000 nits","495.60*292.20*10.50","476.64*268.11","Wide Temp TFT,High-brightness TFT"]
["21.5”","KD215FHFLA023-C007A-Monitor-TR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLA026","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","400 nits","495.60*292.40*10.50","476.64*268.11","Wide Temp TFT"]
["21.5”","KD215FHFLA026-C005B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~80℃","400 nits","505.60*302.20*13.90","476.64*268.11","Capacitive Touch Display,Wide Temp TFT"]
["23.0”","KD230FHFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","200 nits","533.20*312.00*10.50","509.18*286.42"]
["23.6”","KD236FHFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","544.80*320.50*18.70","521.28*293.22","High-brightness TFT"]
["23.6”","KD236WSFLD002-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","180 nits","559.00*335.00*56.20","521.47*293.10","Capacitive Touch Display,Display Monitor"]
["23.6”","KD236WSFLD002-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~50℃","180 nits","559.00*335.00*56.20","521.47*293.10","Display Monitor"]
["23.6”","KD236SXFLA003","PDF","1280x1280","LVDS","TBD","Free V.A","No TP","-20℃~80℃","1500 nits","657.00*657.00*28.65","599.42*599.42","High-brightness TFT,Round TFT"]
["23.8”","KD238FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1500 nits","544.80*320.50*11.50","527.04*296.46","High-brightness TFT"]
["23.8”","KD238FHFLA008","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","600 nits","543.00*317.40*8.20","527.04*296.46"]
["23.8”","KD238FHFVA010-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","583.17*356.46*70.95","524.37*298.46","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["23.8”","KD238FHFVA011-C006A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~45℃","300 nits","598.00*370.00*58.00","529.00*297.50","Display Monitor"]
["23.8”","KD238FHFVA012-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~45℃","300 nits","598.00*370.00*58.00","529.00*297.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270FHFLA002","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","800 nits","630.00*368.20*13.00","597.89*336.31","High-brightness TFT"]
["27.0”","KD270UDOEN003","PDF","3840x2160","eDP","TBD","Free V.A","No TP","-20℃~70℃","400 nits","607.66*348.18*1.24","597.66*336.18","AMOLED Display,LTPS Display"]
["27.0”","KD270WSFLA004-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","180 nits","644.40*382.60*59.40","597.60*336.15","Display Monitor"]
["27.0”","KD270WSFLA004-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","180 nits","644.40*382.60*59.40","597.60*336.15","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270WSFLA005-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","300 nits","645.40*383.20*62.50","598.00*336.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270QHFLA007","PDF","2560x1440","LVDS","TBD","Free V.A","No TP","0℃~50℃","550 nits","613.60*356.85*10.40","596.74*335.66"]
["27.0”","KD270UDFEA006","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","250 nits","609.40*355.60*13.30","596.74*335.66"]
["27.0”","KD270UDFEA008","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","1200 nits","612.20*358.20*14.63","596.74*335.66","High-brightness TFT"]
["27.0”","KD270QHFLA011","PDF","2560x1440","LVDS","TBD","Free V.A","No TP","0℃~50℃","550 nits","614.00*357.05*12.80","596.74*335.66"]
["27.0”","KD270FHFLD012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","350 nits","611.60*352.68*5.00","597.89*336.31"]
["27.0”","KD270FHFVA014-C004A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","402.11*660.90*82.60","336.31*593.43","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["27.0”","KD270UDOEN003-C002B","PDF","3840x2160","eDP","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*4.19","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*13.60","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270FHFLA015","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","630.00*368.20*13.00","597.89*336.31"]
["27.0”","KD270FHFVA020-C009A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~45℃","300 nits","678.00*420.00*58.00","598.00*343.00","Display Monitor"]
["27.0”","KD270FHFVA021-C010A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","678.00*420.00*58.00","598.00*343.00","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA017-C006A-Monitor","PDF","3840x2160","HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA018-C007A-Monitor","PDF","3840x2160","HDMI/DP","TBD","Free V.A","No TP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Display Monitor"]
["27.0”","KD270QHOVD026","PDF","2560x1440","V-By-One","TBD","Free V.A","No TP","0℃~45℃","1300 nits","600.62*346.42*0.78","586.75*330.05","AMOLED Display,High-brightness TFT,LTPS Display"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,Display Monitor,OLED Monitor"]
["27.0”","KD270FHFLA022","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","2000 nits","618.00*360.00*20.80","597.90*336.30","High-brightness TFT"]
["27.0”","KD270FHFLA025","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","630.00*368.20*13.00","597.89*336.31","High-brightness TFT"]
["27.0”","KD270UHFEA023","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","500 nits","615.67*360.26*8.60","596.74*335.66"]
["27.0”","KD270UHFEA024","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","800 nits","615.67*360.26*8.60","596.74*335.66","High-brightness TFT"]
["27.0”","KD270UHFVA016-C005A-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270QHFLA029","PDF","2560x1440","LVDS","TBD","Free V.A","No TP","0℃~50℃","2200 nits","630.74*369.26*20.00","596.74*335.66","High-brightness TFT"]
["27.0”","KD270UHFLA030","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","1200 nits","630.74*369.26*20.00","596.74*335.66","High-brightness TFT"]
["28.0”","KD280FM-1","PDF","1920x360","LVDS","TBD","Free V.A","No TP","0℃~50℃","700 nits","729.30*167.30*19.20","698.40*130.95","Bartype TFT"]
["28.0”","KD280FHFLA001","PDF","1920x360","LVDS","TBD","Free V.A","No TP","0℃~50℃","700 nits","732.00*165.00*16.80","699.84*131.22","Bartype TFT"]
["31.2”","KD312HDFMN001","PDF","720x1280","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","697.20*402.80*1.30","691.20*388.80","E-Paper Display"]
["31.5”","KD315FHFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","725.20*422.70*14.40","698.40*392.85","High-brightness TFT"]
["31.5”","KD315WSFVA002-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","210 nits","739.00*435.00*59.30","698.60*390.10","Display Monitor"]
["31.5”","KD315WSFVA002-ITP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","Infrared Ray TP","0℃~50℃","250 nits","756.70*451.30*59.00","698.60*392.10","Display Monitor"]
["31.5”","KD315WSFVA002-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","748.60*451.20*51.00","698.60*392.10","Capacitive Touch Display,Display Monitor"]
["31.5”","KD315FHFLA001-C001A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","900 nits","746.70*441.30*19.80","698.40*392.85","Capacitive Touch Display,High-brightness TFT"]
["31.5”","KD315UHFLA004","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","200 nits","714.50*411.50*39.90","698.40*392.85"]
["31.5”","KD315WSFVA005-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","290 nits","789.40*483.85*73.00","697.40*391.85","Display Monitor"]
["31.5”","KD315WSFVA006-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","300 nits","781.50*476.00*46.00","698.40*391.30","Display Monitor"]
["31.5”","KD315WSFVA003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","718.80*421.70*58.70","698.40*392.85","Display Monitor"]
["31.5”","KD315WSFVA003A-01-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","718.80*421.70*58.70","698.40*392.85","Display Monitor"]
["31.5”","KD320UHOVD017","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~45℃","230 nits","709.68*407.43*0.80","696.58*391.82","AMOLED Display,LTPS Display"]
["31.5”","KD320FHFLA019","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~60℃","800 nits","727.00*420.00*9.70","698.40*392.85","High-brightness TFT"]
["31.5”","KD320UHFEA020","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","800 nits","727.00*420.00*9.70","697.31*392.23","High-brightness TFT"]
["32.0”","KD320FHFUA003-C003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","400 nits","745.50*440.50*66.50","698.00*393.00","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1700 nits","719.40*416.90*26.60","698.40*392.90","High-brightness TFT,Mini-LED"]
["32.0”","KD320FHFVA006-C005A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","464.82*764.72*97.06","394.82*694.61","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA008-C006A-C1600-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","462.00*762.51*100.03","394.80*693.89","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA011-C1800-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","719.70*420.60*118.70","698.40*392.85","Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA009-C008A-Monitor-BR","PDF","1920x1080","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","463.90*769.40*54.90","394.80*700.40","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320UHFVA007-C007A-Monitor","PDF","3840x2160","HDMI/DP/USB","TBD","Free V.A","CTP","0℃~40℃","300 nits","789.00*485.00*58.20","697.30*392.20","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320UHFEA011","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","450 nits","725.20*422.70*14.40","697.31*392.23"]
["34.0”","KD340UWFVA001-C1500-Monitor","PDF","3440x1440","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","808.70*362.40*126.42","797.22*333.72","Curved Monitor,Display Monitor"]
["42.5”","KD425WSFVA003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","955.20*556.21*94.45","940.90*529.25","Display Monitor"]
["42.5”","KD430FHFLA019","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-5℃~50℃","1000 nits","969.30*557.65*15.00","940.90*529.25","High-brightness TFT"]
["43.0”","KD430WUFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1500 nits","973.20*561.50*29.50","941.18*529.42","High-brightness TFT"]
["43.0”","KD430UHFVA009-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.01*992.60*133.87","530.15*925.79","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA010-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.25*1005.29*164.61","530.75*927.01","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA011-C003A-C1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1003.64*606.45*136.13","925.90*529.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA012-C004A-J1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1016.87*606.45*136.03","933.40*530.75","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430FHFVA014-C006A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","1007.70*595.40*53.60","943.10*529.80","Capacitive Touch Display,Display Monitor"]
["43.0”","KD430UHFVA013-C005A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1028.43*619.42*63.40","941.18*529.42","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFLA018","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","969.30*557.65*15.00","941.18*529.42","High-brightness TFT"]
["49.0”","KD490UHFVA006-C001A-C1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1134.82*122.65","605.03*1053.83","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA007-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1142.15*150.91","605.03*1064.95","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA008-C003A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1168.03*702.00*76.70","1085.50*604.00","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA019","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1103.20*633.40*15.20","1073.78*604.00","High-brightness TFT"]
["49.0”","KD490UHFVA020-C1500-Monitor","PDF","3840x1080","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","1200.00*360.00*43.00","--","Curved Monitor,Display Monitor"]
["55.0”","KD550WSFVA001-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","450 nits","1251.00*722.00*59.30","1210.60*677.10","Display Monitor"]
["55.0”","KD550WSFVA002A-Monitor","PDF","3840x2160","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","1225.70*705.60*82.30","1209.60*680.40","Display Monitor"]
["55.0”","KD550WSFVA005-C002A-J1500-Monitor","PDF","3840x2160","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","772.40*1291.82*207.07","698.20*1227.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA006-C003A-C1800-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","756.80*1270.02*167.40","681.40*1174.66","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA007-C004A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1302.12*780.40*78.70","1209.60*680.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA011-C005A-S1200-Monitor","PDF","3840x2160","HDMI/DP/RS232","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","1293.10*833.40*48.30","1227.40*698.20","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA032","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1239.00*709.80*16.00","1209.60*680.40","High-brightness TFT"]
["64.5”","KD650UHFVA002","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1458.88*833.92*18.50","1428.48*803.52","High-brightness TFT"]

{"sheet":"Capacitive Touch Display","index":1,"n_rows":671,"n_cols":13,"rows_kept":671}
["STARTEK Capacitive Touch Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.0”","KD010LQOSN001-C0000","PDF","340x340","QSPI","SH8601","Free V.A","CTP","-10℃~60℃","630 nits","29.25*30.00*0.68","26.35*26.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN001-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","650 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.4”","KD014HVOIN011-C0000","PDF","320x360","MIPI","FT2390","Free V.A","CTP","-20℃~60℃","450 nits","25.74*29.87*0.79","23.84*26.82","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.5”","KD015QVFMN002-C001B","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","320 nits","37.52*41.10*4.45","27.72*27.72","Capacitive Touch Display,Square TFT"]
["1.5”","KD015QVFMD020-C001D","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","800 nits","37.52*41.10*3.82","27.72*27.72","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["1.6”","KD016HVOMN002-C001A","PDF","320x360","MIPI&SPI","RM69092","Free V.A","CTP","-20℃~70℃","320 nits","31.32*36.05*2.05","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016WVFID001-C002A","PDF","400x400","MIPI","ST7797","Free V.A","CTP","-20℃~70℃","350 nits","51.94*52.94*3.09","39.84*39.84","Capacitive Touch Display,Round TFT"]
["1.6”","KD016HVOQN006-C000O","PDF","320x360","QSPI","RM69092","Free V.A","CTP","-20℃~70℃","450 nits","28.92*33.35*0.76","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.77”","KD018QVFIN016-C001A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","450 nits","39.70*52.50*4.85","26.64*35.52","Capacitive Touch Display"]
["1.77”","KD018QQTBN009-C002A","PDF","128x160","SPI&MCU","ST7735S","V.A 12H","CTP","-20℃~70℃","400 nits","39.70*52.50*4.25","28.03*35.04","Capacitive Touch Display"]
["1.77”","KD018QVFMN010-02-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","200 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*4.85","26.64*35.52","Capacitive Touch Display"]
["1.78”","KD017HVOSN005-C000","PDF","368x448","QSPI/SPI","CO5300","Free V.A","CTP","-20℃~60℃","450 nits","33.50*40.89*2.58","28.70*34.94","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.96”","KD019HVOSN001-C001A","PDF","410x502","QSPI","CO5300AF-46","Free V.A","CTP","-10℃~60℃","600 nits","35.37*42.40*2.76","31.37*38.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.0”","KD020LQFMA014-C003A","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","CTP","-20℃~70℃","550 nits","54.50*47.56*4.15","40.80*30.60","Capacitive Touch Display"]
["2.0”","KD019QQFBN002-C001A","PDF","128x160","SPI&MCU","ST7735","Free V.A","CTP","-20℃~70℃","900 nits","47.47*59.04*3.20","31.87*39.84","Capacitive Touch Display,High-brightness TFT"]
["2.0”","KD020QVFIA013-C001A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","550 nits","35.80*52.10*4.40","30.60*40.80","Capacitive Touch Display"]
["2.0”","KD020LQRMA017-C003A","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","CTP","-20℃~70℃","300 nits","54.50*47.56*4.35","40.80*30.60","Capacitive Touch Display,Transflective TFT"]
["2.0”","KD020WQFPA023-C003B","PDF","480x360","SPI+RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024-C003B","PDF","480x360","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","820 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020LQFMA014-C003A-RS232","PDF","320x240","RS232","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-RS485","PDF","320x240","RS485","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-TTL","PDF","320x240","TTL","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS232","PDF","480x360","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS485","PDF","480x360","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020WQFPA023-C003B-TTL","PDF","480x360","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020QVFMA009-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020QVFMA009-C008A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","420 nits","35.80*52.10*2.65","30.60*40.80","Capacitive Touch Display"]
["2.06”","KD020HVOSN001","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","34.79*43.14*0.78","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001-C001A","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","36.70*44.21*2.55","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002-C002B","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","550 nits","37.35*45.15*2.31","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","600 nits","34.79*43.14*0.83","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.1”","KD021WVFID002-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFPD003-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFPD011-C001A","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVOSN009-C003B","PDF","480x480","QSPI","CO5300AF","Free V.A","CTP","-20℃~60℃","600 nits","42.39*42.39*2.55","38.39*38.39","Capacitive Touch Display,AMOLED Display,Square TFT,LTPS Display"]
["2.2”","KD022QVTBD032-C002A","PDF","240x320","MCU","ST7789V","V.A 6H","CTP","-20℃~70℃","240 nits","41.70*56.16*4.63","33.48*44.64","Capacitive Touch Display"]
["2.2”","KD022QVFMD018-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.3”","KD023C-1-C004A","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","CTP","-20℃~70℃","280 nits","55.20*51.60*4.18","46.75*35.06","Capacitive Touch Display"]
["2.4”","KD024QVFIA073-02-C021B","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","48.72*70.26*3.95","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFIA073-C009A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*4.25","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFIA073-C021A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","500 nits","48.72*70.26*4.25","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits","42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA021-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","450 nits","42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVRMA041A-C012A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","300 nits","42.92*60.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024HVFID078-01-C029A","PDF","320x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","44.52*69.88*4.38","33.12*49.68","Capacitive Touch Display"]
["2.4”","KD024HVFPD079-01-C029A","PDF","320x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","700 nits","44.52*69.88*4.38","33.12*49.68","Capacitive Touch Display"]
["2.4”","KD024WVFLD101-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024VGFPD094-C021D","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFID095-C021D","PDF","480x640","MIPI","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFPD094-C021D-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA021-C003B","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","350 nits","48.72*70.26*4.03","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-06-C003A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits"," 42.92*60.26*3.75","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024QVFMA020-C009A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVRMA038A-C015A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","220 nits","48.72*70.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024VGFPD094-C042A","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","900 nits","42.92*60.26*3.95","36.72*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102-C001A-RS232","PDF","800x480","RS232","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-RS485","PDF","800x480","RS485","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-TTL","PDF","800x480","TTL","HX8283-A","Free V.A","CTP","-20℃~70℃","670 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFIA073-03-C009B","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","550 nits","42.92*60.26*3.53","36.72*48.96","Capacitive Touch Display"]
["2.4”","KD024WVFLD101A-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024VGFPD094-C021D-SP002A-HDMI","PDF","480x640","HDMI","ST7701SI","Free V.A","CTP","-20℃~70℃","700 nits","48.72*70.26*20.00","36.72*48.96","Capacitive Touch Display,HDMI TFT"]
["2.4”","KD024WVFPD102A-C001A","PDF","800x480","RGB","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.5”","KD025EGOIN002-C000","PDF","400x712","MIPI","RM690C0","Free V.A","CTP","-20℃~70℃","800 nits","32.90*58.56*2.00","31.10*55.36","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["2.6”","KD026QVFMD007-C006A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","400 nits","46.00*64.00*4.08","39.60*52.80","Capacitive Touch Display"]
["2.6”","KD026LQTMA008-C001A","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","CTP","-20℃~70℃","270 nits","60.30*51.15*4.05","52.80*39.60","Capacitive Touch Display"]
["2.6”","KD026WXFLD022-C008A","PDF","1280x720","LVDS","SC5014","Free V.A","CTP","-20℃~70℃","1200 nits","73.88*53.46*4.37","57.60*32.40","Capacitive Touch Display,High-brightness TFT"]
["2.6”","KD026HVRMA010-C004B","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","CTP","-30℃~85℃","420 nits","46.76*65.85*4.26","39.84*53.78","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026WXFLD022-C008A-RS232","PDF","1280x720","RS232","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-TTL","PDF","1280x720","TTL","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-RS485","PDF","1280x720","RS485","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.7”","KD027HVFMD010-C004A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009-C004A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A-RS232","PDF","320x320","RS232","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-RS485","PDF","320x320","RS485","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-TTL","PDF","320x320","TTL","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","50.50*69.70*3.85","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-C004A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","56.10*77.29*4.10","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-CTP-001","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","430 nits","56.10*77.29*4.38","44.20*58.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA005-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","410 nits","50.20*69.70*3.85","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028FM-1-01-C019A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","750 nits","56.10*77.29*3.69","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA013-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFMA011-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVTMA005-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.20*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFIA038-C018A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","610 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028VGFID048-C026A","PDF","480x640","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028VGFPD047-C026A","PDF","480x640","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFID051-C028A","PDF","240x320","MIPI","JD9852","Free V.A","CTP","-20℃~70℃","610 nits","50.50*69.70*4.14","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028VGFPD047-C026A-SP001A-HDMI","PDF","480x640","HDMI","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,HDMI TFT"]
["2.8”","KD028WXFPD057-C040A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028WXFID056-C040A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028VGFID048-C026A-SP002A-TypeC","PDF","480x640","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*15.00","43.20*57.60","Capacitive Touch Display,Type-C TFT"]
["2.8”","KD028QVTMA005-C020A-RS232","PDF","240x320","RS232","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-RS485","PDF","240x320","RS485","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-TTL","PDF","240x320","TTL","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*19.00","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVRMD073-C050A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~80℃","150 nits","52.90*79.30*3.95","43.20*57.60","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVFMA011-02-C020A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display"]
["2.8”","KD028QVFMA058-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~85℃","630 nits","50.50*69.70*3.85","43.20*57.60","Capacitive Touch Display,Wide Temp TFT"]
["2.9”","KD029QHFPD002-C001A","PDF","376x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFID001-C004A","PDF","376x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFPD002-C004A","PDF","376x960","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFID001-C001A-SP001A-HDMI","PDF","376x960","HDMI","SC7283","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,HDMI TFT"]
["3.0”","KD030WQFMD019-C020B","PDF","240x400","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*4.30","38.88*64.80","Capacitive Touch Display"]
["3.0”","KD030NHFIN015B-C008A","PDF","360x640","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","300 nits","48.14*83.50*3.82","36.72*65.28","Capacitive Touch Display"]
["3.0”","KD030NHFPN017-C015A","PDF","360x640","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","300 nits","52.57*83.28*4.22","36.72*65.28","Capacitive Touch Display"]
["3.0”","KD030FWFPN022A-C018A","PDF","480x854","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030FWFIN021A-C018A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030WVFID029-C028A","PDF","268x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030WVFPD030-C028A","PDF","268x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","650 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030C-2-C003A","PDF","240x400","MCU&RGB","ILI9327","V.A 12H","CTP","-20℃~70℃","270 nits","45.04*77.00*3.85","38.88*64.80","Capacitive Touch Display"]
["3.0”","KD030WQFMD036A-C020B","PDF","240x400","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*4.30","38.88*64.80","Capacitive Touch Display"]
["3.1”","KD031WVFPD002-C001A","PDF","480x800","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display"]
["3.1”","KD031WVFID001-C001A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","320 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display"]
["3.1”","KD031WVFPD002-C001A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*19.50","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVTMA011-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","370 nits","55.00*77.20*3.85","48.60*64.80","Capacitive Touch Display"]
["3.2”","KD032QVTMA015-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","350 nits","55.00*77.20*3.85","48.60*64.80","Capacitive Touch Display"]
["3.2”","KD032QVFMD028-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-C002A-RS485","PDF","240x320","RS485","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*15.10","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-C002A-TTL","PDF","240x320","TTL","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032VGFPD035-C008A","PDF","480x640","SPI+RGB","ST7701SN","Free V.A","CTP","-20℃~70℃","700 nits","66.85*85.51*4.25","49.25*65.66","Capacitive Touch Display"]
["3.2”","KD032VGFID034-C008A","PDF","480x640","MIPI","ST7701SN","Free V.A","CTP","-20℃~70℃","850 nits","66.85*85.51*4.25","49.25*65.66","Capacitive Touch Display,High-brightness TFT"]
["3.2”","KD032HDFLD038-C009A","PDF","1024x768","LVDS","JD9168","Free V.A","CTP","-20℃~70℃","500 nits","79.41*67.19*6.82","64.51*48.38","Capacitive Touch Display"]
["3.2”","KD032HDFID037-C009A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-20℃~70℃","550 nits","79.41*67.19*4.09","64.51*48.38","Capacitive Touch Display"]
["3.4”","KD034WXFID001-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-C001A-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*16.00","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFLD005-C001A","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","800 nits","65.72*69.64*6.34","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-C001A-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WVFID003-C008A","PDF","800x800","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","111.20*113.20*3.41","87.60*87.60","Capacitive Touch Display,Round TFT"]
["3.5”","KD035LQFPA093-C051A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.85","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPD093-02-C037B","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.51","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVTIA067-C022A","PDF","320x480","MIPI","ILI9488","V.A 6H","CTP","-20℃~70℃","350 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C009A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","270 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA027-C009A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","360 nits","55.50*84.96*4.05","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035LQFPA093-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-C021A","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*4.73","53.28*71.04","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035VGFIA111-C041A","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035VGFPA094-C035A","PDF","480x640","RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","540 nits","64.00*85.00*4.55","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035WVFPD122-C047A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","60.16*96.30*4.46","45.36*75.60","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C052A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA027-C053A","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C052A-RS232","PDF","320x480","RS232","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD094-01-C055A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","570 nits","69.96*92.96*4.93","53.28*71.04","Capacitive Touch Display,Blanview TFT"]
["3.5”","KD035VGFIA111A-01-C041A","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","1250 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFPA094-02-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","1300 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT,Blanview TFT"]
["3.5”","KD035HVFMD145-01-C005C","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","61.90*96.04*3.90","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035HVFMD137-C009A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","550 nits","55.30*84.76*3.31","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA138-C009A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","340 nits","55.50*84.96*3.75"," 48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA139-C030A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMA139-C031A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","61.90*96.04*4.27","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFIA141-C009A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","450 nits","55.50*84.96*3.75","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFIA141-C048A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","500 nits","61.90*96.04*4.43","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFMD143-C047A","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","510 nits","61.90*96.04*4.32","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFID144-C048A","PDF","320x432","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","480 nits","61.90*96.04*4.32","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035VGFPD158-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-20℃~70℃","660 nits","85.80*85.80*4.46","70.00*52.56","Capacitive Touch Display"]
["3.5”","KD035VGFID162-C061B","PDF","640x480","MIPI","ST7703","Free V.A","CTP","-20℃~70℃","670 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display"]
["3.5”","KD035QHFPD154-C062B","PDF","640x960","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035VGFIA111-C041A-SP007A-TypeC","PDF","480x640","Type C","TBD","Free V.A","CTP","-20℃~70℃","360 nits","64.00*85.00*17.00","53.28*71.04","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035VGFID162-C061B-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","CTP","-20℃~70℃","660 nits","85.80*85.80*16.00","70.08*52.56","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035WVFLD237-C047A","PDF","480x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","480 nits","60.16*96.30*6.76","45.36*75.60","Capacitive Touch Display"]
["3.5”","KD035QHFID161-C062B","PDF","640x960","MIPI","ST7703","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFID225-C086A","PDF","320x480","MIPI","AXS15231","Free V.A","CTP","-20℃~70℃","800 nits","61.90*96.04*3.24","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFPD249-C061B","PDF","640x480","RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035QVRMD223-C102A","PDF","240x320","SPI&MCU&RGB","ILI9341","V.A 6H","CTP","-20℃~70℃","120 nits","66.24*87.12*6.16","53.64*71.52","Capacitive Touch Display,Transflective TFT"]
["3.5”","KD035VGFPA094A-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-30℃~70℃","600 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display"]
["3.5”","KD035HVTMA026-C052A-TTL","PDF","320x480","TTL","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035HVTMA026-C052A-RS485","PDF","320x480","RS485","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS232","PDF","240x320","RS232","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS485","PDF","240x320","RS485","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-TTL","PDF","240x320","TTL","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS232","PDF","320x240","RS232","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS485","PDF","320x240","RS485","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-TTL","PDF","320x240","TTL","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-CAN","PDF","320x240","CAN","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS232","PDF","480x640","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS485","PDF","480x640","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-TTL","PDF","480x640","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-CAN","PDF","480x640","CAN","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD167-C061B-SP004A-HDMI","PDF","640x480","HDMI","NV3052CGRB","Free V.A","CTP","-10℃~60℃","500 nits","85.80*85.80*21.36","70.08*52.56","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["3.5”","KD035VGFLD285-C061B","PDF","640x480","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","85.80*85.80*6.88","70.08*52.56","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035HVFMA155A-C055A","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQTMD188-C037B","PDF","320x240","SPI&MCU&RGB","ST7796","V.A 12H","CTP","-20℃~70℃","430 nits","86.84*74.84*4.42","70.08*52.56","Capacitive Touch Display"]
["3.5”","KD035HVFMA155A-C005C","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","61.90*96.04*4.30","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFBA062-01-C009A","PDF","320x480","MCU","ILI9488","Free V.A","CTP","-20℃~70℃","340 nits","55.50*84.96*3.62","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035HVFIA141-C055A","PDF","320x480","MIPI","ILI9488","Free V.A","CTP","-20℃~70℃","500 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display"]
["3.5”","KD035LQFPA093-04-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","76.95*64.00*4.35","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035WVFID121A-C043A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","420 nits","60.16*96.30*4.46","45.36*75.60","Capacitive Touch Display"]
["3.8”","KD038HDFPD002-C001A","PDF","1024x600","RGB","JD9168","Free V.A","CTP","-20℃~70℃","810 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFLD001-C001A","PDF","1024x600","LVDS","JD9168","Free V.A","CTP","-20℃~70℃","800 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFPD002-C001A-RS232","PDF","1024x600","RS232","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-RS485","PDF","1024x600","RS485","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-TTL","PDF","1024x600","TTL","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.9”","KD039WQFPN002-C001A","PDF","480x128","RGB","ST7282","Free V.A","CTP","-30℃~85℃","1900 nits","112.46*44.40*5.61","95.04*25.34","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["3.9”","KD039FHOIN003-01-C0000","PDF","1080x1240","MIPI","SD5302","Free V.A","CTP","-20℃~70℃","500 nits","67.25*79.87*0.80","65.45*75.14","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040WVFID026-C008B","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.25","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFID026-C009B","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFMD022-C021A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","480 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WVFPD025-C008B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","440 nits","58.26*98.10*4.25","51.84*87.40","Capacitive Touch Display"]
["4.0”","KD040WVFPD025-C009B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","440 nits","66.84*111.50*4.38","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFID017-C015A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","950 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","850 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFID026-01-C025A","PDF","480x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.10","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040HDFID032-C026C","PDF","720x720","MIPI","ST7703","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*3.76","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*4.23","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040QHFID049-C039A","PDF","400x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["4.0”","KD040QHFPD047-C039A","PDF","400x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["4.0”","KD040WVFPA027-C022A","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*4.05","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFLD071-C015C","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","77.00*80.00*4.51","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WVFLD070-C008B","PDF","480x800","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","480 nits","57.86*97.70*6.21","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040HDFID032-C026C-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","CTP","-20℃~70℃","650 nits","84.00*85.99*15.50","71.93*71.93","Capacitive Touch Display,Square TFT,Type-C TFT"]
["4.0”","KD040WVFID026-01-C025A-SP005A-TypeC","PDF","480x800","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*16.00","51.84*86.40","Capacitive Touch Display,Type-C TFT"]
["4.0”","KD040WXFID017-C015C-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","77.00*80.00*16.00","71.86*70.18","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["4.0”","KD040HVFID080-C050A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081-C050A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A-RS232","PDF","720x720","RS232","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS485","PDF","720x720","RS485","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-TTL","PDF","720x720","TTL","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-CAN","PDF","720x720","CAN","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040QHFID049-C039A-SP004A-TypeC","PDF","400x960","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*15.00","39.18*94.03","Capacitive Touch Display,Type-C TFT"]
["4.0”","KD040WVTPD090-C008B","PDF","480x800","RGB","ST7701SI","V.A 6H","CTP","-10℃~60℃","150 nits","57.86*97.70*4.08","51.84*86.40","Capacitive Touch Display,Transflective TFT"]
["4.0”","KD040FHFLD058-C041A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","1000 nits","104.87*72.22*4.76","88.59*49.83","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["4.0”","KD040HDFID088-C054A","PDF","720x720","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","800 nits","125.29*127.29*3.41","101.52*101.52","Capacitive Touch Display,High-brightness TFT,Round TFT"]
["4.0”","KD040WVFPD027-02-C008B","PDF","480x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*3.85","51.84*86.40","Capacitive Touch Display"]
["4.0”","KD040WXFPD014-C046B","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","82.80*82.80*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040UXOIN109-C073A","PDF","1080x1200","MIPI","VTDR6130A","Free V.A","CTP","-20℃~70℃","600 nits","72.93*80.53*1.12","68.43*76.03","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040WXFPD014-a","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.1”","KD041HDOIN002-C000","PDF","2480x1860","MIPI","RM69A10","Free V.A","CTP","-20℃~70℃","280 nits","48.24*100.84*2.64","43.55*94.47","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043WVFID083-02-C048A","PDF","480x800","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","69.16*120.05*4.58","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WQFPA042-01-C037C","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-C038A","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","115.40*79.15*4.80","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQTPA097A-01-C009A","PDF","480x272","RGB","NV3047E","V.A 12H","CTP","-20℃~70℃","450 nits","105.40*67.15*4.41","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WQTPA097A-01-C017A","PDF","480x272","RGB","NV3047E","V.A 12H","CTP","-20℃~70℃","450 nits","115.40*79.15*4.79","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WVFBD082-C010A","PDF","480x800","MCU","ILI9806","Free V.A","CTP","-20℃~70℃","430 nits","62.66*105.95*3.68","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFIA083-01-C064A","PDF","480x800","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*4.20","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFPA084-01-C015B","PDF","480x800","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*4.20","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WVFLA096-03-C049A-ZJB-HDMI","PDF","800x480","HDMI","ST7262","Free V.A","CTP","-10℃~60℃","450 nits","105.40*79.15*21.96","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFPD051-01-C050A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*4.25","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPD049-C038B","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","740 nits","115.40*79.15*4.63","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFPA051-02-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C049A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","115.40*79.15*4.86","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQTPA097A-04-C017A-SP003A-HDMI","PDF","480x272","HDMI","TBD","V.A 12H","CTP","-20℃~70℃","500 nits","115.40*79.15*21.89","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFLA096-02A-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPD042-07-C017C-SP004A-HDMI","PDF","480x272","HDMI","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","115.40*79.15*20.40","95.04*53.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["4.3”","KD043WVFPA084-05-C015B-SP001A-HDMI","PDF","480x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","62.50*105.55*21.30","56.16*93.60","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS232","PDF","480x800","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS485","PDF","480x800","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-TTL","PDF","480x800","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS232","PDF","480x272","RS232","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS485","PDF","480x272","RS485","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-TTL","PDF","480x272","TTL","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS232","PDF","800x480","RS232","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS485","PDF","800x480","RS485","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-TTL","PDF","800x480","TTL","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-CAN","PDF","480x272","CAN","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFLA096-03-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043OLEDN001","PDF","568x1210","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","600 nits","49.13*103.55*0.75","47.37*100.91","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043WQFMD134-01-C037A","PDF","480x272","MCU","NV3041A-01","Free V.A","CTP","-30℃~85℃","900 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-C037D","PDF","480x272","RGB","ST7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLD117-C048A","PDF","480x800","LVDS","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","69.16*120.05*4.58","56.16*93.60","Capacitive Touch Display"]
["4.3”","KD043WQTPA115-01-C090A","PDF","480x272","RGB","ST7282","V.A 12H","CTP","-20℃~70℃","440 nits","105.50*67.20*5.40","95.04*53.86","Capacitive Touch Display"]
["4.3”","KD043WQFPA142-01-C037D","PDF","480x272","RGB","ST7282A","Free V.A","CTP","-30℃~80℃","650 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.5”","KD045FWFPA010-01-C001B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWTPA001-02-C001B-SP001A-HDMI","PDF","480x854","HDMI","ILI9806E","V.A 12H","CTP","-20℃~70℃","350 nits","61.54*110.09*19.00","55.44*98.64","Capacitive Touch Display,HDMI TFT"]
["4.5”","KD045FWFLA012-01-C001B","PDF","480x854","LVDS","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFIA011-01-C001B","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","61.54*110.09*4.15","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFPA010-01-C001B-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFID015-C005A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","72.00*121.00*3.85","55.44*98.64","Capacitive Touch Display"]
["4.5”","KD045FWFID016-C005A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","72.00*121.00*3.85","55.44*98.64","Capacitive Touch Display"]
["5.0”","KD050FWFID042-C010B","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPD041-C010B","PDF","480x854","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA029-02-C045A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","120.70*75.90*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFIA019-C019A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-C009A","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*4.03","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050HDFID040-C020B","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","440 nits","78.56*135.65*4.13","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050SXFID039-C045A","PDF","1080x1080","MIPI","HX8399","Free V.A","CTP","-20℃~60℃","270 nits","208.00*208.00*4.16","127.01*127.01","Capacitive Touch Display,Round TFT"]
["5.0”","KD050HDFIA020-06-C020E-SP003A-TYPE C","PDF","720x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*15.35","62.10*110.40","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050HDFIA020-06-C020E","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*4.03","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050HDFPA054-C020A","PDF","720x1280","RGB","NV3052CGRB","Free V.A","CTP","-20℃~70℃","350 nits","78.56*135.65*4.20","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050HDFIA020-06-C020D","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","78.56*135.65*4.20","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-C005A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","310 nits","120.70*75.80*4.48","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-C005A-SP001A-HDMI","PDF","800x480","HDMI","ILI5960/ILI6122","V.A 12H","CTP","-10℃~60℃","310 nits","120.70*75.80*19.81","108.00*64.80","Capacitive Touch Display,HDMI TFT"]
["5.0”","KD050HDFLD091-C020C","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","400 nits","67.56*122.35*4.05","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-02-C009E-SP004A-TYPE C","PDF","480x854","Type C","ILI9806E","Free V.A","CTP","-20℃~70℃","540 nits","67.56*122.35*15.25","61.63*109.65","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050FWFLD099-C010B","PDF","480x854","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","78.56*135.65*4.38","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-CTP-002","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-C010B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.00","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA107-C104A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","900 nits","118.50*77.80*6.34","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109-C107A","PDF","480x272","RGB","ST7282","Free V.A","CTP","-30℃~85℃","900 nits","120.16*75.36*4.56","110.88*62.83","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050HDOIN116-C000","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FWFPA011-09-C009E-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS232","PDF","720x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS485","PDF","720x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-TTL","PDF","720x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS232","PDF","800x480","RS232","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS485","PDF","800x480","RS485","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-TTL","PDF","800x480","TTL","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDOIN116-C116B","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","70.52*123.12*1.67","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050WVRPD092-03-C045A","PDF","800x480","RGB","HX8264+HX8664","V.A 12H","CTP","-20℃~70℃","150 nits","132.72*87.80*4.99","108.00*64.80","Capacitive Touch Display,Transflective TFT"]
["5.0”","KD050HDOIN116-C000-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","64.12*116.72*10.80","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C116B-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","70.52*123.12*12.37","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050FWFIA019-01-C019A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","360 nits","67.26*122.00*3.98","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-02-C002A","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFIA019-02-C009F","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA029-06-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","120.70*75.90*4.48","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVTPA045-C003A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","310 nits","132.72*87.80*5.00","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-02A-C003A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","650 nits","132.72*87.80*4.88","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050WVTPA045-02A-C005A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","650 nits","120.70*75.90*4.60","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050FHFLD102-01-C085B","PDF","1920x1080","LVDS","SC5010B","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["5.0”","KD050HDFID040-02-C020B","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","430 nits","78.56*135.65*4.33","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050WVFLA033-01-C045A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","750 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFLA037-01-C045A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-20℃~70℃","600 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display"]
["5.0”","KD050HDOIN132-C001","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FWFIA019-02-C009E","PDF","480x854","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","490 nits","67.56*122.35*4.05","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050WVFPA018-C020A","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","CTP","-30℃~85℃","630 nits","124.90*78.10*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFPA041-03-C002A","PDF","480x854","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","520 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FHFLD079-C085A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050FWFPA011-09-C002A","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","450 nits","78.56*135.65*4.40","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-C009B","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","67.56*122.35*3.88","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050HDFID040-C020C","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*4.05","62.10*110.40","Capacitive Touch Display"]
["5.0”","KD050FWFPA011-09-C009E","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*4.03","61.63*109.65","Capacitive Touch Display"]
["5.0”","KD050HDOIN116-C000-a","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FHFID103-01-C085B","PDF","1920x1080","MIPI","SC5010E","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050WVFLA146-02-C039A","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","950 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-02-C045A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","850 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C039A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C040C","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","120.70*75.90*4.38","108.50*65.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFID042-C009B","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","67.56*122.35*4.38","61.63*109.65","Capacitive Touch Display"]
["5.5”","KD055HDFIA001-C001A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","360 nits","86.04*144.96*4.75","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055FHFID018B-01-C017C","PDF","1080x1920","MIPI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*2.64","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055HDFLD023-C026A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","650 nits","79.04*137.67*4.39","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055HDFIA001-C001A-SP002A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","500 nits","86.04*144.96*21.85","68.04*120.96","Capacitive Touch Display,HDMI TFT"]
["5.5”","KD055FHFID018-01-C017A-SP003A-HDMI","PDF","1080x1920","HDMI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*19.74","68.04*120.96","Capacitive Touch Display,HDMI TFT,LTPS Display"]
["5.5”","KD055FHFID010-C017A","PDF","1080x1920","MIPI","XM91080","Free V.A","CTP","-20℃~70℃","340 nits","79.04*137.67*2.84","68.04*120.96","Capacitive Touch Display"]
["5.5”","KD055FHFID018-C017A","PDF","1080x1920","MIPI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*2.60","68.04*120.96","Capacitive Touch Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001","PDF","1080x1920","MIPI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*0.82","67.82*120.58","Capacitive Touch Display,AMOLED Display"]
["5.5”","KD055FHOIN031-C0000","PDF","1080x1920","MIPI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.82","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001-SP005A-HDMI","PDF","1080x1920","HDMI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*10.80","67.82*120.58","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN031-C0000-HDMI","PDF","1080x1920","HDMI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.83","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055HDFID028-C001A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","430 nits","86.04*144.96*4.75","67.93*120.77","Capacitive Touch Display"]
["5.6”","KD056VGTPA003-C002A","PDF","640x480","RGB","TBD","V.A 12H","CTP","-20℃~70℃","380 nits","126.50*100.00*6.08","112.90*84.67","Capacitive Touch Display"]
["5.6”","KD056VGTPA004-C004A","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","CTP","-20℃~70℃","750 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display"]
["5.6”","KD056VGTPA004-C004A-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","CTP","-20℃~70℃","750 nits","126.50*100.00*23.60","115.50*86.40","Capacitive Touch Display,HDMI TFT"]
["5.7”","KD057VGFPA011-C004A","PDF","640x480","RGB","JD9186S","Free V.A","CTP","-30℃~80℃","550 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA015A-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFLA012A-C004A","PDF","640x480","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFIA014A-C004A","PDF","640x480","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA018-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","650 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.8”","KD058UXFLA003-C001A","PDF","1920x1080","LVDS","ST5892B","Free V.A","CTP","-20℃~70℃","950 nits","144.56*87.40*7.65","126.72*71.28","Capacitive Touch Display,High-brightness TFT"]
["5.8”","KD058UXFLA003-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","CTP","-20℃~70℃","900 nits","144.56*87.40*21.26","126.72*71.28","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["5.9”","KD059WVFPD001-C001A","PDF","840x512","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.16*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003-C001A","PDF","840x512","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-C001A","PDF","840x512","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.0”","KD060HDFID001-C001A","PDF","720x1440","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","480 nits","95.04*167.63*4.33","68.04*136.08","Capacitive Touch Display"]
["6.0”","KD060HDFID001-C001A-SP001A-HDMI","PDF","720x1440","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","95.04*167.63*19.23","68.04*136.08","Capacitive Touch Display,HDMI TFT"]
["6.0”","KD060HDFID001-C001A-SP002A-TYPEC","PDF","720x1440","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","480 nits","95.04*167.63*15.55","68.04*136.08","Capacitive Touch Display,Type-C TFT"]
["6.0”","KD060HDFLD007-C005A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.0”","KD060HDFID006-C005A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.0”","KD060FPOIN011-C0000","PDF","1080x2160","MIPI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.0”","KD060FPOIN011-C0000-HDMI","PDF","1080x2160","HDMI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.0”","KD060HDFID006-C005A-SP001A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","80.58*146.12*18.21","73.98*131.52","Capacitive Touch Display,HDMI TFT"]
["6.0”","KD060HDFLD007A-C005A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","360 nits","80.58*146.12*3.31","73.98*131.52","Capacitive Touch Display"]
["6.2”","KD062VGFPD003-C002A","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","800 nits","173.80*82.76*4.76","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-C002A-TTL","PDF","640x240","TTL","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS485","PDF","640x240","RS485","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS232","PDF","640x240","RS232","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062HDFLD005-01-C007A","PDF","1024x600","LVDS","JD9168S","Free V.A","CTP","-20℃~70℃","1350 nits","155.40*88.40*6.68","137.47*77.23","Capacitive Touch Display,High-brightness TFT"]
["6.4”","KD064FPOIN001-C0000","PDF","1080x2340","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.4”","KD064FPOIN001-C0000-HDMI","PDF","1080x2340","HDMI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.6”","KD066FHFID010-C011A","PDF","1080x2400","MIPI","FT8725","Free V.A","CTP","-25℃~70℃","550 nits","74.88*167.48*2.19","68.43*152.57","Capacitive Touch Display"]
["6.67”","KD067FPOIN004-C0000","PDF","1080x2400","MIPI","VTDR6130","Free V.A","CTP","-20℃~70℃","500 nits","71.53*200.59*0.33","69.55*154.56","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.7”","KD067WSFLA001-C001A","PDF","1920x1080","LVDS+eDP","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1300 nits","161.12*97.68*7.12","148.32*84.43","Capacitive Touch Display,High-brightness TFT"]
["6.7”","KD067WSFLA001-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1500 nits","161.12*97.68*23.02","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.7”","KD067FHFID002-C003A","PDF","1080x2400","MIPI","ICNL9922CAC-01","Free V.A","CTP","-20℃~70℃","400 nits","74.31*164.56*2.13","70.08*155.74","Capacitive Touch Display"]
["6.7”","KD067WSFLA001-C001A-SP002A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1000 nits","161.12*97.68*23.10","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068HDFID005-C001A","PDF","480x1280","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","2250 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFLD004-C001A","PDF","480x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1450 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068WVFPD007-01-C003A","PDF","800x480","RGB","TBD","Free V.A","CTP","-30℃~85℃","800 nits","155.96*100.77*7.29","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","CTP","-20℃~70℃","800 nits","155.96*100.77*23.19","148.10*88.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS232","PDF","800x480","RS232","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS485","PDF","800x480","RS485","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-TTL","PDF","800x480","TTL","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-CAN","PDF","800x480","CAN","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["7.0”","KD070WVTPA077-C004A","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","1100 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLA011-C010A","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","350 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDTLA020-C030A","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","CTP","-20℃~70℃","550 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDTLA020-C031A","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","CTP","-20℃~70℃","550 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA019-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA019-C002A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA013-01-C018A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","450 nits","182.07*117.60*7.55","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-C004A","PDF","800x480","LVDS","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","380 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-C007A-LVDS","PDF","800x480","LVDS","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","400 nits","182.07*117.60*13.75","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070WVTPA006-C005A","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","400 nits","165.0*100.00*8.18","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070WVFPA065-C010A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","550 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA043-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-C049A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA028-C014A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","600 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA028-C015A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","600 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFIA030-04-C026B","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","850 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFIA030-04-C027B","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","850 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-C027A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD","Free V.A","CTP","-20℃~70℃","520 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLD070-C085A","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","CTP","-30℃~85℃","980 nits","182.45*121.47*9.38","152.45*91.47","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WXFID050-C065A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","103.56*162.38*4.73","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070HDFID067-C080A","PDF","720x1440","MIPI","GC9702P","Free V.A","CTP","-20℃~70℃","350 nits","101.73*186.34*3.53","78.02*156.04","Capacitive Touch Display"]
["7.0”","KD070WVTPA088-01-C004A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-C101A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","182.07*117.60*8.15","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA035A-C049C-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","V.A 12H","CTP","-10℃~60℃","1000 nits","165.40*104.59*24.83","152.40*91.44","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["7.0”","KD070WXFID050-C038A-SP001A-TYPEC","PDF","800x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","119.46*176.78*15.80","94.20*150.72","Capacitive Touch Display,Type-C TFT"]
["7.0”","KD070HDFID086-C102A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID093A-C107A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1200 nits","119.46*176.78*7.27","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVTLA095-01-C004A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-C101A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","450 nits","182.07*117.60*10.55","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLD092-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.62","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA044-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1600 nits","165.10*100.10*6.81","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID094-C074A","PDF","280x1424","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","600 nits","50.20*193.47*5.20","33.60*170.88","Capacitive Touch Display,Bartype TFT"]
["7.0”","KD070HDFLD089-C102A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD092-C113A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.67","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WUFID085-C021A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-20℃~70℃","410 nits","119.46*176.78*19.30","94.50*151.20","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFLD092-C050B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","182.07*117.60*7.22","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA010-02-C010A","PDF","800x480","RGB","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","720 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLA116-CTP-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","550 nits","169.20*104.00*38.26","154.21*85.92","Capacitive Touch Display,Display Monitor"]
["7.0”","KD070FHFID078-01-C021A","PDF","1200x1920","MIPI","HX8279","Free V.A","CTP","-20℃~80℃","400 nits","119.46*176.78*3.98","94.50*151.20","Capacitive Touch Display"]
["7.0”","KD070C-4-05-C004A-RS232","PDF","800x480","RS232","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070HDFIA030-C026A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD","Free V.A","CTP","-20℃~70℃","520 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070WVFPA043A-C049A-RS232","PDF","800x480","RS232","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-RS485","PDF","800x480","RS485","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-TTL","PDF","800x480","TTL","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-RS485","PDF","800x480","RS485","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070C-4-05-C004A-TTL","PDF","800x480","TTL","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070HDFLA028-02-C027B-SP001A-HDMI","PDF","1024x600","HDMI","EK73215&EK79001","Free V.A","CTP","-10℃~60℃","550 nits","165.00*100.00*22.27","154.21*85.92","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFIA030-02-C028A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-02-C029A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLD106-C114A","PDF","800x480","LVDS","ST7277-G6-K","Free V.A","CTP","-20℃~70℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFPA126-C125A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","450 nits","164.90*100.00*4.40","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070WUFID123-C123A","PDF","1200x1920","MIPI","FT7250","Free V.A","CTP","-20℃~70℃","950 nits","109.80*173.00*5.00","94.50*151.20","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFPA127-C128A","PDF","1024x600","RGB","JD9165","Free V.A","CTP","-10℃~60℃","450 nits","164.86*99.96*5.28","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFPA051-01-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","700 nits","182.07*117.60*8.05","154.21*85.92","Capacitive Touch Display"]
["7.0”","KD070FHOIN128-C0000","PDF","1080x1920","MIPI","ICNA3512","Free V.A","CTP","-20℃~70℃","950 nits","89.13*160.91*1.01","87.13*154.91","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["7.0”","KD070HDFPA038-C024A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-SP002A-HDMI","PDF","800x480","HDMI","EK9713/EK73002","V.A 12H","CTP","-10℃~60℃","400 nits","165.00*100.00*24.43","154.08*85.92","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFLA028-06-C014C","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLA028-06-C014A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFPA043A-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A-C049C","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WXFID050-C038A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-10℃~60℃","400 nits","119.46*176.78*4.75","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070WXFID050-02-C038A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","780 nits","119.46*176.78*4.75","94.20*150.72","Capacitive Touch Display"]
["7.0”","KD070C-4-05-CTP-002","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","182.07*117.60*8.13","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070C-4-05-C004A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display"]
["7.0”","KD070HDFLA028-06-C015B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["7.0”","KD070WVFPD140-01-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","1050 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["7.0”","KD070WXFID138-C038B","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","119.46*176.78*6.46","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.84”","KD078HDFID004-C004A","PDF","400x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","950 nits","67.60*206.28*6.27","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002-C003A-RS232","PDF","400x1280","RS232","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS485","PDF","400x1280","RS485","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-TTL","PDF","400x1280","TTL","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFID004-C004A-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","CTP","-20℃~70℃","800 nits","67.60*206.28*21.12","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["8.0”","KD080WXFLD023-C015A-SP002A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","400 nits","130.70*200.10*22.15","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080WXFID015-C015A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*5.04","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080FM-8-C008A","PDF","1600x480","LVDS","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","420 nits","249.20*87.00*6.86","194.40*58.32","Capacitive Touch Display,Bartype TFT"]
["8.0”","KD080WXFID012-C008A","PDF","800x1280","MIPI","TBD","Free V.A","CTP","-20℃~60℃","200 nits","130.70*200.10*4.65","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080C-4-CTP-001","PDF","800x600","RGB","EK9713/EK7330","V.A 6H","CTP","-20℃~70℃","250 nits","199.00*157.00*7.93","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WXFID015-C015A-SP004A-TYPEC","PDF","800x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*16.15","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080FHFID017-C016A-SP001A-TYPEC","PDF","1200x1920","Type C","NT51021","Free V.A","CTP","-10℃~50℃","250 nits","124.60*190.80*15.01","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080WXFID015-C015A-SP003A-HDMI","PDF","800x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~60℃","500 nits","130.70*200.10*22.09","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080C-5-01-C006B-CP001A-HDMI","PDF","1024x768","HDMI","TBD","V.A 12H","CTP","-10℃~60℃","300 nits","174.00*136.00*13.92","162.05*121.54","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080WXFID015-C015A-RS232","PDF","800x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-RS485","PDF","800x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-TTL","PDF","800x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-02-C015A","PDF","800x1280","MIPI","ILI9881","Free V.A","CTP","-20℃~60℃","800 nits","130.70*200.10*4.90","107.64*172.22","Capacitive Touch Display,High-brightness TFT"]
["8.0”","KD080WVFLA034-C030A","PDF","800x600","LVDS","JD9165BA","Free V.A","CTP","-20℃~70℃","730 nits","199.00*157.00*7.87","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WVFPA032-C029A","PDF","800x600","RGB","JD9165BA","Free V.A","CTP","-20℃~70℃","730 nits","199.00*157.00*7.87","162.00*121.50","Capacitive Touch Display"]
["8.0”","KD080WXFID015-C008A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*4.84","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080WXFLD023-C015A","PDF","800x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*5.05","107.64*172.22","Capacitive Touch Display"]
["8.0”","KD080C-5-01-C006B","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-10℃~60℃","310 nits","174.00*136.00*4.83","162.05*121.54","Capacitive Touch Display"]
["8.0”","KD080WUFLD040-C034A","PDF","1920x1200","LVDS","FL5893DA","Free V.A","CTP","-20℃~70℃","1750 nits","181.80*119.85*7.40","172.22*107.64","Capacitive Touch Display,High-brightness TFT"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["8.6”","KD086UXFLD001-C001A","PDF","600x1600","LVDS","GC9704","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.6”","KD086UXFID002-C001A","PDF","600x1600","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.9”","KD089FHFID004-C001A","PDF","480x1920","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","850 nits","76.00*243.10*6.75","54.72*218.88","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["9.0”","KD090HDFLA006-C001A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008-C001A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.7”","KD097HDFLD001-C001A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","0℃~50℃","240 nits","228.10*187.90*8.12","196.60*147.46","Capacitive Touch Display"]
["10.1”","KD101HDFLA010-C016A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","252.70*175.55*9.25","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101UXFID008-C014A","PDF","1200x1920","MIPI","NT51021","Free V.A","CTP","-10℃~50℃","300 nits","159.00*244.60*4.33","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID018-C012A","PDF","800x1280","MIPI","JD9365AA","Free V.A","CTP","-20℃~60℃","300 nits","159.00*244.60*4.96","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID018-C012B","PDF","800x1280","MIPI","JD9365AA","Free V.A","CTP","-20℃~60℃","300 nits","159.00*244.60*4.96","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101UXFLD024-C035A","PDF","1920x1200","LVDS","HX8290-B","Free V.A","CTP","-20℃~70℃","500 nits","246.31*168.75*4.87","216.81*135.50","Capacitive Touch Display"]
["10.1”","KD101WXFID027-C012A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*4.86","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WXFID027-C012B","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*4.86","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101WSFLD028-C040A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101FHFID031-C037A","PDF","440x1920","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*6.23","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["10.1”","KD101WSFID033-C040A","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFPD036-C040A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101FHFID030-01-C014A","PDF","1200x1920","MIPI","HX8279D","Free V.A","CTP","-10℃~50℃","350 nits","159.00*244.60*4.81","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101FHFID030-C036A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","280 nits","174.37*255.12*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101FHFID030-C014A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101WXFID027-C012B-SP001A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*19.76","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101FHFID030-C014A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*19.40","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WXFLD021-01-C009B","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~85℃","590 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101WXFLD021-C009B","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101WXFID045-C009B","PDF","1280x800","MIPI","EK79202D","Free V.A","CTP","-30℃~85℃","500 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101WXFLD047-01-C001B","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","750 nits","229.06*148.70*4.71","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101WSFID033-C040A-SP001A-HDMI","PDF","1024x600","HDMI","EK73217& EK79007","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.76","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101HDFLD020-01-C045C-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","900 nits","232.70*155.56*24.50","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFLD051-01-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","700 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101HDFLD053-C064A-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","293.00*194.00*62.00","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD051-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","350 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFLD028-C040A-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","0℃~50℃","320 nits","258.10*166.10*43.23","222.72*125.28","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFPD036-C040A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFLD028A-C040A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFID033A-C040A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101WSFPD036A-C040A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","480 nits","254.50*162.50*4.87","222.72*125.28","Capacitive Touch Display"]
["10.1”","KD101HDFLA060-CTP-Monitor","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","500 nits","259.96*177.96*29.40","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD021-02-C045C-SP007A-HDMI","PDF","1280x800","HDMI","EK79202D_A","Free V.A","CTP","-20℃~70℃","700 nits","229.06*148.70*22.84","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WSFLA058-C065A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101WSFPA055-C065A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLD056A-C045E","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~80℃","1250 nits","252.96*171.60*6.91","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WSFIA057-C065A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLA020-C016A","PDF","1280x800","LVDS","EK79202B1","Free V.A","CTP","-20℃~70℃","1100 nits","252.70*175.55*10.31","216.96*135.60","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101WXFLD021-C045C-RS232","PDF","1280x800","RS232","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-RS485","PDF","1280x800","RS485","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-TTL","PDF","1280x800","TTL","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101FHFID031-C037A-CP001A-HDMI","PDF","440x1920","HDMI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*12.29","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["10.1”","KD101WSFLA058-C065A-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","254.50*162.50*23.15","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WXFLD021A-C072A-Monitor","PDF","1280x800","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","258.25*176.05*26.68","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101UXFLD024A-C035A","PDF","1920x1200","LVDS","ST5892B","Free V.A","CTP","-20℃~70℃","500 nits","246.31*168.75*4.87","216.81*135.50","Capacitive Touch Display"]
["10.1”","KD101FM-1-10-C032C-SP005A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","254.50*162.50*21.24","216.96*135.60","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WXFLD021-C045C","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*4.79","216.96*135.60","Capacitive Touch Display"]
["10.1”","KD101FHFID063-C070A","PDF","1200x1920","MIPI","OTA7290B","Free V.A","CTP","-10℃~50℃","450 nits","159.00*244.60*4.25","135.36*216.58","Capacitive Touch Display"]
["10.1”","KD101UXFLD024D-01-C035A-SP002A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1100 nits","246.31*168.75*23.98","216.81*135.50","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.4”","KD104C-1-C002A","PDF","800x600","RGB","TBD","V.A 6H","CTP","-10℃~50℃","200 nits","228.40*175.40*8.28","211.20*158.40","Capacitive Touch Display"]
["10.4”","KD104C-1-CTP-001","PDF","800x600","RGB","TBD","V.A 6H","CTP","-10℃~50℃","250 nits","248.40*195.40*8.23","211.20*158.40","Capacitive Touch Display"]
["10.4”","KD104WVTLA009-CTP-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","750 nits","261.60*208.80*43.00","213.20*160.40","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104HDFLA0018-C009A-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","350 nits","283.00*225.20*64.00","211.20*158.48","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104XGFLA011-C009A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1300 nits","266.13*221.29*12.54","210.43*157.82","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID025-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027-C011A","PDF","1024x768","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["11.6”","KD116FHFEA001-C001A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","800 nits","291.52*179.38*8.59","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["11.6”","KD116WSFEA003-CTP-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","1000 nits","298.22*186.10*44.00","257.32*145.18","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["11.6”","KD116WSFEA002-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","291.52*179.38*24.28","256.32*144.18","Capacitive Touch Display,HDMI TFT"]
["11.6”","KD116WSFEA002-C002A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","256.92*144.78","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFPA001-C001B","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~85℃","600 nits","281.80*220.70*11.20","245.76*184.32","Capacitive Touch Display,Wide Temp TFT"]
["12.1”","KD121HDFLA015-CTP-Monitor","PDF","1024x768","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","850 nits","294.50*233.00*44.00","247.00*185.50","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["12.1”","KD121HDFLA013-C007A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-20℃~70℃","700 nits","290.00*228.50*10.90","245.76*184.32","Capacitive Touch Display"]
["12.1”","KD121HDFLA013-C007A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","750 nits","290.00*228.50*31.94","245.76*184.32","Capacitive Touch Display,HDMI TFT"]
["12.1”","KD121HDFLD010-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1100 nits","306.50*196.20*14.50","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLD009-01-C006A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1350 nits","306.50*196.20*15.42","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFPA001-C001C","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-10℃~60℃","600 nits","281.80*220.70*11.00","245.76*184.32","Capacitive Touch Display"]
["12.1”","KD121HDFLA026-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","294.10*196.20*8.10","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121UXFLA037-C014B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","305.00*200.00*8.65","262.83*164.27","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFLA035-C012B","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1200 nits","294.10*196.20*9.33","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.3”","KD123WUFLD006-C002A","PDF","1920x720","LVDS","TBD","Free V.A","CTP","-30℃~85℃","950 nits","311.02*132.60*9.15","292.03*109.51","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.8”","KD128FHFLD001-01-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-30℃~85℃","550 nits","320.59*196.61*29.45","283.39*159.41","Capacitive Touch Display,Wide Temp TFT,HDMI TFT"]
["13.3”","KD133FHFED012-C008A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","750 nits","325.20*199.80*4.90","293.76*165.24","Capacitive Touch Display"]
["13.3”","KD133FHFLA013-C009A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","800 nits","325.20*199.80*9.65","293.47*165.08","Capacitive Touch Display,High-brightness TFT"]
["13.3”","KD133FHFLA013-C009A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-20℃~70℃","900 nits","325.20*199.80*22.55","293.47*165.08","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["13.3”","KD133FHFLA015-C010A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","332.40*206.40*56.80","293.76*165.24","Capacitive Touch Display,Display Monitor"]
["13.3”","KD133FHFED023-C011A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","280 nits","325.20*199.80*6.00","293.76*165.24","Capacitive Touch Display"]
["14.0”","KD140FHFLD003-C003A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","700 nits","337.49*206.76*7.58","308.16*173.34","Capacitive Touch Display,LTPS Display"]
["14.0”","KD140FHFEA010-C003B","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","450 nits","337.49*206.76*7.95","308.16*173.34","Capacitive Touch Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["14.5”","KD145OLEDN003-C003A","PDF","3000x1876","MIPI","HX5318","Free V.A","CTP","-20℃~70℃","400 nits","316.56*201.06*1.62","312.30*192.29","Capacitive Touch Display,AMOLED Display"]
["15.0”","KD150XGFLD002-C001A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","385.50*312.50*30.92","304.10*228.10","Capacitive Touch Display,HDMI TFT"]
["15.0”","KD150HDFLA007-C006B","PDF","1280x242","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","423.30*118.10*14.20","374.78*71.10","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["15.6”","KD156FM-1-01-C003A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","220 nits","425.76*275.19*6.90","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156FHFLA007-C004A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","280 nits","373.58*228.33*11.05","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156WSFEA016-01-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","300 nits","398.00*248.00*46.50","343.54*192.83","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFED015-C010A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","0℃~50℃","400 nits","385.70*235.70*5.20","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156FHFLA021-C011A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","376.40*236.40*43.20","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFED024-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","300 nits","388.55*240.98*41.00","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFLA022-C008A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~80℃","750 nits","392.00*242.00*15.55","344.16*193.59","Capacitive Touch Display"]
["15.6”","KD156UHOEN018-C014A","PDF","3840x2160","eDP","RM98110","Free V.A","CTP","-20℃~70℃","320 nits","357.22*208.27*3.35","344.22*193.62","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["19.0”","KD190SGFLA005-C002A","PDF","1280x1024","LVDS","TBD","Free V.A","CTP","-20℃~70℃","750 nits","423.00*347.70*19.00","376.32*301.06","Capacitive Touch Display"]
["19.0”","KD190SXFLA007-01-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","710 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["19.0”","KD190SXFLA007-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","270 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215WSFVA011-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","400 nits","510.00*306.60*56.20","475.64*268.11","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLA023-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLD007-C005A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","505.60*302.20*13.97","476.06*267.79","Capacitive Touch Display,High-brightness TFT"]
["21.5”","KD215FHFLA023-C007A-Monitor-TR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLA026-C005B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~80℃","400 nits","505.60*302.20*13.90","476.64*268.11","Capacitive Touch Display,Wide Temp TFT"]
["23.6”","KD236WSFLD002-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","180 nits","559.00*335.00*56.20","521.47*293.10","Capacitive Touch Display,Display Monitor"]
["23.8”","KD238FHFVA010-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","583.17*356.46*70.95","524.37*298.46","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["23.8”","KD238FHFVA012-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~45℃","300 nits","598.00*370.00*58.00","529.00*297.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270WSFLA004-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","180 nits","644.40*382.60*59.40","597.60*336.15","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270WSFLA005-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","300 nits","645.40*383.20*62.50","598.00*336.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270FHFVA014-C004A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","402.11*660.90*82.60","336.31*593.43","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["27.0”","KD270UDOEN003-C002B","PDF","3840x2160","eDP","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*4.19","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*13.60","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270FHFVA021-C010A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","678.00*420.00*58.00","598.00*343.00","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA017-C006A-Monitor","PDF","3840x2160","HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA016-C005A-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["31.5”","KD315WSFVA002-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","748.60*451.20*51.00","698.60*392.10","Capacitive Touch Display,Display Monitor"]
["31.5”","KD315FHFLA001-C001A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","900 nits","746.70*441.30*19.80","698.40*392.85","Capacitive Touch Display,High-brightness TFT"]
["32.0”","KD320FHFUA003-C003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","400 nits","745.50*440.50*66.50","698.00*393.00","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320FHFVA006-C005A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","464.82*764.72*97.06","394.82*694.61","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA008-C006A-C1600-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","462.00*762.51*100.03","394.80*693.89","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA009-C008A-Monitor-BR","PDF","1920x1080","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","463.90*769.40*54.90","394.80*700.40","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320UHFVA007-C007A-Monitor","PDF","3840x2160","HDMI/DP/USB","TBD","Free V.A","CTP","0℃~40℃","300 nits","789.00*485.00*58.20","697.30*392.20","Capacitive Touch Display,Display Monitor"]
["43.0”","KD430UHFVA009-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.01*992.60*133.87","530.15*925.79","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA010-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.25*1005.29*164.61","530.75*927.01","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA011-C003A-C1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1003.64*606.45*136.13","925.90*529.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA012-C004A-J1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1016.87*606.45*136.03","933.40*530.75","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430FHFVA014-C006A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","1007.70*595.40*53.60","943.10*529.80","Capacitive Touch Display,Display Monitor"]
["43.0”","KD430UHFVA013-C005A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1028.43*619.42*63.40","941.18*529.42","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA006-C001A-C1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1134.82*122.65","605.03*1053.83","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA007-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1142.15*150.91","605.03*1064.95","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA008-C003A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1168.03*702.00*76.70","1085.50*604.00","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550WSFVA005-C002A-J1500-Monitor","PDF","3840x2160","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","772.40*1291.82*207.07","698.20*1227.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA006-C003A-C1800-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","756.80*1270.02*167.40","681.40*1174.66","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA007-C004A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1302.12*780.40*78.70","1209.60*680.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA011-C005A-S1200-Monitor","PDF","3840x2160","HDMI/DP/RS232","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","1293.10*833.40*48.30","1227.40*698.20","Capacitive Touch Display,Curved Monitor,Display Monitor"]

{"sheet":"Resistive Touch Display","index":2,"n_rows":115,"n_cols":13,"rows_kept":115}
["STARTEK Resistive Touch Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.44”","KD014QQTBN002-TP","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","RTP","-20℃~70℃","640 nits","32.36*38.00*4.20","25.50*26.50","Resistive Touch Display,Square TFT"]
["1.77”","KD018C-2-TP","PDF","128x160","SPI&MCU&RGB","ILI9163V","V.A 12H","RTP","-20℃~70℃","280 nits","34.00*47.00*3.60","28.03*35.04","Resistive Touch Display"]
["1.77”","KD018QQTBN009-RT","PDF","128x160","SPI&MCU","ST7735S","V.A 12H","RTP","-20℃~70℃","330 nits","34.70*46.70*3.55","28.03*35.04","Resistive Touch Display"]
["1.77”","KD018QVFMN010-02-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","300 nits","34.70*46.70*3.55","26.64*35.52","Resistive Touch Display"]
["2.0”","KD020QVTMA008-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","400 nits","35.80*52.10*3.75","30.60*40.80","Resistive Touch Display"]
["2.0”","KD020LQFMA014-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","RTP","-20℃~70℃","540 nits","46.50*41.56*3.70","40.80*30.60","Resistive Touch Display"]
["2.0”","KD020QVFMA009-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","400 nits","35.80*52.10*3.77","30.60*40.80","Resistive Touch Display"]
["2.0”","KD020QCTBN019-TP","PDF","176x220","MCU","ST7775R","V.A 12H","RTP","-20℃~70℃","480 nits","38.40*51.40*3.56","31.68*39.60","Resistive Touch Display"]
["2.0”","KD020QCTBN020-TP","PDF","176x220","SPI&MCU&RGB","ST7775R","V.A 12H","RTP","-20℃~70℃","380 nits","38.40*51.40*3.56","31.68*39.60","Resistive Touch Display"]
["2.0”","KD020LQRMA017-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","RTP","-20℃~70℃","280 nits","46.50*41.56*3.90","40.80*30.60","Resistive Touch Display,Transflective TFT"]
["2.0”","KD020WQFPA023-RT","PDF","480x360","SPI+RGB","ST7701S","Free V.A","RTP","-30℃~85℃","900 nits","46.50*41.56*3.70","40.82*30.62","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD019QQFBN002-RT","PDF","128x160","SPI&MCU","ST7735","Free V.A","RTP","-20℃~70℃","800 nits","37.47*49.04*3.22","31.87*39.84","Resistive Touch Display,High-brightness TFT"]
["2.0”","KD020QVRMA028-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","200 nits","35.80*52.10*3.85","30.60*40.80","Resistive Touch Display,Transflective TFT"]
["2.2”","KD022QVTBD032-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","220 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVTPD005-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","220 nits","41.70*56.16*3.80","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTPD006-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","170 nits","41.70*56.16*3.80","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTBD031-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","400 nits","41.70*56.16*3.70","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVTBD024A-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","900 nits","41.70*56.16*3.70","33.48*44.64","Resistive Touch Display,High-brightness TFT"]
["2.2”","KD022QVFBD014-RT","PDF","240x320","MCU","ER61516","Free V.A","RTP","-20℃~70℃","450 nits","41.70*56.16*3.85","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTPD040-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","170 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.2”","KD022QVFMD018-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","510 nits","41.70*56.16*3.85","33.84*45.12","Resistive Touch Display"]
["2.2”","KD022QVTPD039-RT","PDF","240x320","SPI+RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","240 nits","41.70*56.16*3.80","33.48*44.64","Resistive Touch Display"]
["2.3”","KD023C-1-TP","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","RTP","-20℃~70℃","350 nits","52.35*46.35*3.80","46.75*35.06","Resistive Touch Display"]
["2.4”","KD024B-3C-TP","PDF","240x320","MCU","ST7789V","Free V.A","RTP","-20℃~70℃","350 nits","42.72*60.26*3.50","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024C-1H-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","500 nits","42.72*60.26*3.80","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFMA020-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","450 nits","42.92*60.26*3.78","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFMA021-RT","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","480 nits","42.92*60.26*3.78","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVFMD012-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","400 nits","42.72*60.26*3.30","36.72*48.96","Resistive Touch Display"]
["2.4”","KD024QVRMA041A-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","290 nits","42.92*60.26*3.55","36.72*48.96","Resistive Touch Display,Transflective TFT"]
["2.4”","KD024VGFPD094A-RT","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","RTP","-30℃~80℃","680 nits","42.92*60.26*3.30","36.72*48.96","Resistive Touch Display,Wide Temp TFT"]
["2.4”","KD024HVFMA089-TP","PDF","320x426","SPI&MCU&RGB","ST7796","Free V.A","RTP","-20℃~70℃","550 nits","42.92*60.26*3.78","36.72*48.88","Resistive Touch Display"]
["2.6”","KD026HVRMA010-TP","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","RTP","-30℃~85℃","430 nits","46.76*65.85*3.91","39.84*53.78","Resistive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026LQTMA008-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","V.A 12H","RTP","-20℃~70℃","240 nits","60.30*51.15*3.80","52.80*39.60","Resistive Touch Display"]
["2.6”","KD026QVFMD007-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","240 nits","46.00*64.00*3.80","39.60*52.80","Resistive Touch Display"]
["2.8”","KD028FM-1-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","650 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["2.8”","KD028QVTMA005-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 12H","RTP","-20℃~70℃","450 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["2.8”","KD028QVFMA011-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","500 nits","50.50*69.70*3.80","43.20*57.60","Resistive Touch Display"]
["3.0”","KD030WQFMD019-RT","PDF","240x400","SPI&MCU&RGB","ST7796S","Free V.A","CTP","-20℃~70℃","350 nits","45.04*77.00*3.89","38.88*64.80","Resistive Touch Display"]
["3.0”","KD030C-2-TP","PDF","240x400","MCU&RGB","ILI9327","V.A 12H","RTP","-20℃~70℃","300 nits","45.40*77.00*3.70","38.88*64.80","Resistive Touch Display"]
["3.2”","KD032FM-1-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","430 nits","57.04*78.95*4.20","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTMA011-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","CTP","-20℃~70℃","350 nits","55.00*77.20*3.80","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTMA015-TP","PDF","240x320","SPI&MCU&RGB","ST7789V","V.A 6H","RTP","-20℃~70℃","320 nits","55.00*77.20*3.80","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032QVTBN008-TP","PDF","240x320","MCU","ST7789V","V.A 12H","RTP","-20℃~70℃","220 nits","57.04*78.70*4.20","48.60*64.80","Resistive Touch Display"]
["3.2”","KD032VGFPD035-RTP","PDF","480x640","SPI+RGB","ST7701SN","Free V.A","RTP","-20℃~70℃","800 nits","54.35*73.51*4.09","49.25*65.66","Resistive Touch Display,High-brightness TFT"]
["3.5”","KD035HVTMA026-TP","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","RTP","-20℃~70℃","250 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVTMA027-TP","PDF","320x480","SPI&MCU&RGB","ILI9488","V.A 6H","RTP","-20℃~70℃","320 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035LQFPA093-TP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","450 nits","76.90*63.90*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-TP","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","RTP","-30℃~85℃","360 nits","63.00*85.00*4.05","53.28*71.04","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFMD137-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","500 nits","54.58*83.57*3.38","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFMA138-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","330 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFMA139-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","510 nits","55.50*94.96*3.70","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035HVFMD145-RT","PDF","320x480","SPI&MCU&RGB","ST7796S","Free V.A","RTP","-20℃~70℃","460 nits","54.58*83.57*3.40","48.96*73.44","Resistive Touch Display"]
["3.5”","KD035LQFPA093-04-RTP-A","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","850 nits","76.90*63.90*4.35","70.08*52.56","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQTMN089-TP","PDF","320x240","SPI&MCU&RGB","SSD2119","V.A 12H","RTP","-20℃~70℃","330 nits","78.10*64.90*4.45","70.08*52.56","Resistive Touch Display"]
["3.5”","KD035LQTMD188-RT","PDF","320x240","SPI&MCU&RGB","ST7796","V.A 12H","RTP","-20℃~70℃","400 nits","77.80*64.50*4.30","70.08*52.56","Resistive Touch Display"]
["3.5”","KD035HVFMA155A-RT","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","RTP","-30℃~85℃","610 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-05-RTP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","550 nits","76.95*64.00*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["4.0”","KD040WVFPA027-RT","PDF","480x800","SPI+RGB","ST7701S","Free V.A","RTP","-20℃~70℃","400 nits","58.26*98.10*3.60","51.84*86.40","Resistive Touch Display"]
["4.0”","KD040WXFPD014-01-RTP","PDF","480x480","RGB","ST7701S","Free V.A","RTP","-30℃~85℃","800 nits","77.00*80.00*3.50","71.86*70.18","Resistive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.3”","KD043WQFPA042-01-RT","PDF","480x272","RGB","SC7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQTPA097A-01-RT","PDF","480x272","RGB","NV3047E","V.A 12H","RTP","-20℃~70℃","400 nits","105.40*67.15*4.06","95.04*53.86","Resistive Touch Display"]
["4.3”","KD043WVFBD082-RT","PDF","480x800","MCU","ILI9806","Free V.A","RTP","-20℃~70℃","380 nits","62.66*105.95*3.85","56.16*93.60","Resistive Touch Display"]
["4.3”","KD043WVFPA084-01-RT","PDF","480x800","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","370 nits","62.50*105.55*3.70","56.16*93.60","Resistive Touch Display"]
["4.3”","KD043WVFPA051-02-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","1000 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-RT","PDF","800x480","LVDS","ST7262","Free V.A","RTP","-30℃~85℃","950 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFMD134-01-RT","PDF","480x272","MCU","NV3041A-01","Free V.A","RTP","-20℃~70℃","950 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-RT","PDF","480x272","RGB","ST7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQTPA115-01-RT","PDF","480x272","RGB","ST7282","V.A 12H","RTP","-30℃~85℃","400 nits","105.50*67.20*5.10","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA142-01-RT","PDF","480x272","RGB","ST7282A","Free V.A","RTP","-30℃~80℃","550 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.5”","KD045FWFPA010-01-RT","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","400 nits","61.54*110.09*3.80","55.44*98.64","Resistive Touch Display"]
["5.0”","KD050WVFPA029-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","650 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFPA011-TP","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","430 nits","67.56*122.35*3.80","61.63*109.65","Resistive Touch Display"]
["5.0”","KD050HDFPA054-RT","PDF","720x1280","RGB","NV3052CGRB","Free V.A","RTP","-20℃~70℃","320 nits","67.56*122.35*3.80","62.10*110.40","Resistive Touch Display"]
["5.0”","KD050HDFIA061-RT","PDF","720x1280","MIPI","ILI9881C","Free V.A","RTP","-20℃~70℃","320 nits","67.56*122.35*3.80","62.10*110.40","Resistive Touch Display"]
["5.0”","KD050WVTPA045-RT","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","RTP","-20℃~70℃","280 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display"]
["5.0”","KD050FWFBA002-TP","PDF","480x854","MCU","ILI9806E","Free V.A","RTP","-20℃~70℃","450 nits","67.56*122.35*3.80","61.56*109.53","Resistive Touch Display"]
["5.0”","KD050WVFPA107-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","760 nits","118.50*77.80*5.10","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-06-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","700 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVTPA045-02A-TP","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","RTP","-20℃~70℃","650 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display"]
["5.0”","KD050WVFPA018-RTP","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","RTP","-30℃~85℃","560 nits","124.90*78.10*4.05","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050FWFPA011-09-TP","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","RTP","-20℃~70℃","410 nits","67.56*122.35*3.70","61.63*109.65","Resistive Touch Display"]
["5.6”","KD056VGTPA004-RT","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","RTP","-20℃~70℃","700 nits","126.50*100.00*7.30","115.00*86.40","Resistive Touch Display"]
["5.6”","KD056VGTPA003-RT","PDF","640x480","RGB","TBD","V.A 12H","RTP","-20℃~70℃","350 nits","126.50*100.00*5.50","112.90*84.67","Resistive Touch Display"]
["5.7”","KD057VGFPA015-RT","PDF","640x480","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","480 nits","126.50*100.00*7.40","115.20*86.40","Resistive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGTPA003-TP","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","RTP","-20℃~70℃","600 nits","144.00*104.60*14.60","115.20*86.40","Resistive Touch Display"]
["5.9”","KD059WVFPD001-RTP","PDF","840x512","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.16*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-RTP","PDF","840x512","LVDS","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.76*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-RTP","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","RTP","-30℃~85℃","750 nits","163.10*67.10*4.21","148.80*53.76","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA011-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","300 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDTLA020-TP","PDF","1024x600","LVDS","EK73215&EK79001","V.A 12H","RTP","-20℃~70℃","490 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFPA019-RT","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","630 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070C-4-TP","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","RTP","-20℃~70℃","430 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display"]
["7.0”","KD070WVTPA006-TP","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","RTP","-20℃~70℃","400 nits","165.00*100.00*7.19","154.08*85.92","Resistive Touch Display"]
["7.0”","KD070WVFPA065-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","480 nits","165.40*104.59*7.00","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA043-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1100 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-RT","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1000 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA028-RT","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","580 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070HDFIA030-RT","PDF","1024x600","MIPI","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","480 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["7.0”","KD070WVTPA088-01-RT","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-RT","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA011-02-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","850 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA010-02-RTP","PDF","800x480","RGB","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","640 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFIA030-02-RT","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","RTP","-20℃~70℃","1500 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLA028-06-RT","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","580 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display"]
["8.0”","KD080C-4-TP","PDF","800x600","RGB","TBD","V.A 6H","RTP","-20℃~70℃","270 nits","183.00*141.00*7.11","162.00*121.50","Resistive Touch Display"]
["8.0”","KD080WVFLA034-RT","PDF","800x600","LVDS","JD9165BA","Free V.A","RTP","-20℃~70℃","730 nits","182.90*141.00*7.20","162.00*121.50","Resistive Touch Display"]
["8.0”","KD080WVFPA032-RT","PDF","800x600","RGB","JD9165BA","Free V.A","RTP","-20℃~70℃","730 nits","182.90*141.00*7.20","162.00*121.50","Resistive Touch Display"]
["9.0”","KD090C-1-RT","PDF","800x480","RGB","TBD","V.A 6H","RTP","-20℃~70℃","300 nits","210.70*126.50*6.90","198.00*111.70","Resistive Touch Display"]
["9.0”","KD090HDFLA006-RTP","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-RTP","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008-RTP","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]

{"sheet":"High-brightness TFT","index":3,"n_rows":437,"n_cols":13,"rows_kept":437}
["STARTEK High-brightness TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.96”","KD0096SHFSD006-02","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["0.96”","KD0096SHFSD006-a","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.44”","KD014QQTBN002","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","No TP","-20℃~70℃","800 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.44”","KD014QQFBN006","PDF","128x128","SPI&MCU","ST7735S","Free V.A","No TP","-20℃~70℃","950 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.5”","KD015QVFMD020-C001D","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","800 nits","37.52*41.10*3.82","27.72*27.72","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["1.8”","KD018HVFMD042","PDF","360x360","MCU/SPI/QSPI","ST77916","Free V.A","No TP","-20℃~70℃","800 nits","48.08*49.95*1.94","45.68*45.68","High-brightness TFT,Round TFT"]
["2.0”","KD019QQFBN002-C001A","PDF","128x160","SPI&MCU","ST7735","Free V.A","CTP","-20℃~70℃","900 nits","47.47*59.04*3.20","31.87*39.84","Capacitive Touch Display,High-brightness TFT"]
["2.0”","KD019QQFBN002","PDF","128x160","SPI&MCU","ST7735","Free V.A","No TP","-20℃~70℃","1000 nits","37.47*49.04*2.02","31.87*39.84","High-brightness TFT"]
["2.0”","KD020WQFPA023-RT","PDF","480x360","SPI+RGB","ST7701S","Free V.A","RTP","-30℃~85℃","900 nits","46.50*41.56*3.70","40.82*30.62","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023","PDF","480x360","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024","PDF","480x360","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","900 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023-C003B","PDF","480x360","SPI+RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024-C003B","PDF","480x360","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","820 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD019QQFBN002-RT","PDF","128x160","SPI&MCU","ST7735","Free V.A","RTP","-20℃~70℃","800 nits","37.47*49.04*3.22","31.87*39.84","Resistive Touch Display,High-brightness TFT"]
["2.0”","KD020WQFPA023-C003B-RS232","PDF","480x360","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS485","PDF","480x360","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020WQFPA023-C003B-TTL","PDF","480x360","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.1”","KD021WVFPD003-02","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","56.18*59.71*2.24","53.28*53.28","High-brightness TFT,Round TFT"]
["2.2”","KD022QVTBD024A","PDF","240x320","MCU","ST7789V","V.A 6H","No TP","-20℃~70℃","1000 nits","41.70*56.16*2.72","33.48*44.64","High-brightness TFT"]
["2.2”","KD022QVTBD024A-RT","PDF","240x320","MCU","ST7789V","V.A 6H","RTP","-20℃~70℃","900 nits","41.70*56.16*3.70","33.48*44.64","Resistive Touch Display,High-brightness TFT"]
["2.4”","KD024WVFLD101","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024VGFPD094","PDF","480x640","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFID095","PDF","480x640","MIPI","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFPD094-C042A","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","900 nits","42.92*60.26*3.95","36.72*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102-C001A-RS232","PDF","800x480","RS232","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-RS485","PDF","800x480","RS485","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFLD101A","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101A-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102A","PDF","800x480","RGB","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102A-C001A","PDF","800x480","RGB","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024EGOIN152-01","PDF","450x600","MCU/MIPI","RM690B0","Free V.A","No TP","-20℃~80℃","800 nits","38.72*51.56*1.00","36.72*48.96","AMOLED Display,High-brightness TFT,LTPS Display"]
["2.5”","KD025EGOIN002-C000","PDF","400x712","MIPI","RM690C0","Free V.A","CTP","-20℃~70℃","800 nits","32.90*58.56*2.00","31.10*55.36","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["2.6”","KD026WXFLD022","PDF","1280x720","LVDS","SC5014","Free V.A","No TP","-20℃~70℃","1300 nits","63.88*43.46*2.74","57.60*32.40","High-brightness TFT"]
["2.6”","KD026WXFLD022-C008A","PDF","1280x720","LVDS","SC5014","Free V.A","CTP","-20℃~70℃","1200 nits","73.88*53.46*4.37","57.60*32.40","Capacitive Touch Display,High-brightness TFT"]
["2.6”","KD026WXFLD022-C008A-RS232","PDF","1280x720","RS232","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-TTL","PDF","1280x720","TTL","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-RS485","PDF","1280x720","RS485","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.7”","KD027HVFMD010","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009-C004A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.8”","KD028FM-1","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","850 nits","50.50*69.70*2.60","43.20*57.60","High-brightness TFT"]
["2.8”","KD028WXFID076","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["2.8”","KD028WXFPD075","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["3.2”","KD032VGFPD035-RTP","PDF","480x640","SPI+RGB","ST7701SN","Free V.A","RTP","-20℃~70℃","800 nits","54.35*73.51*4.09","49.25*65.66","Resistive Touch Display,High-brightness TFT"]
["3.2”","KD032VGFID034-C008A","PDF","480x640","MIPI","ST7701SN","Free V.A","CTP","-20℃~70℃","850 nits","66.85*85.51*4.25","49.25*65.66","Capacitive Touch Display,High-brightness TFT"]
["3.4”","KD034WXFID001","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","No TP","-30℃~70℃","950 nits","65.72*69.64*14.00","60.48*60.48","High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFID001-C001A-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*16.00","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFLD005","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*4.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFLD005-C001A","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","800 nits","65.72*69.64*6.34","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-RS232","PDF","480x480","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-RS485","PDF","480x480","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-TTL","PDF","480x480","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.5”","KD035VGFIA111A-01-C041A","PDF","480x640","MIPI","ILI9806E","Free V.A","CTP","-20℃~70℃","1250 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFIA111A-01","PDF","480x640","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","1600 nits","64.00*85.00*3.10","53.28*71.04","High-brightness TFT"]
["3.5”","KD035VGFPA094-02","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","1550 nits","64.00*85.00*3.10","53.28*71.04","High-brightness TFT,Blanview TFT"]
["3.5”","KD035VGFPA094-02-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","1300 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT,Blanview TFT"]
["3.5”","KD035HVFMD145-01-C005C","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","61.90*96.04*3.90","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035HVFMD145-01","PDF","320x480","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","54.58*83.57*2.20","48.96*73.44","High-brightness TFT"]
["3.5”","KD035VGFPD249","PDF","640x480","RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035QVFID225-C086A","PDF","320x480","MIPI","AXS15231","Free V.A","CTP","-20℃~70℃","800 nits","61.90*96.04*3.24","48.96*73.44","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035VGFPD249-C061B","PDF","640x480","RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFID251","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-20℃~70℃","1100 nits","74.38*62.35*2.43","70.08*52.56","High-brightness TFT"]
["3.5”","KD035LQFPA252","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","850 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA252-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035HVFMA155-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS232","PDF","320x240","RS232","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS485","PDF","320x240","RS485","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-TTL","PDF","320x240","TTL","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-CAN","PDF","320x240","CAN","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS232","PDF","320x240","RS232","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS485","PDF","320x240","RS485","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-TTL","PDF","320x240","TTL","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-CAN","PDF","320x240","CAN","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQTMN196-04","PDF","320x240","MCU","ST7796","V.A 12H","No TP","-30℃~85℃","1500 nits","78.10*64.90*3.10","70.08*52.56","High-brightness TFT"]
["3.5”","KD035VGFPD167-C061B-SP004A-HDMI","PDF","640x480","HDMI","NV3052CGRB","Free V.A","CTP","-10℃~60℃","500 nits","85.80*85.80*21.36","70.08*52.56","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["3.5”","KD035VGFIA281","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-30℃~85℃","1100 nits","76.91*63.90*3.15","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFLD285","PDF","640x480","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*4.85","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFLD285-C061B","PDF","640x480","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","85.80*85.80*6.88","70.08*52.56","Capacitive Touch Display,High-brightness TFT"]
["3.5”","KD035LQFPA093-04","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","900 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-RTP-A","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","850 nits","76.90*63.90*4.35","70.08*52.56","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","76.95*64.00*4.35","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.6”","KD036AUFPA002","PDF","544x506","RGB","ST72566","Free V.A","No TP","-35℃~85℃","900 nits","99.88*94.12*7.71","89.76*83.49","Wide Temp TFT,High-brightness TFT,Round TFT"]
["3.8”","KD038HDFPD002","PDF","1024x600","RGB","JD9168","Free V.A","No TP","-20℃~70℃","900 nits","89.92*59.93*2.78","82.64*48.42","High-brightness TFT"]
["3.8”","KD038HDFLD001","PDF","1024x600","LVDS","JD9168","Free V.A","No TP","-20℃~70℃","900 nits","89.92*59.93*2.78","82.64*48.42","High-brightness TFT"]
["3.8”","KD038HDFPD002-C001A","PDF","1024x600","RGB","JD9168","Free V.A","CTP","-20℃~70℃","810 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFLD001-C001A","PDF","1024x600","LVDS","JD9168","Free V.A","CTP","-20℃~70℃","800 nits","97.92*67.93*4.81","82.64*48.42","Capacitive Touch Display,High-brightness TFT"]
["3.8”","KD038HDFPD002-C001A-RS232","PDF","1024x600","RS232","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-RS485","PDF","1024x600","RS485","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-TTL","PDF","1024x600","TTL","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.9”","KD039WQFPN002","PDF","480x128","RGB","ST7282","Free V.A","No TP","-20℃~70℃","2000 nits","102.46*34.40*3.58","95.04*25.34","High-brightness TFT,Bartype TFT"]
["3.9”","KD039WQFPN002-C001A","PDF","480x128","RGB","ST7282","Free V.A","CTP","-30℃~85℃","1900 nits","112.46*44.40*5.61","95.04*25.34","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["4.0”","KD040WXFID017","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-01-RTP","PDF","480x480","RGB","ST7701S","Free V.A","RTP","-30℃~85℃","800 nits","77.00*80.00*3.50","71.86*70.18","Resistive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFID017-C015A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","950 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","850 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFLD071","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-30℃~85℃","950 nits","77.00*80.00*2.35","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFLD071-C015C","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","77.00*80.00*4.51","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFID017-C015C-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","77.00*80.00*16.00","71.86*70.18","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["4.0”","KD040HVFID080","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFID080-C050A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081-C050A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFID088","PDF","720x720","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","900 nits","105.60*109.87*2.16","101.52*101.52","High-brightness TFT,Round TFT"]
["4.0”","KD040FHFLD058-C041A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","1000 nits","104.87*72.22*4.76","88.59*49.83","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["4.0”","KD040FHFLD058","PDF","1920x1080","LVDS","SC5010","Free V.A","No TP","-20℃~70℃","1100 nits","94.87*62.22*2.73","88.59*49.83","High-brightness TFT,LTPS Display"]
["4.0”","KD040HDFID088-C054A","PDF","720x720","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","800 nits","125.29*127.29*3.41","101.52*101.52","Capacitive Touch Display,High-brightness TFT,Round TFT"]
["4.0”","KD040WXFPD014-C046B","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","82.80*82.80*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-a","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.3”","KD043WQFPA042","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-01-C037C","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-C038A","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","115.40*79.15*4.80","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","1250 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","1000 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C049A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","115.40*79.15*4.86","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-RT","PDF","800x480","LVDS","ST7262","Free V.A","RTP","-30℃~85℃","950 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPD042-07-C017C-SP004A-HDMI","PDF","480x272","HDMI","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","115.40*79.15*20.40","95.04*53.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS232","PDF","480x272","RS232","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS485","PDF","480x272","RS485","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-TTL","PDF","480x272","TTL","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-CAN","PDF","480x272","CAN","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFMD134","PDF","480x272","MCU","NV3041A-01","Free V.A","No TP","-30℃~85℃","950 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFMD134-01-RT","PDF","480x272","MCU","NV3041A-01","Free V.A","RTP","-20℃~70℃","950 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,High-brightness TFT"]
["4.3”","KD043WQFMD134-01-C037A","PDF","480x272","MCU","NV3041A-01","Free V.A","CTP","-30℃~85℃","900 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-C037D","PDF","480x272","RGB","ST7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-01","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050FHFLD102","PDF","1920x1080","LVDS","SC5010B","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.76*2.77","110.59*62.21","High-brightness TFT,LTPS Display"]
["5.0”","KD050FWFPA011-010","PDF","480x854","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","950 nits","67.56*122.35*2.60","61.63*109.65","High-brightness TFT"]
["5.0”","KD050FHFID103","PDF","1920x1080","MIPI","SC5010E","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.67*2.77","110.59*62.20","High-brightness TFT,LTPS Display"]
["5.0”","KD050WVFPA107","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","950 nits","118.50*77.80*3.85","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA107-C104A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","900 nits","118.50*77.80*6.34","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109","PDF","480x272","RGB","ST7282","Free V.A","No TP","-30℃~85℃","1000 nits","120.16*75.36*2.53","110.88*62.83","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109-C107A","PDF","480x272","RGB","ST7282","Free V.A","CTP","-30℃~85℃","900 nits","120.16*75.36*4.56","110.88*62.83","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","120.70*75.90*4.48","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVTPA045-02A","PDF","800x480","RGB","ILI5960/ILI6122","V.A 12H","No TP","-20℃~70℃","800 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT"]
["5.0”","KD050WVFPA029-06","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","850 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050FHFLD102-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","116.59*72.76*18.67","110.59*62.21","High-brightness TFT,HDMI TFT"]
["5.0”","KD050FHFLD102-01-C085B","PDF","1920x1080","LVDS","SC5010B","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["5.0”","KD050WVFLA033","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050FHFLD079-C085A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050FWFIA019-004","PDF","480x854","MIPI","ILI9806E","Free V.A","No TP","-20℃~70℃","950 nits","67.56*122.35*2.60","61.63*109.65","High-brightness TFT"]
["5.0”","KD050FHFID103-01-C085B","PDF","1920x1080","MIPI","SC5010E","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT"]
["5.0”","KD050WVFLA146","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-01","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.16*75.36*2.70","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02-C039A","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","950 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-02-C045A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","850 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.6”","KD056VGTPA004","PDF","640x480","RGB","HX8250-A+HX8678-B","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*5.70","115.20*86.40","High-brightness TFT"]
["5.6”","KD056VGTPA004-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*13.08","115.20*86.40","High-brightness TFT,HDMI TFT"]
["5.6”","KD056VGTPA006","PDF","640x480","RGB","ILI6192A-01/ ILI5481A","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*5.70","112.90*84.68","High-brightness TFT"]
["5.8”","KD058UXFLA003-C001A","PDF","1920x1080","LVDS","ST5892B","Free V.A","CTP","-20℃~70℃","950 nits","144.56*87.40*7.65","126.72*71.28","Capacitive Touch Display,High-brightness TFT"]
["5.8”","KD058UXFLA003","PDF","1920x1080","LVDS","ST5892B","Free V.A","No TP","-20℃~70℃","950 nits","144.56*87.40*5.50","126.72*71.28","High-brightness TFT"]
["5.8”","KD058UXFLA003-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","No TP","-10℃~60℃","950 nits","144.56*87.40*20.40","126.72*71.28","High-brightness TFT,HDMI TFT"]
["5.8”","KD058UXFLA003-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","CTP","-20℃~70℃","900 nits","144.56*87.40*21.26","126.72*71.28","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["5.9”","KD059WVFPD001","PDF","840x512","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.16*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-C001A","PDF","840x512","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.16*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-RTP","PDF","840x512","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.16*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003","PDF","840x512","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003-C001A","PDF","840x512","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002","PDF","840x512","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-C001A","PDF","840x512","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-RTP","PDF","840x512","LVDS","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.76*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPA003-01-SP001A-HDMI","PDF","640x240","HDMI","ST5043AA/ST5894AA","Free V.A","No TP","-20℃~70℃","900 nits","163.60*67.60*17.77","148.80*53.76","High-brightness TFT,Bartype TFT,HDMI TFT"]
["6.2”","KD062VGFPD003-C002A","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","800 nits","173.80*82.76*4.76","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.10*67.10*2.71","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-C002A-TTL","PDF","640x240","TTL","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS485","PDF","640x240","RS485","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS232","PDF","640x240","RS232","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPA003-01","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.60*67.60*2.87","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062HDFLD005-01-C007A","PDF","1024x600","LVDS","JD9168S","Free V.A","CTP","-20℃~70℃","1350 nits","155.40*88.40*6.68","137.47*77.23","Capacitive Touch Display,High-brightness TFT"]
["6.7”","KD067WSFLA001","PDF","1920x1080","LVDS","HX8249/HX8678","Free V.A","No TP","-20℃~70℃","1300 nits","161.12*97.68*4.77","148.32*83.43","High-brightness TFT"]
["6.7”","KD067WSFLA001-C001A","PDF","1920x1080","LVDS+eDP","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1300 nits","161.12*97.68*7.12","148.32*84.43","Capacitive Touch Display,High-brightness TFT"]
["6.7”","KD067WSFLA001-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1500 nits","161.12*97.68*23.02","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1100 nits","161.12*97.68*20.67","148.32*83.43","High-brightness TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-C001A-SP002A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1000 nits","161.12*97.68*23.10","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068HDFLD004","PDF","480x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1650 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005","PDF","480x1280","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","2350 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005-C001A","PDF","480x1280","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","2250 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFLD004-C001A","PDF","480x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1450 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068WVFPA007","PDF","800x480","RGB","TBD","Free V.A","No TP","-30℃~85℃","800 nits","156.10*100.91*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPA007-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","No TP","-20℃~70℃","800 nits","156.10*100.91*21.40","140.10*88.86","High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPD007-01-C003A","PDF","800x480","RGB","TBD","Free V.A","CTP","-30℃~85℃","800 nits","155.96*100.77*7.29","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","CTP","-20℃~70℃","800 nits","155.96*100.77*23.19","148.10*88.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPA001","PDF","800x480","RGB","ST72658","Free V.A","No TP","-30℃~85℃","800 nits","165.00*100.00*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS232","PDF","800x480","RS232","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS485","PDF","800x480","RS485","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-TTL","PDF","800x480","TTL","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-CAN","PDF","800x480","CAN","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068HDFPD011","PDF","480x1280","RGB","GC9704","Free V.A","No TP","-20℃~70℃","2000 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009","PDF","480x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","2100 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009-C009A","PDF","480x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","2000 nits","78.20*191.10*6.42","60.19*160.51","High-brightness TFT,Bartype TFT"]
["7.0”","KD070WVTPA077","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","No TP","-20℃~70℃","1300 nits","165.00*100.00*5.80","154.08*85.92","High-brightness TFT"]
["7.0”","KD070WVTPA077-C004A","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","CTP","-20℃~70℃","1100 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFPA010-02","PDF","800x480","RGB","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","800 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLD070","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-30℃~85℃","1100 nits","166.90*108.65*7.40","152.45*91.47","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1100 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-C049A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-RT","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1000 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFIA030-04-C027B","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","850 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD070-C085A","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","CTP","-30℃~85℃","980 nits","182.45*121.47*9.38","152.45*91.47","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","Free V.A","No TP","-10℃~60℃","1100 nits","65.40*104.59*22.90","152.40*91.44","High-brightness TFT,HDMI TFT"]
["7.0”","KD070WVFLA035A-C049C-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","V.A 12H","CTP","-10℃~60℃","1000 nits","165.40*104.59*24.83","152.40*91.44","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["7.0”","KD070WXFID093","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","1200 nits","103.46*162.28*7.63","94.20*150.72","High-brightness TFT"]
["7.0”","KD070HDFLA044","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1600 nits","165.10*100.10*5.50","154.21*85.92","High-brightness TFT"]
["7.0”","KD070HDFID086-C102A","PDF","720x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID093A-C107A","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1200 nits","119.46*176.78*7.27","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFLD083","PDF","800x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1200 nits","103.46*162.28*5.18","94.20*150.72","High-brightness TFT"]
["7.0”","KD070HDFLD092-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.62","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLA044-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1600 nits","165.10*100.10*6.81","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD089","PDF","720x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1150 nits","96.30*167.70*5.22","86.94*154.56","High-brightness TFT"]
["7.0”","KD070HDFLD089-C102A","PDF","720x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1100 nits","107.00*177.00*7.09","86.94*154.56","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD092-C113A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.67","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099","PDF","800x480","RGB","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.10*100.10*5.10","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","850 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","1000 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLD092-C050B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","182.07*117.60*7.22","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVTPA006-02","PDF","800x480","RGB","EK9713/EK7330","V.A 12H","No TP","-20℃~70℃","1000 nits","165.00*100.00*5.80","154.08*85.92","High-brightness TFT"]
["7.0”","KD070WXFID050-02","PDF","800x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~60℃","850 nits","103.56*162.38*2.70","94.20*150.72","High-brightness TFT"]
["7.0”","KD070WVFPA043A-C049A-RS232","PDF","800x480","RS232","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-RS485","PDF","800x480","RS485","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-TTL","PDF","800x480","TTL","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFIA030-02","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","No TP","-20℃~70℃","1700 nits","165.00*100.00*5.80","154.21*85.92","High-brightness TFT"]
["7.0”","KD070HDFIA030-02-C028A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","182.07*117.60*8.25","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-02-C029A","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","CTP","-20℃~70℃","1500 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFIA030-02-RT","PDF","1024x600","MIPI","EK73217BCGA+EK79007AD2","Free V.A","RTP","-20℃~70℃","1500 nits","165.00*100.00*7.30","154.21*85.92","Resistive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLD106-C114A","PDF","800x480","LVDS","ST7277-G6-K","Free V.A","CTP","-20℃~70℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WUFID123-C123A","PDF","1200x1920","MIPI","FT7250","Free V.A","CTP","-20℃~70℃","950 nits","109.80*173.00*5.00","94.50*151.20","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WXFID094-CP001A-HDMI","PDF","280x1424","HDMI","OTA7290N","Free V.A","No TP","-20℃~70℃","900 nits","38.20*181.47*3.44","33.60*170.88","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.0”","KD070WVFLA125","PDF","800x480","LVDS","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070FHOIN128-C0000","PDF","1080x1920","MIPI","ICNA3512","Free V.A","CTP","-20℃~70℃","950 nits","89.13*160.91*1.01","87.13*154.91","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["7.0”","KD070HDFLD070-SP001A-HDMI","PDF","1280x768","HDMI","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-10℃~60℃","1200 nits","166.90*108.65*21.23","152.45*91.47","High-brightness TFT,HDMI TFT"]
["7.0”","KD070HDFPA038-C024A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFLA028-06-C014C","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLA028-06-C014A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*8.15","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070WVFLD106","PDF","800x480","LVDS","ST7277-G6-K","Free V.A","No TP","-20℃~70℃","950 nits","165.10*100.10*5.10","153.84*85.63","High-brightness TFT"]
["7.0”","KD070WVFPA043A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043A-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A-C049C","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFID086","PDF","720x1280","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","1200 nits","96.30*167.70*5.22","86.94*154.56","High-brightness TFT"]
["7.0”","KD070HDFLA028-06-C015B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","165.00*100.00*7.33","154.21*85.92","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["7.0”","KD070WVFPA140","PDF","800x480","RGB","ST7277-G6-K","Free V.A","No TP","-30℃~85℃","1200 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD140-01-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","1050 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["7.0”","KD070WXFID138-C038B","PDF","800x1280","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","1100 nits","119.46*176.78*6.46","94.20*150.72","Capacitive Touch Display,High-brightness TFT"]
["7.0”","KD070HDFLD092","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-30℃~85℃","1600 nits","165.10*100.10*5.12","154.21*85.92","High-brightness TFT,Wide Temp TFT"]
["7.84”","KD078HDFID004","PDF","400x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","1100 nits","67.60*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002","PDF","400x1280","RGB","GC9704C","Free V.A","No TP","-20℃~70℃","1000 nits","67.90*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFID004-C004A","PDF","400x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","950 nits","67.60*206.28*6.27","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002-C003A-RS232","PDF","400x1280","RS232","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS485","PDF","400x1280","RS485","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-TTL","PDF","400x1280","TTL","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFID004-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","No TP","-20℃~70℃","800 nits","67.60*206.28*19.29","59.40*190.08","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078HDFID004-C004A-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","CTP","-20℃~70℃","800 nits","67.60*206.28*21.12","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["8.0”","KD080WUFLD027","PDF","1920x1200","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1500 nits","179.96*119.92*4.20","172.22*107.64","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080WVTPA029","PDF","800x480","RGB","TBD","V.A 6H","No TP","-30℃~80℃","900 nits","192.80*116.90*6.40","176.64*99.36","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080WVFPA032","PDF","800x600","RGB","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WXFID015-02","PDF","800x1280","MIPI","ILI9881","Free V.A","No TP","-20℃~60℃","850 nits","114.70*184.20*2.70","107.64*172.22","High-brightness TFT"]
["8.0”","KD080WXFID015-02-C015A","PDF","800x1280","MIPI","ILI9881","Free V.A","CTP","-20℃~60℃","800 nits","130.70*200.10*4.90","107.64*172.22","Capacitive Touch Display,High-brightness TFT"]
["8.0”","KD080WVFLA034","PDF","800x600","LVDS","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WVFIA033","PDF","800x600","MIPI","JD9165BA","Free V.A","No TP","-20℃~70℃","800 nits","182.90*141.00*5.55","162.00*121.50","High-brightness TFT"]
["8.0”","KD080WUFLD040","PDF","1920x1200","LVDS","FL5893DA","Free V.A","No TP","-20℃~70℃","1800 nits","181.80*119.85*5.35","172.22*107.64","High-brightness TFT"]
["8.0”","KD080WUFLD040-C034A","PDF","1920x1200","LVDS","FL5893DA","Free V.A","CTP","-20℃~70℃","1750 nits","181.80*119.85*7.40","172.22*107.64","Capacitive Touch Display,High-brightness TFT"]
["8.9”","KD089FHFID004","PDF","480x1920","MIPI","OTA7290N","Free V.A","No TP","-20℃~70℃","950 nits","64.10*231.20*4.73","54.72*218.88","High-brightness TFT,Bartype TFT"]
["8.9”","KD089FHFID004-C001A","PDF","480x1920","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","850 nits","76.00*243.10*6.75","54.72*218.88","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["9.0”","KD090HWFLA004","PDF","1280x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1000 nits","210.70*124.15*6.20","198.91*111.89","Wide Temp TFT,High-brightness TFT"]
["9.0”","KD090HDFLA006","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFLA006-SP001A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*22.50","196.61*114.15","High-brightness TFT,HDMI TFT"]
["9.0”","KD090HDFPA007","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFLA006-C001A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFLA006-RTP","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-RTP","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008-RTP","PDF","1024x600","MIPI","EK73217& EK79007","Free V.A","RTP","-20℃~70℃","850 nits","210.70*126.50*6.99","196.61*114.15","Resistive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFIA008","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*5.10","196.61*114.15","High-brightness TFT"]
["9.0”","KD090HDFIA008-C001A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFPA007-C001A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","900 nits","210.70*126.50*7.15","196.61*114.15","Capacitive Touch Display,High-brightness TFT"]
["9.0”","KD090HDFLA006-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.8”","KD098WXTIA-001","PDF","1280x320","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1300 nits","252.75*73.17*11.00","241.15*60.29","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA010","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","252.70*175.55*6.44","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA010-C016A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","252.70*175.55*9.25","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101FHFID031","PDF","440x1920","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","1000 nits","65.08*266.19*4.48","57.95*252.86","High-brightness TFT,Bartype TFT"]
["10.1”","KD101FHFID031-C037A","PDF","440x1920","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*6.23","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["10.1”","KD101HDFLA020","PDF","1280x800","LVDS","EK79202B1","Free V.A","No TP","-20℃~70℃","1000 nits","232.70*155.55*5.00","216.96*135.60","High-brightness TFT"]
["10.1”","KD101HDFLD020-01-C045C-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","900 nits","232.70*155.56*24.50","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLD054","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","1000 nits","228.60*149.10*4.38","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101UXFLD024D","PDF","1920x1200","LVDS","HX8290-B","Free V.A","No TP","-20℃~70℃","1300 nits","229.46*149.10*7.65","216.81*135.50","High-brightness TFT"]
["10.1”","KD101WXFLD021-02-C045C-SP007A-HDMI","PDF","1280x800","HDMI","EK79202D_A","Free V.A","CTP","-20℃~70℃","700 nits","229.06*148.70*22.84","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WSFLA058","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.25","High-brightness TFT"]
["10.1”","KD101WSFLA058-C065A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101WSFPA055","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.28","High-brightness TFT"]
["10.1”","KD101WSFPA055-C065A","PDF","1024x600","RGB","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLD056A","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~80℃","1350 nits","228.80*147.90*4.66","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLD056A-C045E","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~80℃","1250 nits","252.96*171.60*6.91","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WSFIA057","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","No TP","-20℃~70℃","1100 nits","235.00*143.00*4.50","222.72*125.28","High-brightness TFT"]
["10.1”","KD101WSFIA057-C065A","PDF","1024x600","MIPI","EK73217&EK79007","Free V.A","CTP","-20℃~70℃","1000 nits","254.50*162.50*6.75","222.72*125.28","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101HDFLD020-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","232.70*155.55*22.50","216.96*135.60","High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLA020-C016A","PDF","1280x800","LVDS","EK79202B1","Free V.A","CTP","-20℃~70℃","1100 nits","252.70*175.55*10.31","216.96*135.60","Capacitive Touch Display,High-brightness TFT"]
["10.1”","KD101FHFID031-C037A-CP001A-HDMI","PDF","440x1920","HDMI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*12.29","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["10.1”","KD101UXFLD024D-SP001A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1000 nits","229.46*149.10*22.73","216.81*135.50","High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLD069","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~60℃","1000 nits","229.30*149.10*2.60","216.96*135.60","High-brightness TFT"]
["10.1”","KD101WSFLA058-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","235.00*143.00*20.90","222.72*125.28","High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLA059","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~85℃","1300 nits","229.46*149.10*7.06","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101WXFLD047-01","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","850 nits","229.06*148.70*2.51","216.96*135.60","High-brightness TFT"]
["10.1”","KD101UXFLD024D-01-C035A-SP002A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1100 nits","246.31*168.75*23.98","216.81*135.50","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.3”","KD103WUFLD001","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","258.60*107.00*6.37","243.65*91.37","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["10.4”","KD104WSTPA003","PDF","1024x100","RGB","HX8282，HX8678","V.A 12H","No TP","-20℃~70℃","1000 nits","288.92*41.50*6.89","264.19*25.80","High-brightness TFT,Bartype TFT"]
["10.4”","KD104XGFLA011","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","238.60*175.80*9.20","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104WVTLA008","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","900 nits","228.40*175.40*5.90","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD022","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1200 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA011-C009A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1300 nits","266.13*221.29*12.54","210.43*157.82","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA022-01","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1050 nits","225.80*174.35*5.92","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID025-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027-C011A","PDF","1024x768","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026","PDF","1024x768","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["11.6”","KD116WSFEA002","PDF","1920x1080","eDP","TBD","Free V.A","No TP","-20℃~70℃","1100 nits","268.00*158.00*4.87","256.32*144.18","High-brightness TFT"]
["11.6”","KD116FHFEA001-C001A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","800 nits","291.52*179.38*8.59","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["11.6”","KD116WSFEA003-CTP-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","1000 nits","298.22*186.10*44.00","257.32*145.18","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["11.6”","KD116WSFEA002-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","268.00*158.00*21.56","256.32*144.18","High-brightness TFT,HDMI TFT"]
["11.6”","KD116WSFEA002-C002A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","256.92*144.78","256.32*144.18","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFLA007","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","278.00*184.00*10.00","261.12*163.20","High-brightness TFT"]
["12.1”","KD121HDFLA009","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","283.00*185.10*9.40","261.12*163.20","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA013","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-20℃~70℃","800 nits","260.50*204.00*8.60","245.76*184.32","High-brightness TFT"]
["12.1”","KD121HDFLA014","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~85℃","800 nits","260.50*204.00*8.60","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA015-CTP-Monitor","PDF","1024x768","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","850 nits","294.50*233.00*44.00","247.00*185.50","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["12.1”","KD121HDFLD010-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1100 nits","306.50*196.20*14.50","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLD009-01-C006A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1350 nits","306.50*196.20*15.42","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121XGFLD024","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1250 nits","260.49*203.45*6.88","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA026","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","277.70*180.60*6.00","261.12*163.20","High-brightness TFT"]
["12.1”","KD121HDFLA026-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","294.10*196.20*8.10","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121UXFLA037","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1200 nits","276.60*179.50*5.70","262.83*164.27","High-brightness TFT"]
["12.1”","KD121UXFLA037-C014B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","305.00*200.00*8.65","262.83*164.27","Capacitive Touch Display,High-brightness TFT"]
["12.1”","KD121HDFLA035-C012B","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-20℃~70℃","1200 nits","294.10*196.20*9.33","261.12*163.20","Capacitive Touch Display,High-brightness TFT"]
["12.3”","KD123WUFLA003","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","308.10*130.00*15.10","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD005","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.63*123.61*6.55","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD006","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.10*125.50*6.35","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD006-C002A","PDF","1920x720","LVDS","TBD","Free V.A","CTP","-30℃~85℃","950 nits","311.02*132.60*9.15","292.03*109.51","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.8”","KD128FHFLD001-01","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~70℃","1000 nits","294.40*175.00*5.00","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["12.8”","KD128FHFLA002","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-40℃~85℃","800 nits","321.46*181.08*13.29","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["13.0”","KD130UXOEN001-C001A","PDF","2560x1440","eDP","RM98120","Free V.A","CTP","-40℃~85℃","800 nits","292.69*168.27*2.10","286.69*161.27","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["13.3”","KD133FHFED012","PDF","1920x1080","eDP","TBD","Free V.A","No TP","0℃~50℃","1250 nits","298.76*177.04*3.80","293.76*165.24","High-brightness TFT"]
["13.3”","KD133FHFLA013","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","800 nits","309.70*184.10*9.60","293.47*165.08","High-brightness TFT"]
["13.3”","KD133FHFLA013-C009A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~70℃","800 nits","325.20*199.80*9.65","293.47*165.08","Capacitive Touch Display,High-brightness TFT"]
["13.3”","KD133FHFLA013-C009A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-20℃~70℃","900 nits","325.20*199.80*22.55","293.47*165.08","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["13.3”","KD133FHFLA013-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-20℃~70℃","950 nits","309.70*184.10*19.35","293.47*165.08","High-brightness TFT,HDMI TFT"]
["13.5”","KD135HDFLA001","PDF","1280x235","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","360.00*83.00*15.90","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.5”","KD135HDFLA001-C001A","PDF","1280x235","LVDS","TBD","Free V.A","CTP","0℃~50℃","800 nits","380.00*106.00*18.95","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.9”","KD139HDFLD001","PDF","1280x400","LVDS","HX8249/HX8678","Free V.A","No TP","0℃~50℃","1400 nits","358.50*135.00*13.30","337.92*105.14","High-brightness TFT,Bartype TFT"]
["14.0”","KD140FHFLD003","PDF","1920x1080","eDP","TBD","Free V.A","No TP","-20℃~70℃","800 nits","317.52*186.73*4.80","308.16*173.34","High-brightness TFT,LTPS Display"]
["15.0”","KD150HDFLA007","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1200 nits","403.30*98.10*11.00","374.78*70.86","High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA007-C006B","PDF","1280x242","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","423.30*118.10*14.20","374.78*71.10","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA008","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","403.30*98.10*14.00","374.79*70.86","High-brightness TFT,Bartype TFT"]
["15.1”","KD151WQOEN001-C0000","PDF","2560x1600","eDP","RM98121","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*1.30","324.10*202.56","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["15.6”","KD156FHFLA011","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","360.00*212.30*5.70","344.16*193.59","High-brightness TFT"]
["15.6”","KD156FHFLA012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","363.80*215.90*9.30","344.16*193.59","Wide Temp TFT,High-brightness TFT"]
["15.6”","KD156FHFLA022-01","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","1200 nits","363.80*215.90*9.50","344.16*193.59","High-brightness TFT"]
["15.6”","KD156FHFLA022-02","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","800 nits","363.80*215.90*9.50","344.16*193.59","High-brightness TFT"]
["16.7”","KD167FHFLA001","PDF","1920x540","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1200 nits","439.00*144.00*14.00","408.96*115.02","High-brightness TFT,Bartype TFT"]
["17.0”","KD170SXFLA002","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","0℃~50℃","900 nits","358.50*296.50*10.30","337.92*270.34","High-brightness TFT"]
["17.0”","KD170SXTLA003","PDF","1280x1024","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1400 nits","358.50*296.50*10.50","337.92*270.34","Wide Temp TFT,High-brightness TFT"]
["18.5”","KD185FHFLA004","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","800 nits","430.37*254.60*11.50","408.96*230.04","High-brightness TFT"]
["18.5”","KD185FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1000 nits","430.40*254.60*12.00","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["18.5”","KD185FHFLA010","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","430.37*254.60*11.50","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["19.0”","KD190SGFLA005","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","-20℃~70℃","900 nits","395.60*323.80*15.00","376.32*301.06","High-brightness TFT"]
["21.5”","KD215FHFLD007","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","495.60*292.20*10.57","476.06*267.79","High-brightness TFT"]
["21.5”","KD215WSFLA012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","495.60*292.20*10.62","476.05*267.79","High-brightness TFT"]
["21.5”","KD215FHFLD007-C005A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","505.60*302.20*13.97","476.06*267.79","Capacitive Touch Display,High-brightness TFT"]
["21.5”","KD215FHFLA022","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~85℃","1000 nits","495.60*292.20*10.50","476.64*268.11","Wide Temp TFT,High-brightness TFT"]
["23.6”","KD236FHFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","544.80*320.50*18.70","521.28*293.22","High-brightness TFT"]
["23.6”","KD236SXFLA003","PDF","1280x1280","LVDS","TBD","Free V.A","No TP","-20℃~80℃","1500 nits","657.00*657.00*28.65","599.42*599.42","High-brightness TFT,Round TFT"]
["23.8”","KD238FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1500 nits","544.80*320.50*11.50","527.04*296.46","High-brightness TFT"]
["27.0”","KD270FHFLA002","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","800 nits","630.00*368.20*13.00","597.89*336.31","High-brightness TFT"]
["27.0”","KD270UDFEA008","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","1200 nits","612.20*358.20*14.63","596.74*335.66","High-brightness TFT"]
["27.0”","KD270QHOVD026","PDF","2560x1440","V-By-One","TBD","Free V.A","No TP","0℃~45℃","1300 nits","600.62*346.42*0.78","586.75*330.05","AMOLED Display,High-brightness TFT,LTPS Display"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,Display Monitor,OLED Monitor"]
["27.0”","KD270FHFLA022","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","2000 nits","618.00*360.00*20.80","597.90*336.30","High-brightness TFT"]
["27.0”","KD270FHFLA025","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","630.00*368.20*13.00","597.89*336.31","High-brightness TFT"]
["27.0”","KD270UHFEA024","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","800 nits","615.67*360.26*8.60","596.74*335.66","High-brightness TFT"]
["27.0”","KD270QHFLA029","PDF","2560x1440","LVDS","TBD","Free V.A","No TP","0℃~50℃","2200 nits","630.74*369.26*20.00","596.74*335.66","High-brightness TFT"]
["27.0”","KD270UHFLA030","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","1200 nits","630.74*369.26*20.00","596.74*335.66","High-brightness TFT"]
["31.5”","KD315FHFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","725.20*422.70*14.40","698.40*392.85","High-brightness TFT"]
["31.5”","KD315FHFLA001-C001A","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","0℃~50℃","900 nits","746.70*441.30*19.80","698.40*392.85","Capacitive Touch Display,High-brightness TFT"]
["31.5”","KD320FHFLA019","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~60℃","800 nits","727.00*420.00*9.70","698.40*392.85","High-brightness TFT"]
["31.5”","KD320UHFEA020","PDF","3840x2160","eDP","TBD","Free V.A","No TP","0℃~50℃","800 nits","727.00*420.00*9.70","697.31*392.23","High-brightness TFT"]
["32.0”","KD320FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1700 nits","719.40*416.90*26.60","698.40*392.90","High-brightness TFT,Mini-LED"]
["42.5”","KD430FHFLA019","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-5℃~50℃","1000 nits","969.30*557.65*15.00","940.90*529.25","High-brightness TFT"]
["43.0”","KD430WUFLA001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","0℃~50℃","1500 nits","973.20*561.50*29.50","941.18*529.42","High-brightness TFT"]
["43.0”","KD430UHFLA018","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","969.30*557.65*15.00","941.18*529.42","High-brightness TFT"]
["49.0”","KD490UHFVA019","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1103.20*633.40*15.20","1073.78*604.00","High-brightness TFT"]
["55.0”","KD550UHFVA032","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1239.00*709.80*16.00","1209.60*680.40","High-brightness TFT"]
["64.5”","KD650UHFVA002","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~50℃","800 nits","1458.88*833.92*18.50","1428.48*803.52","High-brightness TFT"]

{"sheet":"Wide Temp TFT","index":4,"n_rows":335,"n_cols":13,"rows_kept":335}
["STARTEK Wide Temp TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.91”","KD0091SQOIN001","PDF","128x32","i2C","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","38.00*12.00*3.80","22.38*5.58","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["0.96”","KD0096SQOSN009","PDF","128x64","SPI","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","27.30*27.80*4.10","21.74*10.86","PMOLED Display,Wide Temp TFT"]
["0.96”","KD0096SQOSN012","PDF","128x64","SPI/IIC","SSD1315","Free V.A","No TP","-40℃~85℃","80 nits","24.70*16.60*1.30","21.74*11.18","PMOLED Display,Wide Temp TFT"]
["1.1”","KD011SQOSN002","PDF","64x128","SPI","CH1115","Free V.A","No TP","-40℃~70℃","180 nits","24.00*33.00*3.80","10.86*25.58","PMOLED Display,Wide Temp TFT"]
["1.3”","KD013SQOIN012","PDF","128x64","i2C","SH1106","Free V.A","No TP","-40℃~70℃","150 nits","35.40*33.50*4.00","29.42*14.70","PMOLED Display,Wide Temp TFT"]
["1.5”","KD015SQOSN013","PDF","128x128","SPI","SH1107","Free V.A","No TP","-40℃~70℃","100 nits","34.00*49.30*5.00","26.86*26.86","PMOLED Display,Wide Temp TFT"]
["1.54”","KD0154WEOLN006","PDF","128x64","Parallel/SPI/I2C","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","42.04*27.22*1.46","35.04*17.51","PMOLED Display,Wide Temp TFT"]
["1.7”","KD017SQOIN003","PDF","128x32","i2C","SSD1312","Free V.A","No TP","-40℃~70℃","120 nits","60.50*18.75*4.95","42.22*10.54","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.0”","KD020WQFPA023-RT","PDF","480x360","SPI+RGB","ST7701S","Free V.A","RTP","-30℃~85℃","900 nits","46.50*41.56*3.70","40.82*30.62","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023","PDF","480x360","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024","PDF","480x360","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","900 nits","46.50*41.56*2.50","40.82*30.62","Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFPA023-C003B","PDF","480x360","SPI+RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020WQFIA024-C003B","PDF","480x360","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","820 nits","54.50*47.56*4.15","40.82*30.62","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.0”","KD020VGFPA038","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","No TP","-30℃~85℃","700 nits","35.80*52.10*2.65","30.60*40.80","Wide Temp TFT"]
["2.0”","KD020VGFIA039","PDF","480x640","MIPI","ST7701SI","Free V.A","No TP","-30℃~85℃","700 nits","35.80*52.10*2.65","30.60*40.80","Wide Temp TFT"]
["2.1”","KD021SCOIN007","PDF","256x64","i2C","SH1122","Free V.A","No TP","-40℃~70℃","150 nits","72.50*27.24*5.10","51.18*12.78","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.2”","KD022SQOSN037","PDF","128x32","SPI/IIC","SSD1305","Free V.A","No TP","-40℃~70℃","120 nits","74.00*30.00*8.20","55.02*13.10","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.4”","KD024VGFPD094","PDF","480x640","SPI+RGB","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFPD094A-RT","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","RTP","-30℃~80℃","680 nits","42.92*60.26*3.30","36.72*48.96","Resistive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFPD094-C021D","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024VGFID095","PDF","480x640","MIPI","ST7701S","Free V.A","No TP","-30℃~80℃","800 nits","42.92*60.26*2.30","36.72*48.96","Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024VGFID095-C021D","PDF","480x640","MIPI","ST7701SI","Free V.A","CTP","-30℃~80℃","680 nits","48.72*70.26*3.94","36.72*48.96","Capacitive Touch Display,Wide Temp TFT"]
["2.4”","KD024SQOSN132","PDF","128x64","SPI","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","72.00*43.00*7.00","55.01*27.49","PMOLED Display,Wide Temp TFT"]
["2.4”","KD024VGFPD094-C042A","PDF","480x640","SPI+RGB","ST7701SI","Free V.A","CTP","-30℃~80℃","900 nits","42.92*60.26*3.95","36.72*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.6”","KD026HVRMA010-TP","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","RTP","-30℃~85℃","430 nits","46.76*65.85*3.91","39.84*53.78","Resistive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRIA009","PDF","320x432","MIPI","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRMA010","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRMA010-C004B","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","CTP","-30℃~85℃","420 nits","46.76*65.85*4.26","39.84*53.78","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.7”","KD027HVFMD010","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009-C004A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027WVOIN011","PDF","800x600","MIPI","RM69700","Free V.A","No TP","-40℃~85℃","400 nits","56.60*47.25*1.50","54.60*40.95","AMOLED Display,Wide Temp TFT,LTPS Display"]
["2.8”","KD028QVFMA058","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-30℃~85℃","700 nits","50.50*69.70*2.60","43.20*57.60","Wide Temp TFT"]
["2.8”","KD028QVRMD073","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-30℃~80℃","160 nits","50.50*69.70*2.50","43.20*57.60","Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVRMD073-C050A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~80℃","150 nits","52.90*79.30*3.95","43.20*57.60","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVFMA058-C002A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~85℃","630 nits","50.50*69.70*3.85","43.20*57.60","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030FWFIN021A","PDF","480x854","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","550 nits","42.04*73.67*2.17","36.72*65.28","Wide Temp TFT"]
["3.0”","KD030FWFPN022A","PDF","480x854","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","550 nits","42.04*73.67*2.17","36.72*65.28","Wide Temp TFT"]
["3.0”","KD030FWFPN022A-C018A","PDF","480x854","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.0”","KD030FWFIN021A-C018A","PDF","480x854","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","500 nits","52.72*83.28*4.22","36.72*65.28","Capacitive Touch Display,Wide Temp TFT"]
["3.2”","KD032QVFMD028","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-30℃~85℃","500 nits","54.99*77.20*2.40","48.60*64.80","Wide Temp TFT"]
["3.5”","KD035LQFPA093-C051A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.85","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPD093-02-C037B","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.51","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","76.90*63.90*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","470 nits","86.84*74.84*4.40","70.08*52.56","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-TP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","450 nits","76.90*63.90*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064","PDF","240x320","MCU","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*3.00","53.28*71.04","Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-C021A","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*4.73","53.28*71.04","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035QVFMA064-04-TP","PDF","240x320","SPI&MCU&RGB","HX8347A","Free V.A","RTP","-30℃~85℃","360 nits","63.00*85.00*4.05","53.28*71.04","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035QHFID161","PDF","640x960","MIPI","ST7703","Free V.A","No TP","-30℃~85℃","500 nits","54.98*85.02*2.55","49.92*74.88","Wide Temp TFT"]
["3.5”","KD035QHFPD154","PDF","640x960","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","500 nits","54.98*84.42*2.55","49.92*74.88","Wide Temp TFT"]
["3.5”","KD035QHFPD154-C062B","PDF","640x960","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035QHFID161-C062B","PDF","640x960","MIPI","ST7703","Free V.A","CTP","-30℃~85℃","450 nits","61.90*96.04*4.57","49.92*74.88","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035VGFPD249","PDF","640x480","RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD249-C061B","PDF","640x480","RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*2.43","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFPD250-C061B","PDF","640x480","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*85.80*4.46","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA252","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","850 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA252-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035QVFMA064-RS232","PDF","240x320","RS232","HX8347A","Free V.A","No TP","-30℃~80℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-RS485","PDF","240x320","RS485","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-TTL","PDF","240x320","TTL","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS232","PDF","240x320","RS232","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS485","PDF","240x320","RS485","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-TTL","PDF","240x320","TTL","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS232","PDF","320x240","RS232","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS485","PDF","320x240","RS485","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-TTL","PDF","320x240","TTL","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-CAN","PDF","320x240","CAN","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS232","PDF","320x240","RS232","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS485","PDF","320x240","RS485","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-TTL","PDF","320x240","TTL","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-CAN","PDF","320x240","CAN","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFIA281","PDF","640x480","MIPI","ST7703","Free V.A","No TP","-30℃~85℃","1100 nits","76.91*63.90*3.15","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035VGFLD285","PDF","640x480","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","74.38*62.35*4.85","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04","PDF","320x240","RGB","ST7272A","Free V.A","No TP","-30℃~85℃","900 nits","76.95*64.00*3.17","70.08*52.56","Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-RTP-A","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","850 nits","76.90*63.90*4.35","70.08*52.56","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035LQFPA093-04-C037A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","86.84*74.84*4.90","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.5”","KD035HVFMA155A","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","No TP","-30℃~85℃","700 nits","55.50*84.96*2.50","48.96*73.44","Wide Temp TFT"]
["3.5”","KD035HVFMA155A-C055A","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","55.50*84.96*4.25","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFMA155A-C005C","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","CTP","-30℃~85℃","630 nits","61.90*96.04*4.30","48.96*73.44","Capacitive Touch Display,Wide Temp TFT"]
["3.5”","KD035HVFMA155A-RT","PDF","320x480","SPI&MCU&RGB","ST7796SI","Free V.A","RTP","-30℃~85℃","610 nits","55.50*84.96*3.70","48.96*73.44","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-05-RTP","PDF","320x240","RGB","ST7272A","Free V.A","RTP","-30℃~85℃","550 nits","76.95*64.00*4.32","70.08*52.56","Resistive Touch Display,Wide Temp TFT"]
["3.5”","KD035LQFPA093-04-C036A","PDF","320x240","RGB","ST7272A","Free V.A","CTP","-30℃~85℃","800 nits","76.95*64.00*4.35","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["3.6”","KD036AUFPA002","PDF","544x506","RGB","ST72566","Free V.A","No TP","-35℃~85℃","900 nits","99.88*94.12*7.71","89.76*83.49","Wide Temp TFT,High-brightness TFT,Round TFT"]
["3.7”","KD037WVOPD004","PDF","480x800","RGB","TL2796","Free V.A","No TP","-30℃~80℃","250 nits","53.94*90.00*1.50","48.24*80.40","AMOLED Display,Wide Temp TFT,LTPS Display"]
["3.9”","KD039WQFPN002-C001A","PDF","480x128","RGB","ST7282","Free V.A","CTP","-30℃~85℃","1900 nits","112.46*44.40*5.61","95.04*25.34","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["4.0”","KD040WXFID017","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-01-RTP","PDF","480x480","RGB","ST7701S","Free V.A","RTP","-30℃~85℃","800 nits","77.00*80.00*3.50","71.86*70.18","Resistive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFID017-C015A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","950 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","850 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFID032","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID032-C026C","PDF","720x720","MIPI","ST7703","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*3.76","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID035","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*4.23","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040QHFPD047","PDF","400x960","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","500 nits","42.50*102.08*2.02","39.18*94.03","Wide Temp TFT,Bartype TFT"]
["4.0”","KD040WXFLD071","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-30℃~85℃","950 nits","77.00*80.00*2.35","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFLD071-C015C","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","77.00*80.00*4.51","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFLD072","PDF","720x720","LVDS","NV3051F-L","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A-RS232","PDF","720x720","RS232","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS485","PDF","720x720","RS485","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-TTL","PDF","720x720","TTL","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-CAN","PDF","720x720","CAN","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WXFPD014-C046B","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","82.80*82.80*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-a","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.3”","KD043WQFPA042","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-01-RT","PDF","480x272","RGB","SC7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA042-01-C037C","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-C038A","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","800 nits","115.40*79.15*4.80","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPD051-01-C050A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*4.25","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFLA096-02","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPD049-C038B","PDF","480x272","RGB","SC7283","Free V.A","CTP","-30℃~85℃","740 nits","115.40*79.15*4.63","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFPA051-02","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","1250 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","1000 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFPA051-02-C049A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","115.40*79.15*4.86","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-RT","PDF","800x480","LVDS","ST7262","Free V.A","RTP","-30℃~85℃","950 nits","105.40*67.15*4.01","95.04*53.86","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-02A-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","1100 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS232","PDF","480x272","RS232","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS485","PDF","480x272","RS485","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-TTL","PDF","480x272","TTL","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS232","PDF","800x480","RS232","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS485","PDF","800x480","RS485","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-TTL","PDF","800x480","TTL","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-CAN","PDF","480x272","CAN","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFMD134","PDF","480x272","MCU","NV3041A-01","Free V.A","No TP","-30℃~85℃","950 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-03","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","650 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142","PDF","480x272","RGB","ST7282A","Free V.A","No TP","-30℃~80℃","700 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA137","PDF","480x272","RGB","ILI6485","Free V.A","No TP","-30℃~80℃","600 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFPA051-05","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFPA051-05-C030A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WVFLA096","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFLA096-02A","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","1200 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WVFLA096-03","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","600 nits","105.40*67.15*2.91","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WVFLA096-03-C030A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","105.40*67.15*4.36","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFMD134-01-C037A","PDF","480x272","MCU","NV3041A-01","Free V.A","CTP","-30℃~85℃","900 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01","PDF","480x272","RGB","ST7283","Free V.A","No TP","-30℃~85℃","850 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-C037D","PDF","480x272","RGB","ST7283","Free V.A","CTP","-30℃~85℃","800 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQFPA124-01-RT","PDF","480x272","RGB","ST7283","Free V.A","RTP","-30℃~85℃","750 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA042-01","PDF","480x272","RGB","SC7283","Free V.A","No TP","-30℃~85℃","900 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT,High-brightness TFT"]
["4.3”","KD043WQTPA115","PDF","480x272","RGB","ST7282","V.A 12H","No TP","-30℃~85℃","500 nits","105.50*67.20*3.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQTPA115-01-RT","PDF","480x272","RGB","ST7282","V.A 12H","RTP","-30℃~85℃","400 nits","105.50*67.20*5.10","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQFPA142-01","PDF","480x272","RGB","ST7282A","Free V.A","No TP","-30℃~80℃","700 nits","105.40*67.15*2.85","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142-01-RT","PDF","480x272","RGB","ST7282A","Free V.A","RTP","-30℃~80℃","550 nits","105.40*67.15*4.05","95.04*53.86","Resistive Touch Display,Wide Temp TFT"]
["4.3”","KD043WQRPA140","PDF","480x272","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","650 nits","105.50*67.20*3.80","95.04*53.86","Wide Temp TFT"]
["4.3”","KD043WQFPA142-01-C037D","PDF","480x272","RGB","ST7282A","Free V.A","CTP","-30℃~80℃","650 nits","105.40*67.15*4.35","95.04*53.86","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-02-C045A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","700 nits","120.70*75.90*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","650 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA107","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","950 nits","118.50*77.80*3.85","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA107-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","760 nits","118.50*77.80*5.10","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA107-C104A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","900 nits","118.50*77.80*6.34","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109","PDF","480x272","RGB","ST7282","Free V.A","No TP","-30℃~85℃","1000 nits","120.16*75.36*2.53","110.88*62.83","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WQFPD109-C107A","PDF","480x272","RGB","ST7282","Free V.A","CTP","-30℃~85℃","900 nits","120.16*75.36*4.56","110.88*62.83","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA124A","PDF","800x480","RGB","TBD","Free V.A","No TP","-30℃~85℃","700 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050WVFPA029-06-C039A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-C040A","PDF","800x480","RGB","ST7262","Free V.A","CTP","-30℃~85℃","800 nits","120.70*75.90*4.48","108.00*64.80","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA029-06-RT","PDF","800x480","RGB","ST7262","Free V.A","RTP","-30℃~85℃","700 nits","120.70*75.90*4.15","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA029-06","PDF","800x480","RGB","ST7262","Free V.A","No TP","-30℃~85℃","850 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFLA033-01-C045A","PDF","800x480","LVDS","ST7262","Free V.A","CTP","-30℃~85℃","750 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFLA022","PDF","800x480","LVDS","HX8678C/HX8249A","Free V.A","No TP","-30℃~85℃","700 nits","124.90*78.10*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050WVFLA033","PDF","800x480","LVDS","ST7262","Free V.A","No TP","-30℃~85℃","800 nits","120.70*75.90*2.95","108.00*64.80","Wide Temp TFT,High-brightness TFT"]
["5.0”","KD050WVFPA018","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","No TP","-30℃~85℃","700 nits","124.90*78.10*2.95","108.00*64.80","Wide Temp TFT"]
["5.0”","KD050WVFPA018-C020A","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","CTP","-30℃~85℃","630 nits","124.90*78.10*4.38","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA018-RTP","PDF","800x480","RGB","HX8678C/HX8249A","Free V.A","RTP","-30℃~85℃","560 nits","124.90*78.10*4.05","108.00*64.80","Resistive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFLA146","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-01","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.16*75.36*2.70","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","900 nits","120.70*75.90*2.95","108.00*64.80","High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFLA146-02-C039A","PDF","800x480","LVDS","ST7265","Free V.A","No TP","-25℃~80℃","950 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-02-C045A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","850 nits","132.72*87.80*4.73","108.00*64.80","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C039A","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","132.72*87.80*4.90","108.00*64.80","Capacitive Touch Display,Wide Temp TFT"]
["5.0”","KD050WVFPA124A-03-C040C","PDF","800x480","RGB","ST7265","Free V.A","CTP","-25℃~80℃","650 nits","120.70*75.90*4.38","108.50*65.80","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA011-C004A","PDF","640x480","RGB","JD9186S","Free V.A","CTP","-30℃~80℃","550 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA011","PDF","640x480","RGB","JD9186S","Free V.A","No TP","-30℃~80℃","600 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","600 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015-RT","PDF","640x480","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","480 nits","126.50*100.00*7.40","115.20*86.40","Resistive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA015A","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA015A-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFLA012A","PDF","640x480","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFLA012A-C004A","PDF","640x480","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFIA014A","PDF","640x480","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","650 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFIA014A-C004A","PDF","640x480","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","600 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.7”","KD057VGFPA018","PDF","640x480","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","700 nits","126.50*100.00*5.70","115.20*86.40","Wide Temp TFT"]
["5.7”","KD057VGFPA018-C004A","PDF","640x480","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","650 nits","126.50*100.00*7.42","115.20*86.40","Capacitive Touch Display,Wide Temp TFT"]
["5.9”","KD059WVFPD001","PDF","840x512","RGB","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.16*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-C001A","PDF","840x512","RGB","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.16*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFPD001-RTP","PDF","840x512","RGB","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.16*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003","PDF","840x512","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFID003-C001A","PDF","840x512","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002","PDF","840x512","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","950 nits","133.66*86.83*5.53","127.76*77.88","Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-C001A","PDF","840x512","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","850 nits","134.16*87.33*7.63","127.76*77.88","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["5.9”","KD059WVFLD002-RTP","PDF","840x512","LVDS","JD9168S","Free V.A","RTP","-30℃~80℃","830 nits","134.16*87.08*7.23","127.76*77.88","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-C002A","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","800 nits","173.80*82.76*4.76","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-RTP","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","RTP","-30℃~85℃","750 nits","163.10*67.10*4.21","148.80*53.76","Resistive Touch Display,Wide Temp TFT"]
["6.2”","KD062VGFPD003","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.10*67.10*2.71","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.2”","KD062VGFPD003-C002A-TTL","PDF","640x240","TTL","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS485","PDF","640x240","RS485","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS232","PDF","640x240","RS232","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPA003-01","PDF","640x240","RGB","ST5043AA/ST5894AA","Free V.A","No TP","-30℃~85℃","900 nits","163.60*67.60*2.87","148.80*53.76","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPA007","PDF","800x480","RGB","TBD","Free V.A","No TP","-30℃~85℃","800 nits","156.10*100.91*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A","PDF","800x480","RGB","TBD","Free V.A","CTP","-30℃~85℃","800 nits","155.96*100.77*7.29","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPA001","PDF","800x480","RGB","ST72658","Free V.A","No TP","-30℃~85℃","800 nits","165.00*100.00*5.50","148.10*88.86","Wide Temp TFT,High-brightness TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS232","PDF","800x480","RS232","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS485","PDF","800x480","RS485","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-TTL","PDF","800x480","TTL","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-CAN","PDF","800x480","CAN","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA010-02","PDF","800x480","RGB","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","800 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","400 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT"]
["7.0”","KD070WVFPA065","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","600 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT"]
["7.0”","KD070WVFLA035","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLD070","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-30℃~85℃","1100 nits","166.90*108.65*7.40","152.45*91.47","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-C010A","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","350 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA011-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","300 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA065-C010A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","550 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA065-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","480 nits","165.40*104.59*7.00","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFPA043-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043-RT","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1100 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-C049A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035-RT","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","RTP","-30℃~85℃","1000 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLD070-C085A","PDF","1280x768","LVDS","HX8298-Ax3+HX8695Ex1","Free V.A","CTP","-30℃~85℃","980 nits","182.45*121.47*9.38","152.45*91.47","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVTPA088","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","No TP","-30℃~85℃","500 nits","165.00*100.00*5.80","154.08*85.92","Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-RT","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-C004A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.33","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTPA088-01-C101A","PDF","800x480","RGB","EK9713/EK73002","V.A 12H","CTP","-30℃~85℃","500 nits","182.07*117.60*8.15","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","No TP","-30℃~85℃","500 nits","165.00*100.00*5.80","154.08*85.92","Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-RT","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","RTP","-30℃~85℃","500 nits","165.00*100.00*7.30","154.08*85.92","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-C004A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","500 nits","165.00*100.00*7.40","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVTLA095-01-C101A","PDF","800x480","LVDS","EK9713+EK73002+THC63LVDF84C","V.A 12H","CTP","-30℃~85℃","450 nits","182.07*117.60*10.55","154.08*85.92","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLD092-C061D","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.62","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070HDFLD092-C113A","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","165.10*100.10*6.67","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099","PDF","800x480","RGB","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.10*100.10*5.10","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD099-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","900 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02-RT","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","850 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA011-02","PDF","800x480","LVDS","SC5004/SC5005","Free V.A","No TP","-30℃~85℃","1000 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA010-02-RTP","PDF","800x480","RGB","SC5004/SC5005","Free V.A","RTP","-30℃~85℃","640 nits","165.40*104.59*6.85","152.40*91.44","Resistive Touch Display,Wide Temp TFT"]
["7.0”","KD070HDFLD092-C050B","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","CTP","-30℃~85℃","1600 nits","182.07*117.60*7.22","154.21*85.92","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA010-02-C010A","PDF","800x480","RGB","SC5004/SC5005","Free V.A","CTP","-30℃~85℃","720 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT"]
["7.0”","KD070WVFLA125","PDF","800x480","LVDS","ST72568-G6-K","Free V.A","No TP","-30℃~85℃","950 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1300 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPA043A-C049A","PDF","800x480","RGB","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1150 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","No TP","-30℃~85℃","1100 nits","165.40*104.59*5.80","152.40*91.44","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFLA035A-C049C","PDF","800x480","LVDS","RM533CO+RM577C1","Free V.A","CTP","-30℃~85℃","1000 nits","165.40*104.59*7.73","152.40*91.44","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["7.0”","KD070WVFPA140","PDF","800x480","RGB","ST7277-G6-K","Free V.A","No TP","-30℃~85℃","1200 nits","165.00*100.00*5.80","153.84*85.63","Wide Temp TFT,High-brightness TFT"]
["7.0”","KD070WVFPD140-01-C114A","PDF","800x480","RGB","ST72568-G6-K","Free V.A","CTP","-30℃~85℃","1050 nits","165.10*100.10*6.65","153.84*85.63","Capacitive Touch Display,High-brightness TFT,Wide Temp TFT"]
["7.0”","KD070HDFLD092","PDF","1024x600","LVDS","EK73215&EK79001","Free V.A","No TP","-30℃~85℃","1600 nits","165.10*100.10*5.12","154.21*85.92","High-brightness TFT,Wide Temp TFT"]
["8.0”","KD080WUFLD027","PDF","1920x1200","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1500 nits","179.96*119.92*4.20","172.22*107.64","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080WVTPA029","PDF","800x480","RGB","TBD","V.A 6H","No TP","-30℃~80℃","900 nits","192.80*116.90*6.40","176.64*99.36","Wide Temp TFT,High-brightness TFT"]
["8.0”","KD080WQOIN035","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-C000-a","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["9.0”","KD090HWFLA004","PDF","1280x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1000 nits","210.70*124.15*6.20","198.91*111.89","Wide Temp TFT,High-brightness TFT"]
["9.8”","KD098WXTIA-001","PDF","1280x320","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1300 nits","252.75*73.17*11.00","241.15*60.29","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA010","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","252.70*175.55*6.44","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA010-C016A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","252.70*175.55*9.25","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101UXFLD009","PDF","1920x1200","LVDS","4*HX8255+2*HX8678","Free V.A","No TP","-30℃~80℃","400 nits","237.92*157.88*13.00","217.44*135.90","Wide Temp TFT"]
["10.1”","KD101HDFLA034-01","PDF","1280x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","650 nits","238.60*148.00*6.50","223.68*125.82","Wide Temp TFT"]
["10.1”","KD101WXFLD021","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","450 nits","229.06*148.70*2.56","216.96*135.60","Wide Temp TFT"]
["10.1”","KD101WXFLD021-01-C009B","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~85℃","590 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101WXFID045","PDF","1280x800","MIPI","EK79202DA","Free V.A","No TP","-30℃~85℃","550 nits","229.06*148.70*2.56","216.96*135.60","Wide Temp TFT"]
["10.1”","KD101WXFID045-C009B","PDF","1280x800","MIPI","EK79202D","Free V.A","CTP","-30℃~85℃","500 nits","244.45*173.88*4.76","216.96*135.60","Capacitive Touch Display,Wide Temp TFT"]
["10.1”","KD101HDFLD054","PDF","1280x800","LVDS","EK79202D","Free V.A","No TP","-30℃~85℃","1000 nits","228.60*149.10*4.38","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLD056A","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~80℃","1350 nits","228.80*147.90*4.66","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLD056A-C045E","PDF","1280x800","LVDS","EK79202D_A","Free V.A","CTP","-30℃~80℃","1250 nits","252.96*171.60*6.91","216.96*135.60","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.1”","KD101HDFLA059","PDF","1280x800","LVDS","EK79202D_A","Free V.A","No TP","-30℃~85℃","1300 nits","229.46*149.10*7.06","216.96*135.60","Wide Temp TFT,High-brightness TFT"]
["10.3”","KD103WUFLD001","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","258.60*107.00*6.37","243.65*91.37","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["10.4”","KD104XGFLA011","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","238.60*175.80*9.20","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104WVTLA008","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","900 nits","228.40*175.40*5.90","210.43*157.82","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD022","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1200 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA011-C009A","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1300 nits","266.13*221.29*12.54","210.43*157.82","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLA022-01","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1050 nits","225.80*174.35*5.92","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID025-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFLD027-C011A","PDF","1024x768","LVDS","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026","PDF","1024x768","MIPI","JD9168S","Free V.A","No TP","-30℃~80℃","1100 nits","225.90*174.40*5.55","211.20*158.40","Wide Temp TFT,High-brightness TFT"]
["10.4”","KD104XGFID026-C011A","PDF","1024x768","MIPI","JD9168S","Free V.A","CTP","-30℃~80℃","1050 nits","225.90*174.40*7.65","211.20*158.40","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFPA001","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~85℃","600 nits","260.50*204.00*8.80","245.76*184.32","Wide Temp TFT"]
["12.1”","KD121HDFPA001-C001B","PDF","1024x768","LVDS","TBD","Free V.A","CTP","-30℃~85℃","600 nits","281.80*220.70*11.20","245.76*184.32","Capacitive Touch Display,Wide Temp TFT"]
["12.1”","KD121HDFLA011","PDF","1280x800","LVDS","HX8245-J+HX8695-E","Free V.A","No TP","-30℃~80℃","400 nits","278.00*184.00*9.20","261.12*163.20","Wide Temp TFT"]
["12.1”","KD121HDFLA009","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","283.00*185.10*9.40","261.12*163.20","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA014","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~85℃","800 nits","260.50*204.00*8.60","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLD010-C008A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~80℃","1100 nits","306.50*196.20*14.50","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLD009-01-C006A","PDF","1280x800","LVDS","TBD","Free V.A","CTP","-30℃~85℃","1350 nits","306.50*196.20*15.42","261.12*163.20","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121XGFLD024","PDF","1024x768","LVDS","JD9168S","Free V.A","No TP","-30℃~85℃","1250 nits","260.49*203.45*6.88","245.76*184.32","Wide Temp TFT,High-brightness TFT"]
["12.1”","KD121HDFLA042","PDF","1280x800","LVDS","TBD","Free V.A","No TP","-30℃~85℃","400 nits","278.00*184.09*9.29","261.12*163.20","Wide Temp TFT"]
["12.3”","KD123WUFLA003","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","308.10*130.00*15.10","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD005","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.63*123.61*6.55","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD006","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.10*125.50*6.35","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLA002","PDF","1920x720","LVDS","HX8255A*4, HX8695H*1","Free V.A","No TP","-30℃~85℃","700 nits","312.90*132.20*13.20","292.03*109.51","Wide Temp TFT,Bartype TFT"]
["12.3”","KD123WUFLD006-C002A","PDF","1920x720","LVDS","TBD","Free V.A","CTP","-30℃~85℃","950 nits","311.02*132.60*9.15","292.03*109.51","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.8”","KD128FHFLD001","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~85℃","700 nits","294.40*175.01*6.50","283.39*159.41","Wide Temp TFT"]
["12.8”","KD128FHFLD001-01","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~70℃","1000 nits","294.40*175.00*5.00","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["12.8”","KD128FHFLA002","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-40℃~85℃","800 nits","321.46*181.08*13.29","283.39*159.41","Wide Temp TFT,High-brightness TFT"]
["12.8”","KD128FHFLD001-01-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-30℃~85℃","650 nits","294.40*175.00*26.20","283.39*159.41","Wide Temp TFT,HDMI TFT"]
["12.8”","KD128FHFLD001-01-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-30℃~85℃","550 nits","320.59*196.61*29.45","283.39*159.41","Capacitive Touch Display,Wide Temp TFT,HDMI TFT"]
["13.0”","KD130UXOEN001-C001A","PDF","2560x1440","eDP","RM98120","Free V.A","CTP","-40℃~85℃","800 nits","292.69*168.27*2.10","286.69*161.27","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["15.0”","KD150XGFLD002","PDF","1024x768","LVDS","TBD","Free V.A","No TP","-30℃~80℃","450 nits","326.50*253.50*9.00","304.10*228.10","Wide Temp TFT"]
["15.1”","KD151WQOEN001-C0000","PDF","2560x1600","eDP","RM98121","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*1.30","324.10*202.56","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["15.1”","KD151WQOEN001-SP001A-HDMI","PDF","2560x1600","HDMI","TBD","Free V.A","No TP","-40℃~85℃","550 nits","328.90*210.46*5.80","324.10*202.56","AMOLED Display,Wide Temp TFT,LTPS Display,HDMI AMOLED"]
["15.6”","KD156FHFLA012","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1300 nits","363.80*215.90*9.30","344.16*193.59","Wide Temp TFT,High-brightness TFT"]
["17.0”","KD170SXTLA003","PDF","1280x1024","LVDS","TBD","V.A 6H","No TP","-30℃~85℃","1400 nits","358.50*296.50*10.50","337.92*270.34","Wide Temp TFT,High-brightness TFT"]
["18.5”","KD185FHFLA003","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","350 nits","430.40*254.60*12.00","408.96*230.04","Wide Temp TFT"]
["18.5”","KD185FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1000 nits","430.40*254.60*12.00","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["18.5”","KD185FHFLA010","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-30℃~80℃","1500 nits","430.37*254.60*11.50","408.96*230.04","High-brightness TFT,Wide Temp TFT"]
["19.0”","KD190SXTLA004","PDF","1280x1024","LVDS","TBD","Free V.A","No TP","-30℃~85℃","450 nits","396.00*324.00*12.88","376.32*301.06","Wide Temp TFT"]
["21.5”","KD215FHFLA022","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~85℃","1000 nits","495.60*292.20*10.50","476.64*268.11","Wide Temp TFT,High-brightness TFT"]
["21.5”","KD215FHFLA026","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~80℃","400 nits","495.60*292.40*10.50","476.64*268.11","Wide Temp TFT"]
["21.5”","KD215FHFLA026-C005B","PDF","1920x1080","LVDS","TBD","Free V.A","CTP","-20℃~80℃","400 nits","505.60*302.20*13.90","476.64*268.11","Capacitive Touch Display,Wide Temp TFT"]

{"sheet":"Square TFT","index":5,"n_rows":61,"n_cols":13,"rows_kept":61}
["STARTEK Square TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.3”","KD013QVFMD010","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","550 nits","26.16*29.22*1.79","23.40*23.40","Square TFT"]
["1.3”","KD013QVFMD010A","PDF","240x240","SPI&MCU&RGB","ST7789T3-G4-1","Free V.A","No TP","-20℃~70℃","550 nits","26.16*29.22*1.79","23.40*23.40","Square TFT"]
["1.44”","KD014QQTBN002","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","No TP","-20℃~70℃","800 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.44”","KD014QQTBN002-TP","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","RTP","-20℃~70℃","640 nits","32.36*38.00*4.20","25.50*26.50","Resistive Touch Display,Square TFT"]
["1.44”","KD014QQFBN006","PDF","128x128","SPI&MCU","ST7735S","Free V.A","No TP","-20℃~70℃","950 nits","32.36*38.00*3.00","25.50*26.50","High-brightness TFT,Square TFT"]
["1.44”","KD014QQTBN001-01","PDF","128x128","SPI&MCU","ST7735S","V.A 6H","No TP","-20℃~70℃","200 nits","32.36*38.00*2.60","25.50*26.50","Square TFT"]
["1.5”","KD015QVFMN002-C001B","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","320 nits","37.52*41.10*4.45","27.72*27.72","Capacitive Touch Display,Square TFT"]
["1.5”","KD015QVFMN002","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","33.32*36.06*2.25","27.72*27.72","Square TFT"]
["1.5”","KD015QVFMD020-C001D","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","800 nits","37.52*41.10*3.82","27.72*27.72","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["1.54”","KD015QVFSN012","PDF","152x152","SPI","SSD1681","Free V.A","No TP","0℃~50℃","0 nit","31.80*37.32*1.14","27.51*27.51","Square TFT,E-Paper Display"]
["1.54”","KD015QVFSN015","PDF","200x200","SPI","SSD1681","Free V.A","No TP","0℃~40℃","0 nit","31.80*37.32*1.00","27.00*27.00","Square TFT,E-Paper Display"]
["2.1”","KD021WVOSN009-C003B","PDF","480x480","QSPI","CO5300AF","Free V.A","CTP","-20℃~60℃","600 nits","42.39*42.39*2.55","38.39*38.39","Capacitive Touch Display,AMOLED Display,Square TFT,LTPS Display"]
["2.7”","KD027HVFMD010","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFMD010-C004A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-30℃~85℃","900 nits","53.40*59.90*2.29","48.96*48.96","Wide Temp TFT,High-brightness TFT,Square TFT"]
["2.7”","KD027HVFID009-C004A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-30℃~85℃","800 nits","63.40*69.90*3.77","48.96*48.96","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","65.72*69.64*2.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","65.72*69.64*4.13","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFID001-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","No TP","-30℃~70℃","950 nits","65.72*69.64*14.00","60.48*60.48","High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFID001-C001A-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*16.00","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFLD005","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*4.45","60.48*60.48","High-brightness TFT,Square TFT"]
["3.4”","KD034WXFLD005-C001A","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-20℃~70℃","800 nits","65.72*69.64*6.34","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["3.4”","KD034WXFPD002-RS232","PDF","480x480","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-RS485","PDF","480x480","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-TTL","PDF","480x480","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.5”","KD035VGFID162-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","No TP","-20℃~70℃","740 nits","74.38*62.35*14.00","70.08*52.56","Square TFT,Type-C TFT"]
["4.0”","KD040WXFID017","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-01-RTP","PDF","480x480","RGB","ST7701S","Free V.A","RTP","-30℃~85℃","800 nits","77.00*80.00*3.50","71.86*70.18","Resistive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFID017-C015A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-30℃~85℃","950 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-C015C","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","850 nits","77.00*80.00*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFID032","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID032-C026C","PDF","720x720","MIPI","ST7703","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*3.76","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFID035","PDF","720x720","MIPI","ST7703","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A","PDF","720x720","SPI+RGB","NV3052CGRB","Free V.A","CTP","-30℃~80℃","650 nits","84.00*85.99*4.23","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT"]
["4.0”","KD040WXFLD071","PDF","480x480","LVDS","ST7701S","Free V.A","No TP","-30℃~85℃","950 nits","77.00*80.00*2.35","71.86*70.18","Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFLD071-C015C","PDF","480x480","LVDS","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","77.00*80.00*4.51","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFID032-C026C-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","CTP","-20℃~70℃","650 nits","84.00*85.99*15.50","71.93*71.93","Capacitive Touch Display,Square TFT,Type-C TFT"]
["4.0”","KD040HDFID032-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","No TP","-20℃~70℃","700 nits","77.00*80.00*14.00","71.93*71.93","Square TFT,Type-C TFT"]
["4.0”","KD040WXFID017-C015C-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","77.00*80.00*16.00","71.86*70.18","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["4.0”","KD040HDFLD072","PDF","720x720","LVDS","NV3051F-L","Free V.A","No TP","-30℃~80℃","700 nits","77.00*80.00*2.60","71.93*71.93","Wide Temp TFT,Square TFT"]
["4.0”","KD040HVFID080","PDF","320x320","MIPI","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFID080-C050A","PDF","320x320","MIPI","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","No TP","-20℃~70℃","950 nits","77.00*80.00*2.46","71.14*69.82","High-brightness TFT,Square TFT"]
["4.0”","KD040HVFMD081-C050A","PDF","320x320","SPI&MCU&RGB","ST7796","Free V.A","CTP","-20℃~70℃","900 nits","77.00*80.00*4.49","71.14*69.82","Capacitive Touch Display,High-brightness TFT,Square TFT"]
["4.0”","KD040HDFPD039-C026A-RS232","PDF","720x720","RS232","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS485","PDF","720x720","RS485","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-TTL","PDF","720x720","TTL","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-CAN","PDF","720x720","CAN","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WXFPD014-C046B","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-30℃~85℃","900 nits","82.80*82.80*4.35","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]
["4.0”","KD040WXFPD014-a","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","1000 nits","77.00*80.00*2.30","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Square TFT"]

{"sheet":"Round TFT","index":6,"n_rows":38,"n_cols":13,"rows_kept":38}
["STARTEK Round TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.0”","KD010LQOSN001-C0000","PDF","340x340","QSPI","SH8601","Free V.A","CTP","-10℃~60℃","630 nits","29.25*30.00*0.68","26.35*26.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.3”","KD013QVFMD002-01","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","450 nits","35.90*39.70*1.39","32.40*32.40","Round TFT"]
["1.3”","KD013QVFMD007A","PDF","240x240","SPI&MCU&RGB","GC9A01","Free V.A","No TP","-20℃~70℃","500 nits","35.60*37.74*1.48","32.40*32.40","Round TFT"]
["1.3”","KD013QVFMD002-03","PDF","240x240","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","450 nits","35.90*39.70*1.39","32.40*32.40","Round TFT"]
["1.4”","KD014VGOSN001-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","650 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.6”","KD016WVFID001","PDF","400x400","MIPI","ST7797","Free V.A","No TP","-20℃~70℃","350 nits","42.94*45.89*1.94","39.84*39.84","Round TFT"]
["1.6”","KD016WVFID001-C002A","PDF","400x400","MIPI","ST7797","Free V.A","CTP","-20℃~70℃","350 nits","51.94*52.94*3.09","39.84*39.84","Capacitive Touch Display,Round TFT"]
["1.8”","KD018HVFMD042","PDF","360x360","MCU/SPI/QSPI","ST77916","Free V.A","No TP","-20℃~70℃","800 nits","48.08*49.95*1.94","45.68*45.68","High-brightness TFT,Round TFT"]
["2.1”","KD021WVFID002-C001A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFPD003-C001A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.1”","KD021WVFID002","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021WVFPD003","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021WVFPD003-02","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1000 nits","56.18*59.71*2.24","53.28*53.28","High-brightness TFT,Round TFT"]
["2.1”","KD021WVFPD011","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","650 nits","56.18*59.71*2.24","53.28*53.28","Round TFT"]
["2.1”","KD021WVFPD011-C001A","PDF","480x480","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","600 nits","70.61*72.61*3.39","53.28*53.28","Capacitive Touch Display,Round TFT"]
["2.47”","KD024HVFID076","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-10℃~60℃","430 nits","69.19*71.74*2.50","62.64*62.64","Round TFT"]
["2.47”","KD024HVFPD088","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-30℃~70℃","480 nits","69.19*71.74*2.50","62.64*62.64","Round TFT"]
["2.8”","KD028WXFPD057","PDF","480x480","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","73.03*76.48*2.24","70.13*70.13","Round TFT"]
["2.8”","KD028WXFID056","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","73.03*76.48*2.24","70.13*70.13","Round TFT"]
["2.8”","KD028WXFPD057-C040A","PDF","480x480","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028WXFID056-C040A","PDF","480x480","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","87.73*89.73*3.39","70.13*70.13","Capacitive Touch Display,Round TFT"]
["2.8”","KD028WXFID076","PDF","480x480","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["2.8”","KD028WXFPD075","PDF","480x480","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","1700 nits","75.00*78.26*5.90","70.13*70.13","High-brightness TFT,Round TFT"]
["3.4”","KD034WVFID003","PDF","800x800","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","430 nits","94.90*96.95*2.18","87.60*87.60","Round TFT"]
["3.4”","KD034WVFLD004","PDF","800x800","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","420 nits","94.90*96.95*2.18","87.60*87.60","Round TFT"]
["3.4”","KD034WVFID003-SP001A-HDMI","PDF","800x800","HDMI","ILI9881C","Free V.A","No TP","-20℃~70℃","600 nits","94.89*96.95*17.08","87.60*87.60","Round TFT,HDMI TFT"]
["3.4”","KD034WVFID003-C008A","PDF","800x800","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","111.20*113.20*3.41","87.60*87.60","Capacitive Touch Display,Round TFT"]
["3.6”","KD036AUFPA002","PDF","544x506","RGB","ST72566","Free V.A","No TP","-35℃~85℃","900 nits","99.88*94.12*7.71","89.76*83.49","Wide Temp TFT,High-brightness TFT,Round TFT"]
["4.0”","KD040HDFID088","PDF","720x720","MIPI","ILI9881C","Free V.A","No TP","-20℃~70℃","900 nits","105.60*109.87*2.16","101.52*101.52","High-brightness TFT,Round TFT"]
["4.0”","KD040HDFID088-C054A","PDF","720x720","MIPI","ILI9881C","Free V.A","CTP","-20℃~70℃","800 nits","125.29*127.29*3.41","101.52*101.52","Capacitive Touch Display,High-brightness TFT,Round TFT"]
["5.0”","KD050SXFID039","PDF","1080x1080","MIPI","HX8399","Free V.A","No TP","-20℃~60℃","300 nits","136.53*132.21*1.98","127.01*127.01","Round TFT"]
["5.0”","KD050SXFID039-C045A","PDF","1080x1080","MIPI","HX8399","Free V.A","CTP","-20℃~60℃","270 nits","208.00*208.00*4.16","127.01*127.01","Capacitive Touch Display,Round TFT"]
["23.6”","KD236SXFLA003","PDF","1280x1280","LVDS","TBD","Free V.A","No TP","-20℃~80℃","1500 nits","657.00*657.00*28.65","599.42*599.42","High-brightness TFT,Round TFT"]

{"sheet":"Bartype TFT","index":7,"n_rows":78,"n_cols":13,"rows_kept":78}
["STARTEK Bartype TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.91”","KD0091SQOIN001","PDF","128x32","i2C","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","38.00*12.00*3.80","22.38*5.58","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["0.95”","KD0095OLEDN010","PDF","120x240","SPI","RM69310","Free V.A","No TP","-20℃~70℃","450 nits","12.80*27.35*0.74","10.80*21.60","AMOLED Display,Bartype TFT,LTPS Display"]
["0.96”","KD0096SHFSD006-02","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["0.96”","KD0096SHFSD006-a","PDF","80x160","SPI","ST7735S","Free V.A","No TP","-20℃~70℃","1200 nits","13.50*27.95*1.50","10.80*21.70","High-brightness TFT,Bartype TFT"]
["1.7”","KD017SQOIN003","PDF","128x32","i2C","SSD1312","Free V.A","No TP","-40℃~70℃","120 nits","60.50*18.75*4.95","42.22*10.54","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.1”","KD021SCOIN007","PDF","256x64","i2C","SH1122","Free V.A","No TP","-40℃~70℃","150 nits","72.50*27.24*5.10","51.18*12.78","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.2”","KD022SQOSN037","PDF","128x32","SPI/IIC","SSD1305","Free V.A","No TP","-40℃~70℃","120 nits","74.00*30.00*8.20","55.02*13.10","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.9”","KD029QHFID001","PDF","376x960","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","31.20*76.60*2.13","26.51*67.68","Bartype TFT"]
["2.9”","KD029QHFPD002","PDF","376x960","RGB","ST7701S","Free V.A","No TP","-20℃~70℃","550 nits","31.20*76.60*2.13","26.51*67.68","Bartype TFT"]
["2.9”","KD029QHFPD002-C001A","PDF","376x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFID001-C004A","PDF","376x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["2.9”","KD029QHFPD002-C004A","PDF","376x960","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030WVFID029","PDF","268x800","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","400 nits","26.96*80.08*1.66","24.12*72.00","Bartype TFT"]
["3.0”","KD030WVFID029-C028A","PDF","268x800","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.0”","KD030WVFPD030","PDF","268x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","26.96*80.08*1.66","24.12*72.00","Bartype TFT"]
["3.0”","KD030WVFPD030-C028A","PDF","268x800","SPI+RGB","ST7701S","Free V.A","CTP","-20℃~70℃","650 nits","36.96*90.08*2.79","24.12*72.00","Capacitive Touch Display,Bartype TFT"]
["3.5”","KD035WVFPD107","PDF","340x800","SPI+RGB","ST7701S","Free V.A","No TP","-20℃~70℃","400 nits","37.27*89.00*1.60","33.97*81.00","Bartype TFT"]
["3.9”","KD39QWQ01HS","PDF","480x128","RGB","ILI6480","V.A 12H","No TP","-20℃~70℃","500 nits","105.50*40.64*2.95","95.04*25.34","Bartype TFT"]
["3.9”","KD039WQFPN002","PDF","480x128","RGB","ST7282","Free V.A","No TP","-20℃~70℃","2000 nits","102.46*34.40*3.58","95.04*25.34","High-brightness TFT,Bartype TFT"]
["3.9”","KD039WQFPN002-C001A","PDF","480x128","RGB","ST7282","Free V.A","CTP","-30℃~85℃","1900 nits","112.46*44.40*5.61","95.04*25.34","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["4.0”","KD040QHFID049","PDF","400x960","MIPI","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","42.50*102.08*2.02","39.18*94.03","Bartype TFT"]
["4.0”","KD040QHFPD047","PDF","400x960","RGB","ST7701S","Free V.A","No TP","-30℃~85℃","500 nits","42.50*102.08*2.02","39.18*94.03","Wide Temp TFT,Bartype TFT"]
["4.0”","KD040QHFID049-C039A","PDF","400x960","MIPI","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["4.0”","KD040QHFPD047-C039A","PDF","400x960","RGB","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*3.55","39.18*94.03","Capacitive Touch Display,Bartype TFT"]
["6.2”","KD062VGFPA003-01-SP001A-HDMI","PDF","640x240","HDMI","ST5043AA/ST5894AA","Free V.A","No TP","-20℃~70℃","900 nits","163.60*67.60*17.77","148.80*53.76","High-brightness TFT,Bartype TFT,HDMI TFT"]
["6.8”","KD068HDFLD004","PDF","480x1280","LVDS","NV3051F-L","Free V.A","No TP","-20℃~70℃","1650 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005","PDF","480x1280","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","2350 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID005-C001A","PDF","480x1280","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","2250 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFLD004-C001A","PDF","480x1280","LVDS","NV3051F-L","Free V.A","CTP","-20℃~70℃","1450 nits","78.02*191.10*6.34","60.19*160.51","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFPD011","PDF","480x1280","RGB","GC9704","Free V.A","No TP","-20℃~70℃","2000 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009","PDF","480x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","2100 nits","66.50*180.80*4.59","60.19*160.51","High-brightness TFT,Bartype TFT"]
["6.8”","KD068HDFID009-C009A","PDF","480x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","2000 nits","78.20*191.10*6.42","60.19*160.51","High-brightness TFT,Bartype TFT"]
["7.0”","KD070WXFID094","PDF","280x1424","MIPI","OTA7290N","Free V.A","No TP","-20℃~70℃","650 nits","38.20*181.47*3.40","33.60*170.88","Bartype TFT"]
["7.0”","KD070WXFID094-C074A","PDF","280x1424","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","600 nits","50.20*193.47*5.20","33.60*170.88","Capacitive Touch Display,Bartype TFT"]
["7.0”","KD070WXFID094-CP001A-HDMI","PDF","280x1424","HDMI","OTA7290N","Free V.A","No TP","-20℃~70℃","900 nits","38.20*181.47*3.44","33.60*170.88","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078HDFID004","PDF","400x1280","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","1100 nits","67.60*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002","PDF","400x1280","RGB","GC9704C","Free V.A","No TP","-20℃~70℃","1000 nits","67.90*206.28*4.44","59.40*190.08","High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFID006","PDF","400x1280","MIPI","OTA7290B","Free V.A","No TP","-20℃~70℃","480 nits","67.80*205.78*4.60","59.40*190.08","Bartype TFT"]
["7.84”","KD078HDFID004-C004A","PDF","400x1280","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","950 nits","67.60*206.28*6.27","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["7.84”","KD078HDFPD002-C003A-RS232","PDF","400x1280","RS232","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS485","PDF","400x1280","RS485","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-TTL","PDF","400x1280","TTL","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFID004-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","No TP","-20℃~70℃","800 nits","67.60*206.28*19.29","59.40*190.08","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078HDFID004-C004A-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","CTP","-20℃~70℃","800 nits","67.60*206.28*21.12","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["8.0”","KD080FM-8","PDF","1600x480","LVDS","HX8249/HX8678","Free V.A","No TP","-20℃~70℃","500 nits","208.00*73.00*5.50","194.40*58.32","Bartype TFT"]
["8.0”","KD080FM-8-C008A","PDF","1600x480","LVDS","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","420 nits","249.20*87.00*6.86","194.40*58.32","Capacitive Touch Display,Bartype TFT"]
["8.6”","KD086UXFLD001","PDF","600x1600","LVDS","GC9704","Free V.A","No TP","-20℃~70℃","350 nits","82.18*212.85*2.57","76.36*203.62","Bartype TFT"]
["8.6”","KD086UXFLD001-C001A","PDF","600x1600","LVDS","GC9704","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.6”","KD086UXFID002","PDF","600x1600","MIPI","GC9703C","Free V.A","No TP","-20℃~70℃","350 nits","82.18*212.85*2.57","76.36*203.62","Bartype TFT"]
["8.6”","KD086UXFID002-C001A","PDF","600x1600","MIPI","GC9703C","Free V.A","CTP","-20℃~70℃","300 nits","92.18*222.85*4.30","76.36*203.62","Capacitive Touch Display,Bartype TFT"]
["8.9”","KD089FHFID004","PDF","480x1920","MIPI","OTA7290N","Free V.A","No TP","-20℃~70℃","950 nits","64.10*231.20*4.73","54.72*218.88","High-brightness TFT,Bartype TFT"]
["8.9”","KD089FHFID004-C001A","PDF","480x1920","MIPI","OTA7290N","Free V.A","CTP","-20℃~70℃","850 nits","76.00*243.10*6.75","54.72*218.88","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["10.1”","KD101FHFIA026","PDF","440x1920","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","750 nits","64.98*266.44*4.60","57.95*252.86","Bartype TFT"]
["10.1”","KD101FHFID031","PDF","440x1920","MIPI","ICNL9707","Free V.A","No TP","-20℃~70℃","1000 nits","65.08*266.19*4.48","57.95*252.86","High-brightness TFT,Bartype TFT"]
["10.1”","KD101FHFID031-C037A","PDF","440x1920","MIPI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*6.23","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["10.1”","KD101FHFID031-C037A-CP001A-HDMI","PDF","440x1920","HDMI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*12.29","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["10.3”","KD103WUFLD001","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","1100 nits","258.60*107.00*6.37","243.65*91.37","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["10.4”","KD104WSTPA003","PDF","1024x100","RGB","HX8282，HX8678","V.A 12H","No TP","-20℃~70℃","1000 nits","288.92*41.50*6.89","264.19*25.80","High-brightness TFT,Bartype TFT"]
["10.4”","KD104WSTPA-001","PDF","1024x100","RGB","HX8282-A*1, HX8678-C*1","V.A 12H","No TP","0℃~50℃","450 nits","288.92*41.50*7.12","264.19*25.80","Bartype TFT"]
["12.3”","KD123WUFLA003","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","308.10*130.00*15.10","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD005","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.63*123.61*6.55","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLD006","PDF","1920x720","LVDS","TBD","Free V.A","No TP","-30℃~85℃","850 nits","302.10*125.50*6.35","292.03*109.51","Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["12.3”","KD123WUFLA002","PDF","1920x720","LVDS","HX8255A*4, HX8695H*1","Free V.A","No TP","-30℃~85℃","700 nits","312.90*132.20*13.20","292.03*109.51","Wide Temp TFT,Bartype TFT"]
["12.3”","KD123WUFLD006-C002A","PDF","1920x720","LVDS","TBD","Free V.A","CTP","-30℃~85℃","950 nits","311.02*132.60*9.15","292.03*109.51","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,Bartype TFT"]
["13.5”","KD135HDFLA001","PDF","1280x235","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","360.00*83.00*15.90","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.5”","KD135HDFLA001-C001A","PDF","1280x235","LVDS","TBD","Free V.A","CTP","0℃~50℃","800 nits","380.00*106.00*18.95","337.92*62.04","High-brightness TFT,Bartype TFT"]
["13.9”","KD139HDFLD001","PDF","1280x400","LVDS","HX8249/HX8678","Free V.A","No TP","0℃~50℃","1400 nits","358.50*135.00*13.30","337.92*105.14","High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA007","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1200 nits","403.30*98.10*11.00","374.78*70.86","High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA007-C006B","PDF","1280x242","LVDS","TBD","Free V.A","CTP","0℃~50℃","950 nits","423.30*118.10*14.20","374.78*71.10","Capacitive Touch Display,High-brightness TFT,Bartype TFT"]
["15.0”","KD150HDFLA008","PDF","1280x242","LVDS","TBD","Free V.A","No TP","0℃~50℃","1000 nits","403.30*98.10*14.00","374.79*70.86","High-brightness TFT,Bartype TFT"]
["16.7”","KD167FHFLA001","PDF","1920x540","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1200 nits","439.00*144.00*14.00","408.96*115.02","High-brightness TFT,Bartype TFT"]
["20.8”","KD208FHFLA001","PDF","1920x184","LVDS","TBD","Free V.A","No TP","0℃~50℃","500 nits","592.00*75.00*12.30","527.04*50.60","Bartype TFT"]
["28.0”","KD280FM-1","PDF","1920x360","LVDS","TBD","Free V.A","No TP","0℃~50℃","700 nits","729.30*167.30*19.20","698.40*130.95","Bartype TFT"]
["28.0”","KD280FHFLA001","PDF","1920x360","LVDS","TBD","Free V.A","No TP","0℃~50℃","700 nits","732.00*165.00*16.80","699.84*131.22","Bartype TFT"]

{"sheet":"Transflective TFT","index":8,"n_rows":33,"n_cols":13,"rows_kept":33}
["STARTEK Transflective TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.75”","KD018LQRMN029","PDF","296x222","MCU","ILI9342C","Free V.A","No TP","-20℃~70℃","350 nits","42.07*39.71*2.50","35.52*26.64","Transflective TFT"]
["1.75”","KD018LQRBD028","PDF","296x222","MCU","ILI9342C","Free V.A","No TP","-20℃~70℃","320 nits","40.80*36.20*2.26","35.52*26.64","Transflective TFT"]
["2.0”","KD020QVRMA028","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","260 nits","35.80*52.10*2.65","30.60*40.80","Transflective TFT"]
["2.0”","KD020LQRMA017","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","No TP","-20℃~70℃","350 nits","46.50*41.56*2.70","40.80*30.60","Transflective TFT"]
["2.0”","KD020LQRMA017-RT","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","RTP","-20℃~70℃","280 nits","46.50*41.56*3.90","40.80*30.60","Resistive Touch Display,Transflective TFT"]
["2.0”","KD020LQRMA017-C003A","PDF","320x240","SPI&MCU&RGB","ILI9342C","Free V.A","CTP","-20℃~70℃","300 nits","54.50*47.56*4.35","40.80*30.60","Capacitive Touch Display,Transflective TFT"]
["2.0”","KD020QVRMA028-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","200 nits","35.80*52.10*3.85","30.60*40.80","Resistive Touch Display,Transflective TFT"]
["2.4”","KD024QVRBA050","PDF","240x320","MCU","ST7789V","Free V.A","No TP","-20℃~70℃","170 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA041A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","300 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA041A-C012A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","300 nits","42.92*60.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024QVRMA041A-RT","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","RTP","-20℃~70℃","290 nits","42.92*60.26*3.55","36.72*48.96","Resistive Touch Display,Transflective TFT"]
["2.4”","KD024QVRMD137","PDF","240x320","SPI&MCU&RGB","ST7789T3-G4-1","V.A 6H","No TP","-20℃~70℃","250 nits","42.72*60.26*2.63","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA038A-C015A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","CTP","-20℃~70℃","220 nits","48.72*70.26*4.20","36.72*48.96","Capacitive Touch Display,Transflective TFT"]
["2.4”","KD024QVRMA138","PDF","240x320","SPI&MCU&RGB","ST7789T3-G4-1","V.A 3H","No TP","-20℃~70℃","350 nits","42.92*60.26*2.46","36.72*48.96","Transflective TFT"]
["2.4”","KD024QVRMA038A","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-20℃~70℃","250 nits","42.92*60.26*2.45","36.72*48.96","Transflective TFT"]
["2.6”","KD026HVRMA010-TP","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","RTP","-30℃~85℃","430 nits","46.76*65.85*3.91","39.84*53.78","Resistive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRIA009","PDF","320x432","MIPI","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRMA010","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","No TP","-30℃~85℃","500 nits","46.76*65.85*2.60","39.84*53.78","Wide Temp TFT,Transflective TFT"]
["2.6”","KD026HVRMA010-C004B","PDF","320x432","SPI&MCU&RGB","ILI9488","Free V.A","CTP","-30℃~85℃","420 nits","46.76*65.85*4.26","39.84*53.78","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["2.8”","KD028WQRMD039-01","PDF","240x400","SPI&MCU&RGB","ILI9327","V.A 5H","No TP","-20℃~70℃","120 nits","44.00*72.50*2.54","36.72*61.20","Transflective TFT"]
["2.8”","KD028QVRMD073","PDF","240x320","SPI&MCU&RGB","ST7789V","Free V.A","No TP","-30℃~80℃","160 nits","50.50*69.70*2.50","43.20*57.60","Wide Temp TFT,Transflective TFT"]
["2.8”","KD028QVRMD073-C050A","PDF","240x320","SPI&MCU&RGB","ST7789V2","Free V.A","CTP","-30℃~80℃","150 nits","52.90*79.30*3.95","43.20*57.60","Capacitive Touch Display,Wide Temp TFT,Transflective TFT"]
["3.5”","KD035QVRMA223","PDF","240x320","SPI&MCU&RGB","ILI9341","V.A 6H","No TP","-20℃~70℃","120 nits","60.00*82.90*2.78","53.64*71.52","Transflective TFT"]
["3.5”","KD035QVRMD223-C102A","PDF","240x320","SPI&MCU&RGB","ILI9341","V.A 6H","CTP","-20℃~70℃","120 nits","66.24*87.12*6.16","53.64*71.52","Capacitive Touch Display,Transflective TFT"]
["3.5”","KD035HVRPD288","PDF","320x480","SPI&MCU","ST7365","TBD","No TP","-20℃~70℃","150 nits","52.26*80.60*2.21","48.96*75.60","Transflective TFT"]
["4.0”","KD040WVTPD090","PDF","480x800","RGB","ST7701SI","V.A 6H","No TP","-20℃~70℃","150 nits","57.14*96.85*2.60","51.84*86.40","Transflective TFT"]
["4.0”","KD040WVTPD090-C008B","PDF","480x800","RGB","ST7701SI","V.A 6H","CTP","-10℃~60℃","150 nits","57.86*97.70*4.08","51.84*86.40","Capacitive Touch Display,Transflective TFT"]
["5.0”","KD050WVRPA092","PDF","800x480","RGB","HX8264+HX8664","V.A 12H","No TP","-20℃~70℃","180 nits","120.70*75.90*2.96","108.00*64.80","Transflective TFT"]
["5.0”","KD050WVRPD092-03-C045A","PDF","800x480","RGB","HX8264+HX8664","V.A 12H","CTP","-20℃~70℃","150 nits","132.72*87.80*4.99","108.00*64.80","Capacitive Touch Display,Transflective TFT"]

{"sheet":"Reflective TFT","index":9,"n_rows":5,"n_cols":13,"rows_kept":5}
["STARTEK Reflective TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["10.0”","KD100UXFIN002","PDF","1200x1600","MIPI","HX8279","Free V.A","No TP","-20℃~70℃","0 nit","157.86*211.88*0.72","152.46*203.28","Reflective TFT"]

{"sheet":"Blanview TFT","index":10,"n_rows":8,"n_cols":13,"rows_kept":8}
["STARTEK Blanview TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["3.5”","KD035VGFPA094","PDF","480x640","RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*3.10","53.28*71.04","Blanview TFT"]
["3.5”","KD035VGFPD094-01-C055A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","570 nits","69.96*92.96*4.93","53.28*71.04","Capacitive Touch Display,Blanview TFT"]
["3.5”","KD035VGFPA094-02","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","No TP","-20℃~70℃","1550 nits","64.00*85.00*3.10","53.28*71.04","High-brightness TFT,Blanview TFT"]
["3.5”","KD035VGFPA094-02-C041A","PDF","480x640","SPI+RGB","ILI9806E","Free V.A","CTP","-20℃~70℃","1300 nits","64.00*85.00*4.75","53.28*71.04","Capacitive Touch Display,High-brightness TFT,Blanview TFT"]

{"sheet":"Flexible AM-OLED Display","index":11,"n_rows":12,"n_cols":13,"rows_kept":12}
["STARTEK Flexible AM-OLED Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["6.5”","KD065FPOIN003","PDF","1080x2400","MIPI","RM692E5","Free V.A","No TP","-20℃~70℃","500 nits","71.45*156.64*0.29","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.5”","KD065FPOIN003-HDMI","PDF","1080x2400","HDMI","TBD","Free V.A","No TP","-20℃~70℃","450 nits","71.45*156.64*11.00","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["6.67”","KD067FPOIN004-C0000","PDF","1080x2400","MIPI","VTDR6130","Free V.A","CTP","-20℃~70℃","500 nits","71.53*200.59*0.33","69.55*154.56","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display"]
["8.0”","KD080WQOIN035","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-C000-a","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["13.3”","KD133QXFEN020","PDF","1536x2048","eDP","TBD","Free V.A","No TP","0℃~50℃","300 nits","213.80*284.80*0.53","202.75*270.34","AMOLED Display,Flexible AMOLED,LTPS Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]

{"sheet":"AM-OLED Display","index":12,"n_rows":68,"n_cols":13,"rows_kept":68}
["STARTEK AM-OLED Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.95”","KD0095OLEDN010","PDF","120x240","SPI","RM69310","Free V.A","No TP","-20℃~70℃","450 nits","12.80*27.35*0.74","10.80*21.60","AMOLED Display,Bartype TFT,LTPS Display"]
["1.0”","KD010LQOSN001-C0000","PDF","340x340","QSPI","SH8601","Free V.A","CTP","-10℃~60℃","630 nits","29.25*30.00*0.68","26.35*26.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN001-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","650 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.4”","KD014HVOIN011-C0000","PDF","320x360","MIPI","FT2390","Free V.A","CTP","-20℃~60℃","450 nits","25.74*29.87*0.79","23.84*26.82","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016HVOMN002-C001A","PDF","320x360","MIPI&SPI","RM69092","Free V.A","CTP","-20℃~70℃","320 nits","31.32*36.05*2.05","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016HVOQN006-C000O","PDF","320x360","QSPI","RM69092","Free V.A","CTP","-20℃~70℃","450 nits","28.92*33.35*0.76","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.78”","KD017HVOSN005-C000","PDF","368x448","QSPI/SPI","CO5300","Free V.A","CTP","-20℃~60℃","450 nits","33.50*40.89*2.58","28.70*34.94","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.96”","KD019HVOSN001-C001A","PDF","410x502","QSPI","CO5300AF-46","Free V.A","CTP","-10℃~60℃","600 nits","35.37*42.40*2.76","31.37*38.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","34.79*43.14*0.78","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001-C001A","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","36.70*44.21*2.55","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002-C002B","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","550 nits","37.35*45.15*2.31","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","600 nits","34.79*43.14*0.83","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.1”","KD021WVOSN009-C003B","PDF","480x480","QSPI","CO5300AF","Free V.A","CTP","-20℃~60℃","600 nits","42.39*42.39*2.55","38.39*38.39","Capacitive Touch Display,AMOLED Display,Square TFT,LTPS Display"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.4”","KD024EGOIN152-01","PDF","450x600","MCU/MIPI","RM690B0","Free V.A","No TP","-20℃~80℃","800 nits","38.72*51.56*1.00","36.72*48.96","AMOLED Display,High-brightness TFT,LTPS Display"]
["2.5”","KD025EGOIN002-C000","PDF","400x712","MIPI","RM690C0","Free V.A","CTP","-20℃~70℃","800 nits","32.90*58.56*2.00","31.10*55.36","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["2.7”","KD027WVOIN011","PDF","800x600","MIPI","RM69700","Free V.A","No TP","-40℃~85℃","400 nits","56.60*47.25*1.50","54.60*40.95","AMOLED Display,Wide Temp TFT,LTPS Display"]
["2.9”","KD029FHOIN010","PDF","1080x1200","MIPI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*0.65","50.11*55.68","AMOLED Display,LTPS Display"]
["2.9”","KD029FHOIN010-HDMI","PDF","1080x1200","HDMI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*11.00","50.11*55.68","AMOLED Display,LTPS Display,HDMI AMOLED"]
["3.7”","KD037WVOPD004","PDF","480x800","RGB","TL2796","Free V.A","No TP","-30℃~80℃","250 nits","53.94*90.00*1.50","48.24*80.40","AMOLED Display,Wide Temp TFT,LTPS Display"]
["3.9”","KD039FHOIN003-01-C0000","PDF","1080x1240","MIPI","SD5302","Free V.A","CTP","-20℃~70℃","500 nits","67.25*79.87*0.80","65.45*75.14","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040UXOIN109-C073A","PDF","1080x1200","MIPI","VTDR6130A","Free V.A","CTP","-20℃~70℃","600 nits","72.93*80.53*1.12","68.43*76.03","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.1”","KD041HDOIN002-C000","PDF","2480x1860","MIPI","RM69A10","Free V.A","CTP","-20℃~70℃","280 nits","48.24*100.84*2.64","43.55*94.47","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043OLEDN001","PDF","568x1210","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","600 nits","49.13*103.55*0.75","47.37*100.91","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C000","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C116B","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","70.52*123.12*1.67","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C000-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","64.12*116.72*10.80","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C116B-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","70.52*123.12*12.37","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN132-C001","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C000-a","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001","PDF","1080x1920","MIPI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*0.82","67.82*120.58","Capacitive Touch Display,AMOLED Display"]
["5.5”","KD055FHOIN031-C0000","PDF","1080x1920","MIPI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.82","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001-SP005A-HDMI","PDF","1080x1920","HDMI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*10.80","67.82*120.58","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN031-C0000-HDMI","PDF","1080x1920","HDMI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.83","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.0”","KD060FPOIN011-C0000","PDF","1080x2160","MIPI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.0”","KD060FPOIN011-C0000-HDMI","PDF","1080x2160","HDMI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.4”","KD064FPOIN001-C0000","PDF","1080x2340","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.4”","KD064FPOIN001-C0000-HDMI","PDF","1080x2340","HDMI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.5”","KD065FPOIN003","PDF","1080x2400","MIPI","RM692E5","Free V.A","No TP","-20℃~70℃","500 nits","71.45*156.64*0.29","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.5”","KD065FPOIN003-HDMI","PDF","1080x2400","HDMI","TBD","Free V.A","No TP","-20℃~70℃","450 nits","71.45*156.64*11.00","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["6.67”","KD067FPOIN004-C0000","PDF","1080x2400","MIPI","VTDR6130","Free V.A","CTP","-20℃~70℃","500 nits","71.53*200.59*0.33","69.55*154.56","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display"]
["7.0”","KD070FHOIN128-C0000","PDF","1080x1920","MIPI","ICNA3512","Free V.A","CTP","-20℃~70℃","950 nits","89.13*160.91*1.01","87.13*154.91","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-C000-a","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["12.8”","KD128OLED004","PDF","1728x1888","LVDS","HX8160-G01","Free V.A","No TP","-40℃~85℃","600 nits","224.96*248.22*5.80","218.76*239.02","AMOLED Display"]
["13.0”","KD130UXOEN001-C001A","PDF","2560x1440","eDP","RM98120","Free V.A","CTP","-40℃~85℃","800 nits","292.69*168.27*2.10","286.69*161.27","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["13.3”","KD133QXFEN020","PDF","1536x2048","eDP","TBD","Free V.A","No TP","0℃~50℃","300 nits","213.80*284.80*0.53","202.75*270.34","AMOLED Display,Flexible AMOLED,LTPS Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["14.5”","KD145OLEDN003-C003A","PDF","3000x1876","MIPI","HX5318","Free V.A","CTP","-20℃~70℃","400 nits","316.56*201.06*1.62","312.30*192.29","Capacitive Touch Display,AMOLED Display"]
["15.1”","KD151WQOEN001-C0000","PDF","2560x1600","eDP","RM98121","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*1.30","324.10*202.56","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["15.1”","KD151WQOEN001-SP001A-HDMI","PDF","2560x1600","HDMI","TBD","Free V.A","No TP","-40℃~85℃","550 nits","328.90*210.46*5.80","324.10*202.56","AMOLED Display,Wide Temp TFT,LTPS Display,HDMI AMOLED"]
["15.6”","KD156UHOEN018","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*1.05","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN025","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.22*201.62*1.10","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN018-C014A","PDF","3840x2160","eDP","RM98110","Free V.A","CTP","-20℃~70℃","320 nits","357.22*208.27*3.35","344.22*193.62","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN018-SP001A-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*15.00","344.22*193.62","AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270UDOEN003","PDF","3840x2160","eDP","TBD","Free V.A","No TP","-20℃~70℃","400 nits","607.66*348.18*1.24","597.66*336.18","AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B","PDF","3840x2160","eDP","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*4.19","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*13.60","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270QHOVD026","PDF","2560x1440","V-By-One","TBD","Free V.A","No TP","0℃~45℃","1300 nits","600.62*346.42*0.78","586.75*330.05","AMOLED Display,High-brightness TFT,LTPS Display"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,Display Monitor,OLED Monitor"]
["31.5”","KD320UHOVD017","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~45℃","230 nits","709.68*407.43*0.80","696.58*391.82","AMOLED Display,LTPS Display"]

{"sheet":"PM-OLED Display","index":13,"n_rows":17,"n_cols":13,"rows_kept":17}
["STARTEK PM-OLED Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.91”","KD0091SQOIN001","PDF","128x32","i2C","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","38.00*12.00*3.80","22.38*5.58","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["0.96”","KD0096SQOSN009","PDF","128x64","SPI","SSD1306","Free V.A","No TP","-40℃~70℃","180 nits","27.30*27.80*4.10","21.74*10.86","PMOLED Display,Wide Temp TFT"]
["0.96”","KD0096SQOSN012","PDF","128x64","SPI/IIC","SSD1315","Free V.A","No TP","-40℃~85℃","80 nits","24.70*16.60*1.30","21.74*11.18","PMOLED Display,Wide Temp TFT"]
["1.1”","KD011SQOSN002","PDF","64x128","SPI","CH1115","Free V.A","No TP","-40℃~70℃","180 nits","24.00*33.00*3.80","10.86*25.58","PMOLED Display,Wide Temp TFT"]
["1.3”","KD013SQOIN012","PDF","128x64","i2C","SH1106","Free V.A","No TP","-40℃~70℃","150 nits","35.40*33.50*4.00","29.42*14.70","PMOLED Display,Wide Temp TFT"]
["1.5”","KD015SQOSN013","PDF","128x128","SPI","SH1107","Free V.A","No TP","-40℃~70℃","100 nits","34.00*49.30*5.00","26.86*26.86","PMOLED Display,Wide Temp TFT"]
["1.54”","KD0154WEOLN006","PDF","128x64","Parallel/SPI/I2C","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","42.04*27.22*1.46","35.04*17.51","PMOLED Display,Wide Temp TFT"]
["1.7”","KD017SQOIN003","PDF","128x32","i2C","SSD1312","Free V.A","No TP","-40℃~70℃","120 nits","60.50*18.75*4.95","42.22*10.54","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.1”","KD021SCOIN007","PDF","256x64","i2C","SH1122","Free V.A","No TP","-40℃~70℃","150 nits","72.50*27.24*5.10","51.18*12.78","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.2”","KD022SQOSN037","PDF","128x32","SPI/IIC","SSD1305","Free V.A","No TP","-40℃~70℃","120 nits","74.00*30.00*8.20","55.02*13.10","PMOLED Display,Wide Temp TFT,Bartype TFT"]
["2.4”","KD024SQOSN132","PDF","128x64","SPI","SSD1309","Free V.A","No TP","-40℃~70℃","120 nits","72.00*43.00*7.00","55.01*27.49","PMOLED Display,Wide Temp TFT"]
["3.1”","KD031SCOSN004","PDF","256x64","SPI","SSD1322","Free V.A","No TP","-40℃~70℃","80 nits","102.00*35.00*6.60","76.78*19.18","PMOLED Display"]
["5.5”","KD055SCOSN025","PDF","256x64","SPI","SSD1322","Free V.A","No TP","-40℃~70℃","80 nits","160.00*50.00*6.60","135.65*33.89","PMOLED Display"]

{"sheet":"Mini-LED","index":14,"n_rows":5,"n_cols":13,"rows_kept":5}
["STARTEK Mini-LED 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["32.0”","KD320FHFLA005","PDF","1920x1080","LVDS","TBD","Free V.A","No TP","-20℃~70℃","1700 nits","719.40*416.90*26.60","698.40*392.90","High-brightness TFT,Mini-LED"]

{"sheet":"HDMI TFT","index":15,"n_rows":76,"n_cols":13,"rows_kept":76}
["STARTEK HDMI TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["2.4”","KD024VGFPD094-C021D-SP002A-HDMI","PDF","480x640","HDMI","ST7701SI","Free V.A","CTP","-20℃~70℃","700 nits","48.72*70.26*20.00","36.72*48.96","Capacitive Touch Display,HDMI TFT"]
["2.8”","KD028VGFPD047-SP001A-HDMI","PDF","480x640","HDMI","ST7701S","Free V.A","No TP","-20℃~70℃","750 nits","47.00*66.25*1.83","43.20*57.60","HDMI TFT"]
["2.8”","KD028VGFPD047-C026A-SP001A-HDMI","PDF","480x640","HDMI","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,HDMI TFT"]
["2.9”","KD029QHFID001-C001A-SP001A-HDMI","PDF","376x960","HDMI","SC7283","Free V.A","CTP","-20℃~70℃","500 nits","40.20*85.60*3.26","26.51*67.68","Capacitive Touch Display,HDMI TFT"]
["3.4”","KD034WVFID003-SP001A-HDMI","PDF","800x800","HDMI","ILI9881C","Free V.A","No TP","-20℃~70℃","600 nits","94.89*96.95*17.08","87.60*87.60","Round TFT,HDMI TFT"]
["3.5”","KD035VGFPD167-C061B-SP004A-HDMI","PDF","640x480","HDMI","NV3052CGRB","Free V.A","CTP","-10℃~60℃","500 nits","85.80*85.80*21.36","70.08*52.56","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["4.0”","KD040WVFPA027-SP002A-HDMI","PDF","480x800","HDMI","ST7701S","Free V.A","No TP","-10℃~60℃","480 nits","58.26*98.10*13.78","51.84*86.40","HDMI TFT"]
["4.3”","KD043WVFLA096-03-C049A-ZJB-HDMI","PDF","800x480","HDMI","ST7262","Free V.A","CTP","-10℃~60℃","450 nits","105.40*79.15*21.96","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WVFPA084-02-SP001A-HDMI","PDF","480x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","730 nits","62.50*105.55*19.75","56.16*93.60","HDMI TFT"]
["4.3”","KD043WQTPA097A-04-C017A-SP003A-HDMI","PDF","480x272","HDMI","TBD","V.A 12H","CTP","-20℃~70℃","500 nits","115.40*79.15*21.89","95.04*53.86","Capacitive Touch Display,HDMI TFT"]
["4.3”","KD043WQFPD042-07-C017C-SP004A-HDMI","PDF","480x272","HDMI","TBD","Free V.A","CTP","-20℃~70℃","1000 nits","115.40*79.15*20.40","95.04*53.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["4.3”","KD043WVFPA084-05-C015B-SP001A-HDMI","PDF","480x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","62.50*105.55*21.30","56.16*93.60","Capacitive Touch Display,HDMI TFT"]
["4.5”","KD045FWTPA001-02-SP001A-HDMI","PDF","480x854","HDMI","ILI9806E","V.A 12H","No TP","-20℃~70℃","350 nits","61.54*110.09*17.45","55.44*98.64","HDMI TFT"]
["4.5”","KD045FWTPA001-02-C001B-SP001A-HDMI","PDF","480x854","HDMI","ILI9806E","V.A 12H","CTP","-20℃~70℃","350 nits","61.54*110.09*19.00","55.44*98.64","Capacitive Touch Display,HDMI TFT"]
["5.0”","KD050WVTPA045-C005A-SP001A-HDMI","PDF","800x480","HDMI","ILI5960/ILI6122","V.A 12H","CTP","-10℃~60℃","310 nits","120.70*75.80*19.81","108.00*64.80","Capacitive Touch Display,HDMI TFT"]
["5.0”","KD050FHFLD102-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","116.59*72.76*18.67","110.59*62.21","High-brightness TFT,HDMI TFT"]
["5.5”","KD055HDFIA001-C001A-SP002A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","500 nits","86.04*144.96*21.85","68.04*120.96","Capacitive Touch Display,HDMI TFT"]
["5.5”","KD055FHFID018-01-C017A-SP003A-HDMI","PDF","1080x1920","HDMI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*19.74","68.04*120.96","Capacitive Touch Display,HDMI TFT,LTPS Display"]
["5.6”","KD056VGTPA004-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","No TP","-20℃~70℃","850 nits","126.50*100.00*13.08","115.20*86.40","High-brightness TFT,HDMI TFT"]
["5.6”","KD056VGTPA004-C004A-SP001A-HDMI","PDF","640x480","HDMI","HX8250-A+HX8678-B","V.A 12H","CTP","-20℃~70℃","750 nits","126.50*100.00*23.60","115.50*86.40","Capacitive Touch Display,HDMI TFT"]
["5.8”","KD058UXFLA003-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","No TP","-10℃~60℃","950 nits","144.56*87.40*20.40","126.72*71.28","High-brightness TFT,HDMI TFT"]
["5.8”","KD058UXFLA003-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","ST5892B","Free V.A","CTP","-20℃~70℃","900 nits","144.56*87.40*21.26","126.72*71.28","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.0”","KD060HDFID001-SP001A-HDMI","PDF","720x1440","HDMI","ILI9881C","Free V.A","No TP","-20℃~70℃","450 nits","75.04*147.63*17.25","68.04*136.08","HDMI TFT"]
["6.0”","KD060HDFID001-C001A-SP001A-HDMI","PDF","720x1440","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","95.04*167.63*19.23","68.04*136.08","Capacitive Touch Display,HDMI TFT"]
["6.0”","KD060HDFID006-C005A-SP001A-HDMI","PDF","720x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","80.58*146.12*18.21","73.98*131.52","Capacitive Touch Display,HDMI TFT"]
["6.2”","KD062VGFPA003-01-SP001A-HDMI","PDF","640x240","HDMI","ST5043AA/ST5894AA","Free V.A","No TP","-20℃~70℃","900 nits","163.60*67.60*17.77","148.80*53.76","High-brightness TFT,Bartype TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-C001A-SP001A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1500 nits","161.12*97.68*23.02","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1100 nits","161.12*97.68*20.67","148.32*83.43","High-brightness TFT,HDMI TFT"]
["6.7”","KD067WSFLA001-C001A-SP002A-HDMI","PDF","1920x1080","HDMI","HX8249/HX8678","Free V.A","CTP","-20℃~70℃","1000 nits","161.12*97.68*23.10","148.32*83.43","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPA007-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","No TP","-20℃~70℃","800 nits","156.10*100.91*21.40","140.10*88.86","High-brightness TFT,HDMI TFT"]
["6.8”","KD068WVFPD007-01-C003A-SP001A-HDMI","PDF","800x480","HDMI","TBD","Free V.A","CTP","-20℃~70℃","800 nits","155.96*100.77*23.19","148.10*88.86","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["7.0”","KD070WVFLA035A-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","Free V.A","No TP","-10℃~60℃","1100 nits","65.40*104.59*22.90","152.40*91.44","High-brightness TFT,HDMI TFT"]
["7.0”","KD070WVFLA035A-C049C-SP001A-HDMI","PDF","800x480","HDMI","RM533CO+RM577C1","V.A 12H","CTP","-10℃~60℃","1000 nits","165.40*104.59*24.83","152.40*91.44","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["7.0”","KD070C-4-SP003A-HDMI","PDF","800x480","HDMI","TBD","V.A 12H","No TP","-10℃~60℃","450 nits","165.00*100.00*22.90","154.08*85.92","HDMI TFT"]
["7.0”","KD070WUFID085-C021A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-20℃~70℃","410 nits","119.46*176.78*19.30","94.50*151.20","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070HDFLA028-02-C027B-SP001A-HDMI","PDF","1024x600","HDMI","EK73215&EK79001","Free V.A","CTP","-10℃~60℃","550 nits","165.00*100.00*22.27","154.21*85.92","Capacitive Touch Display,HDMI TFT"]
["7.0”","KD070WXFID094-CP001A-HDMI","PDF","280x1424","HDMI","OTA7290N","Free V.A","No TP","-20℃~70℃","900 nits","38.20*181.47*3.44","33.60*170.88","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.0”","KD070HDFLD070-SP001A-HDMI","PDF","1280x768","HDMI","HX8298-Ax3+HX8695Ex1","Free V.A","No TP","-10℃~60℃","1200 nits","166.90*108.65*21.23","152.45*91.47","High-brightness TFT,HDMI TFT"]
["7.0”","KD070C-4-05-C004A-SP002A-HDMI","PDF","800x480","HDMI","EK9713/EK73002","V.A 12H","CTP","-10℃~60℃","400 nits","165.00*100.00*24.43","154.08*85.92","Capacitive Touch Display,HDMI TFT"]
["7.84”","KD078HDFID004-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","No TP","-20℃~70℃","800 nits","67.60*206.28*19.29","59.40*190.08","High-brightness TFT,Bartype TFT,HDMI TFT"]
["7.84”","KD078HDFID004-C004A-SP001A-HDMI","PDF","400x1280","HDMI","GC9703C","Free V.A","CTP","-20℃~70℃","800 nits","67.60*206.28*21.12","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["8.0”","KD080WXFLD023-C015A-SP002A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","400 nits","130.70*200.10*22.15","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080WXFID015-C015A-SP003A-HDMI","PDF","800x1280","HDMI","ILI9881C","Free V.A","CTP","-20℃~60℃","500 nits","130.70*200.10*22.09","107.64*172.22","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080C-5-01-C006B-CP001A-HDMI","PDF","1024x768","HDMI","TBD","V.A 12H","CTP","-10℃~60℃","300 nits","174.00*136.00*13.92","162.05*121.54","Capacitive Touch Display,HDMI TFT"]
["8.0”","KD080C-5-01-CP001A-HDMI","PDF","1024x768","HDMI","TBD","V.A 12H","No TP","-10℃~60℃","450 nits","174.00*136.00*11.53","162.05*121.54","HDMI TFT"]
["9.0”","KD090HDFLA006-SP001A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*22.50","196.61*114.15","High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFID027-C012B-SP001A-HDMI","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-20℃~60℃","350 nits","159.00*244.60*19.76","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101FHFID030-C014A-SP001A-HDMI","PDF","1200x1920","HDMI","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*19.40","135.36*216.58","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101WSFID033-C040A-SP001A-HDMI","PDF","1024x600","HDMI","EK73217& EK79007","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.76","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101HDFLD020-01-C045C-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","900 nits","232.70*155.56*24.50","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFLD021-02-C045C-SP007A-HDMI","PDF","1280x800","HDMI","EK79202D_A","Free V.A","CTP","-20℃~70℃","700 nits","229.06*148.70*22.84","216.96*135.60","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.1”","KD101HDFLD020-SP009A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","1000 nits","232.70*155.55*22.50","216.96*135.60","High-brightness TFT,HDMI TFT"]
["10.1”","KD101WXFLD047-01-SP001A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","600 nits","229.06*148.70*12.41","216.96*135.60","HDMI TFT"]
["10.1”","KD101FHFID031-C037A-CP001A-HDMI","PDF","440x1920","HDMI","ICNL9707","Free V.A","CTP","-20℃~70℃","900 nits","85.00*288.45*12.29","57.95*252.86","Capacitive Touch Display,High-brightness TFT,Bartype TFT,HDMI TFT"]
["10.1”","KD101WSFLA058-C065A-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","254.50*162.50*23.15","222.72*125.28","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101UXFLD024A-SP003A-HDMI","PDF","1920x1200","HDMI","TBD","Free V.A","No TP","-10℃~60℃","550 nits","226.37*148.81*19.04","216.81*135.50","HDMI TFT"]
["10.1”","KD101UXFLD024D-SP001A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1000 nits","229.46*149.10*22.73","216.81*135.50","High-brightness TFT,HDMI TFT"]
["10.1”","KD101WSFLA058-SP012A-HDMI","PDF","1024x600","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","235.00*143.00*20.90","222.72*125.28","High-brightness TFT,HDMI TFT"]
["10.1”","KD101FM-1-10-C032C-SP005A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","CTP","-10℃~60℃","650 nits","254.50*162.50*21.24","216.96*135.60","Capacitive Touch Display,HDMI TFT"]
["10.1”","KD101UXFLD024D-01-C035A-SP002A-HDMI","PDF","1920x1200","HDMI","HX8290-Bx3","Free V.A","No TP","-20℃~70℃","1100 nits","246.31*168.75*23.98","216.81*135.50","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["10.4”","KD104HDFLD006-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","No TP","-10℃~60℃","680 nits","236.00*174.34*18.95","211.20*158.40","HDMI TFT"]
["11.6”","KD116WSFEA002-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","800 nits","268.00*158.00*21.56","256.32*144.18","High-brightness TFT,HDMI TFT"]
["11.6”","KD116WSFEA002-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","750 nits","291.52*179.38*24.28","256.32*144.18","Capacitive Touch Display,HDMI TFT"]
["12.1”","KD121HDFLA011-SP001A-HDMI","PDF","1280x800","HDMI","TBD","Free V.A","No TP","-10℃~60℃","350 nits","278.00*184.00*15.60","261.12*163.20","HDMI TFT"]
["12.1”","KD121HDFLA013-C007A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","750 nits","290.00*228.50*31.94","245.76*184.32","Capacitive Touch Display,HDMI TFT"]
["12.8”","KD128FHFLD001-01-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-30℃~85℃","650 nits","294.40*175.00*26.20","283.39*159.41","Wide Temp TFT,HDMI TFT"]
["12.8”","KD128FHFLD001-01-C002A-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-30℃~85℃","550 nits","320.59*196.61*29.45","283.39*159.41","Capacitive Touch Display,Wide Temp TFT,HDMI TFT"]
["13.3”","KD133FHFLA013-C009A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-20℃~70℃","900 nits","325.20*199.80*22.55","293.47*165.08","Capacitive Touch Display,High-brightness TFT,HDMI TFT"]
["13.3”","KD133FHFLA013-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-20℃~70℃","950 nits","309.70*184.10*19.35","293.47*165.08","High-brightness TFT,HDMI TFT"]
["14.0”","KD140FHFLD003-SP001A-HDMI","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","-10℃~60℃","650 nits","317.52*186.73*27.77","308.16*173.34","HDMI TFT"]
["15.0”","KD150XGFLD002-C001A-SP001A-HDMI","PDF","1024x768","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","385.50*312.50*30.92","304.10*228.10","Capacitive Touch Display,HDMI TFT"]
["19.0”","KD190SGFLA005-C002A-SP001A-HDMI","PDF","1280x1024","HDMI","TBD","Free V.A","CTP","-10℃~60℃","720 nits","423.00*347.70*37.00","376.32*301.06","HDMI TFT"]

{"sheet":"HDMI AMOLED","index":16,"n_rows":16,"n_cols":13,"rows_kept":16}
["STARTEK HDMI AMOLED 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["2.9”","KD029FHOIN010-HDMI","PDF","1080x1200","HDMI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*11.00","50.11*55.68","AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C000-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","64.12*116.72*10.80","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C116B-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","70.52*123.12*12.37","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN030-C001-SP005A-HDMI","PDF","1080x1920","HDMI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*10.80","67.82*120.58","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN031-C0000-HDMI","PDF","1080x1920","HDMI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.83","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.0”","KD060FPOIN011-C0000-HDMI","PDF","1080x2160","HDMI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.4”","KD064FPOIN001-C0000-HDMI","PDF","1080x2340","HDMI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.5”","KD065FPOIN003-HDMI","PDF","1080x2400","HDMI","TBD","Free V.A","No TP","-20℃~70℃","450 nits","71.45*156.64*11.00","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["15.1”","KD151WQOEN001-SP001A-HDMI","PDF","2560x1600","HDMI","TBD","Free V.A","No TP","-40℃~85℃","550 nits","328.90*210.46*5.80","324.10*202.56","AMOLED Display,Wide Temp TFT,LTPS Display,HDMI AMOLED"]
["15.6”","KD156UHOEN018-SP001A-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*15.00","344.22*193.62","AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270UDOEN003-C002B-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*13.60","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]

{"sheet":"Type-C TFT","index":17,"n_rows":25,"n_cols":13,"rows_kept":25}
["STARTEK Type-C TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["2.8”","KD028VGFID048-C026A-SP002A-TypeC","PDF","480x640","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*15.00","43.20*57.60","Capacitive Touch Display,Type-C TFT"]
["3.4”","KD034WXFID001-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","No TP","-30℃~70℃","950 nits","65.72*69.64*14.00","60.48*60.48","High-brightness TFT,Square TFT,Type-C TFT"]
["3.4”","KD034WXFID001-C001A-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*16.00","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["3.5”","KD035VGFIA111-C041A-SP007A-TypeC","PDF","480x640","Type C","TBD","Free V.A","CTP","-20℃~70℃","360 nits","64.00*85.00*17.00","53.28*71.04","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035VGFIA111-SP007A-TypeC","PDF","480x640","Type C","TBD","Free V.A","No TP","-20℃~70℃","460 nits","64.00*85.00*14.60","53.28*71.04","Type-C TFT"]
["3.5”","KD035VGFID162-C061B-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","CTP","-20℃~70℃","660 nits","85.80*85.80*16.00","70.08*52.56","Capacitive Touch Display,Type-C TFT"]
["3.5”","KD035VGFID162-SP005A-TypeC","PDF","640x480","Type C","TBD","Free V.A","No TP","-20℃~70℃","740 nits","74.38*62.35*14.00","70.08*52.56","Square TFT,Type-C TFT"]
["4.0”","KD040HDFID032-C026C-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","CTP","-20℃~70℃","650 nits","84.00*85.99*15.50","71.93*71.93","Capacitive Touch Display,Square TFT,Type-C TFT"]
["4.0”","KD040HDFID032-SP003A-TypeC","PDF","720x720","Type C","ST7703","Free V.A","No TP","-20℃~70℃","700 nits","77.00*80.00*14.00","71.93*71.93","Square TFT,Type-C TFT"]
["4.0”","KD040WVFID026-01-C025A-SP005A-TypeC","PDF","480x800","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","430 nits","58.26*98.10*16.00","51.84*86.40","Capacitive Touch Display,Type-C TFT"]
["4.0”","KD040WXFID017-C015C-SP002A-TypeC","PDF","480x480","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","1000 nits","77.00*80.00*16.00","71.86*70.18","Capacitive Touch Display,High-brightness TFT,Square TFT,Type-C TFT"]
["4.0”","KD040QHFID049-SP004A-TypeC","PDF","400x960","Type C","ST7701S","Free V.A","No TP","-20℃~70℃","500 nits","42.50*102.08*13.50","39.18*94.03","Type-C TFT"]
["4.0”","KD040QHFID049-C039A-SP004A-TypeC","PDF","400x960","Type C","ST7701S","Free V.A","CTP","-20℃~70℃","450 nits","52.50*112.08*15.00","39.18*94.03","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050HDFIA020-SP003A-TYPE C","PDF","720x1280","Type C","ILI9881C","Free V.A","No TP","-20℃~70℃","500 nits","67.56*122.35*13.75","62.10*110.40","Type-C TFT"]
["5.0”","KD050HDFIA020-06-C020E-SP003A-TYPE C","PDF","720x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","67.56*122.35*15.35","62.10*110.40","Capacitive Touch Display,Type-C TFT"]
["5.0”","KD050FWFIA019-SP004-TYPE C","PDF","480x854","Type C","ILI9806E","Free V.A","No TP","-20℃~70℃","610 nits","67.56*122.35*13.70","61.63*109.65","Type-C TFT"]
["5.0”","KD050FWFIA019-02-C009E-SP004A-TYPE C","PDF","480x854","Type C","ILI9806E","Free V.A","CTP","-20℃~70℃","540 nits","67.56*122.35*15.25","61.63*109.65","Capacitive Touch Display,Type-C TFT"]
["6.0”","KD060HDFID001-C001A-SP002A-TYPEC","PDF","720x1440","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","480 nits","95.04*167.63*15.55","68.04*136.08","Capacitive Touch Display,Type-C TFT"]
["7.0”","KD070WXFID050-C038A-SP001A-TYPEC","PDF","800x1280","Type C","ILI9881C","Free V.A","CTP","-20℃~70℃","420 nits","119.46*176.78*15.80","94.20*150.72","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101FHFID030-C036A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","280 nits","174.37*255.12*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]
["10.1”","KD101FHFID030-C014A-SP005A-TYPEC","PDF","1200x1920","Type C","TBD","Free V.A","CTP","-10℃~50℃","220 nits","159.00*244.60*15.90","135.36*216.58","Capacitive Touch Display,Type-C TFT"]

{"sheet":"UART TFT","index":18,"n_rows":170,"n_cols":13,"rows_kept":170}
["STARTEK UART TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.77”","KD018QVFMN010-02-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","250 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["1.77”","KD018QVFMN010-02-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","200 nits","39.70*52.50*20.27","26.64*35.52","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-RS232","PDF","320x240","RS232","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-RS485","PDF","320x240","RS485","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020LQFMA014-C003A-TTL","PDF","320x240","TTL","ILI9342C","Free V.A","CTP","-20℃~70℃","600 nits","54.50*47.56*18.26","40.80*30.60","Capacitive Touch Display,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS232","PDF","480x360","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020WQFPA023-C003B-RS485","PDF","480x360","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020WQFPA023-C003B-TTL","PDF","480x360","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","950 nits","54.49*47.56*18.39","40.82*30.62","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.0”","KD020QVFMA009-C001A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.0”","KD020QVFMA009-C001A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","600 nits","35.80*52.10*18.51","30.60*40.80","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.2”","KD022QVFMD018-C002A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","700 nits","41.70*56.16*18.87","33.84*45.12","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024VGFPD094-C021D-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","740 nits","48.72*70.26*19.71","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024QVFMA020-C009A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","500 nits","42.92*60.26*20.00","36.72*48.96","Capacitive Touch Display,UART TFT"]
["2.4”","KD024WVFPD102-C001A-RS232","PDF","800x480","RS232","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-RS485","PDF","800x480","RS485","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.4”","KD024WVFPD102-C001A-TTL","PDF","800x480","TTL","HX8283-A","Free V.A","CTP","-20℃~70℃","670 nits","66.00*49.30*21.00","52.32*31.39","Capacitive Touch Display,UART TFT"]
["2.6”","KD026WXFLD022-C008A-RS232","PDF","1280x720","RS232","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-TTL","PDF","1280x720","TTL","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.6”","KD026WXFLD022-C008A-RS485","PDF","1280x720","RS485","SC5014","Free V.A","CTP","-20℃~70℃","1400 nits","73.88*53.46*18.61","57.60*32.40","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["2.7”","KD027HVFMD010-C004A-RS232","PDF","320x320","RS232","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-RS485","PDF","320x320","RS485","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.7”","KD027HVFMD010-C004A-TTL","PDF","320x320","TTL","ST7796","Free V.A","CTP","-20℃~70℃","800 nits","63.40*69.90*19.50","48.96*48.96","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-RS232","PDF","240x320","RS232","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-RS485","PDF","240x320","RS485","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028QVTMA005-C020A-TTL","PDF","240x320","TTL","ST7789V","V.A 12H","CTP","-20℃~70℃","550 nits","50.50*69.70*4.35","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS232","PDF","480x640","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*19.00","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-RS485","PDF","480x640","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028VGFPD047-C026A-TTL","PDF","480x640","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","670 nits","56.10*77.29*3.29","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-RS485","PDF","240x320","RS485","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["2.8”","KD028FM-1-04-C020A-TTL","PDF","240x320","TTL","ST7789V","Free V.A","CTP","-20℃~70℃","650 nits","50.50*69.70*4.36","43.20*57.60","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*3.83","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.1”","KD031WVFPD002-C001A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","350 nits","62.80*86.80*19.50","40.32*67.20","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-TTL","PDF","240x320","TTL","ST7789V","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*2.40","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-C002A-RS232","PDF","240x320","RS232","ST7789V","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-RS232","PDF","240x320","RS232","ST7789V2","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*2.40","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-RS485","PDF","240x320","RS485","ST7789V2","Free V.A","No TP","-20℃~70℃","500 nits","54.99*77.20*15.10","48.60*64.80","UART TFT"]
["3.2”","KD032QVFMD028-C002A-RS485","PDF","240x320","RS485","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*15.10","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.2”","KD032QVFMD028-C002A-TTL","PDF","240x320","TTL","ST7789V2","Free V.A","CTP","-20℃~70℃","450 nits","54.99*77.20*3.65","48.60*64.80","Capacitive Touch Display,UART TFT"]
["3.4”","KD034WXFPD002-RS232","PDF","480x480","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-RS485","PDF","480x480","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-TTL","PDF","480x480","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","900 nits","65.72*69.64*15.10","60.48*60.48","High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.4”","KD034WXFPD002-C001A-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","850 nits","65.72*69.64*15.10","60.48*60.48","Capacitive Touch Display,High-brightness TFT,Square TFT,UART TFT"]
["3.5”","KD035HVTMA026-C052A-RS232","PDF","320x480","RS232","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035QVFMA064-RS232","PDF","240x320","RS232","HX8347A","Free V.A","No TP","-30℃~80℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-RS485","PDF","240x320","RS485","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-TTL","PDF","240x320","TTL","HX8347A","Free V.A","No TP","-30℃~85℃","450 nits","63.00*85.00*15.10","53.28*71.04","Wide Temp TFT,UART TFT"]
["3.5”","KD035HVTMA026-C052A-TTL","PDF","320x480","TTL","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035HVTMA026-C052A-RS485","PDF","320x480","RS485","ILI9488","V.A 6H","CTP","-20℃~70℃","300 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,UART TFT"]
["3.5”","KD035HVFMA155-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVFMA155-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","No TP","-30℃~85℃","800 nits","55.50*84.96*15.10","48.96*73.44","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS232","PDF","240x320","RS232","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-RS485","PDF","240x320","RS485","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035QVFMA064-04-C021A-TTL","PDF","240x320","TTL","HX8347A","Free V.A","CTP","-30℃~85℃","400 nits","63.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS232","PDF","320x480","RS232","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-RS485","PDF","320x480","RS485","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035HVFMA155-C055A-TTL","PDF","320x480","TTL","ST7796SI","Free V.A","CTP","-30℃~85℃","720 nits","55.50*84.96*15.10","48.96*73.44","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS232","PDF","320x240","RS232","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-RS485","PDF","320x240","RS485","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-TTL","PDF","320x240","TTL","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-C037A-CAN","PDF","320x240","CAN","ST7272A","Free V.A","CTP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS232","PDF","320x240","RS232","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-RS485","PDF","320x240","RS485","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-TTL","PDF","320x240","TTL","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035LQFPA093-04-CAN","PDF","320x240","CAN","ST7272A","Free V.A","No TP","-30℃~85℃","1250 nits","86.84*74.84*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035HVTMA026-RS232","PDF","320x480","RS232","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035HVTMA026-RS485","PDF","320x480","RS485","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035HVTMA026-TTL","PDF","320x480","TTL","ILI9488","V.A 6H","No TP","-20℃~70℃","350 nits","55.50*84.96*15.10","48.96*73.44","UART TFT"]
["3.5”","KD035VGFPA094-RS232","PDF","480x640","RS232","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-RS485","PDF","480x640","RS485","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-TTL","PDF","480x640","TTL","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-CAN","PDF","480x640","CAN","ILI9806E","Free V.A","No TP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS232","PDF","480x640","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-RS485","PDF","480x640","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-TTL","PDF","480x640","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPA094-C041A-CAN","PDF","480x640","CAN","ILI9806E","Free V.A","CTP","-20℃~70℃","600 nits","64.00*85.00*15.10","53.28*71.04","Capacitive Touch Display,UART TFT"]
["3.5”","KD035VGFPD250-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","No TP","-30℃~85℃","1100 nits","73.08*59.56*15.10","70.08*52.56","Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS232","PDF","640x480","RS232","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-RS485","PDF","640x480","RS485","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035VGFPD250-C061B-TTL","PDF","640x480","TTL","NV3052CGRB","Free V.A","CTP","-30℃~85℃","1000 nits","85.80*82.15*15.10","70.08*52.56","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-C047A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","400 nits","60.16*96.30*15.10","45.36*75.60","Capacitive Touch Display,UART TFT"]
["3.5”","KD035WVFPD122-RS232","PDF","480x800","RS232","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.5”","KD035WVFPD122-RS485","PDF","480x800","RS485","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.5”","KD035WVFPD122-TTL","PDF","480x800","TTL","ST7701S","Free V.A","No TP","-20℃~70℃","450 nits","50.16*86.30*15.10","45.36*75.60","UART TFT"]
["3.8”","KD038HDFPD002-C001A-RS232","PDF","1024x600","RS232","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-RS485","PDF","1024x600","RS485","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["3.8”","KD038HDFPD002-C001A-TTL","PDF","1024x600","TTL","JD9168","Free V.A","CTP","-20℃~70℃","1000 nits","97.92*67.93*19.76","82.64*48.42","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS232","PDF","720x720","RS232","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-RS485","PDF","720x720","RS485","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-TTL","PDF","720x720","TTL","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS232","PDF","480x800","RS232","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-RS485","PDF","480x800","RS485","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WVFPA027-C022A-TTL","PDF","480x800","TTL","ST7701S","Free V.A","CTP","-20℃~70℃","470 nits","58.26*98.10*19.00","51.84*86.40","Capacitive Touch Display,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS232","PDF","480x480","RS232","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-RS485","PDF","480x480","RS485","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040WXFPD014-C015C-TTL","PDF","480x480","TTL","ST7701S","Free V.A","CTP","-30℃~85℃","1000 nits","77.00*80.00*15.31","71.86*70.18","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.0”","KD040HDFPD039-C026A-CAN","PDF","720x720","CAN","NV3052C","Free V.A","CTP","-30℃~80℃","600 nits","84.00*85.99*19.18","71.93*71.93","Capacitive Touch Display,Wide Temp TFT,Square TFT,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS232","PDF","480x800","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-RS485","PDF","480x800","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WVFPA084-01-C015B-TTL","PDF","480x800","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","400 nits","62.50*105.55*19.15","56.16*93.60","Capacitive Touch Display,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS232","PDF","480x272","RS232","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-RS485","PDF","480x272","RS485","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-TTL","PDF","480x272","TTL","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS232","PDF","800x480","RS232","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-RS485","PDF","800x480","RS485","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WVFPA051-05-C049A-TTL","PDF","800x480","TTL","ST7262","Free V.A","CTP","-30℃~85℃","550 nits","115.40*79.15*19.81","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,UART TFT"]
["4.3”","KD043WQFPA042-01-C038A-CAN","PDF","480x272","CAN","SC7283","Free V.A","CTP","-30℃~85℃","950 nits","115.40*79.15*19.75","95.04*53.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["4.5”","KD045FWFPA010-01-C001B-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","61.54*110.09*19.10","55.44*98.64","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-RS232","PDF","480x854","RS232","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-RS485","PDF","480x854","RS485","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050FWFPA011-09-C009E-TTL","PDF","480x854","TTL","ILI9806E","Free V.A","CTP","-20℃~70℃","500 nits","67.56*122.35*20.00","61.63*109.65","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS232","PDF","720x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-RS485","PDF","720x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050HDFIA020-06-C020D-TTL","PDF","720x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~70℃","400 nits","78.56*135.65*20.00","62.10*110.40","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS232","PDF","800x480","RS232","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-RS485","PDF","800x480","RS485","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["5.0”","KD050WVTPA045-C003A-TTL","PDF","800x480","TTL","ILI5960/ILI6122","V.A 12H","CTP","-20℃~70℃","350 nits","132.72*87.80*20.50","108.00*64.80","Capacitive Touch Display,UART TFT"]
["6.2”","KD062VGFPD003-C002A-TTL","PDF","640x240","TTL","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS485","PDF","640x240","RS485","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.2”","KD062VGFPD003-C002A-RS232","PDF","640x240","RS232","ST5043AA/ST5894AA","Free V.A","CTP","-30℃~85℃","850 nits","173.80*82.76*19.71","148.80*53.76","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS232","PDF","800x480","RS232","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-RS485","PDF","800x480","RS485","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-TTL","PDF","800x480","TTL","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["6.8”","KD068WVFPD007-01-C003A-CAN","PDF","800x480","CAN","TBD","Free V.A","CTP","-30℃~85℃","1100 nits","155.96*100.77*22.24","148.10*88.86","Capacitive Touch Display,Wide Temp TFT,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-RS232","PDF","800x480","RS232","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-RS232","PDF","800x480","RS232","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-RS485","PDF","800x480","RS485","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070WVFPA043A-C049A-TTL","PDF","800x480","TTL","RM533C0+RM577C1","Free V.A","CTP","-20℃~70℃","1150 nits","165.40*104.59*23.00","152.40*91.44","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070C-4-05-C004A-RS485","PDF","800x480","RS485","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070C-4-05-C004A-TTL","PDF","800x480","TTL","EK9713/EK73002","V.A 12H","CTP","-20℃~70℃","400 nits","165.00*100.00*23.00","154.08*85.92","Capacitive Touch Display,UART TFT"]
["7.0”","KD070HDFPA038-C024A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.0”","KD070HDFPA038-C024A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","800 nits","182.07*117.60*24.00","154.21*85.92","Capacitive Touch Display,High-brightness TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS232","PDF","400x1280","RS232","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-RS485","PDF","400x1280","RS485","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["7.84”","KD078HDFPD002-C003A-TTL","PDF","400x1280","TTL","GC9704C","Free V.A","CTP","-20℃~70℃","900 nits","67.60*206.28*17.02","59.40*190.08","Capacitive Touch Display,High-brightness TFT,Bartype TFT,UART TFT"]
["8.0”","KD080WXFID015-C015A-RS232","PDF","800x1280","RS232","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-RS485","PDF","800x1280","RS485","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["8.0”","KD080WXFID015-C015A-TTL","PDF","800x1280","TTL","ILI9881C","Free V.A","CTP","-20℃~60℃","400 nits","130.70*200.10*13.59","107.64*172.22","Capacitive Touch Display,UART TFT"]
["9.0”","KD090HDFLA006-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["9.0”","KD090HDFLA006-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","No TP","-20℃~70℃","1000 nits","210.70*126.50*21.00","196.61*114.15","High-brightness TFT,UART TFT"]
["10.1”","KD101WSFPD036-C040A-RS232","PDF","1024x600","RS232","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-RS485","PDF","1024x600","RS485","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WSFPD036-C040A-TTL","PDF","1024x600","TTL","EK73215&EK79001","Free V.A","CTP","-20℃~70℃","550 nits","254.50*162.50*19.78","222.72*125.28","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-RS232","PDF","1280x800","RS232","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-RS485","PDF","1280x800","RS485","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]
["10.1”","KD101WXFLD021-C045C-TTL","PDF","1280x800","TTL","EK79202D_A","Free V.A","CTP","-20℃~70℃","400 nits","229.06*148.70*19.74","216.96*135.60","Capacitive Touch Display,UART TFT"]

{"sheet":"E-Paper Display","index":19,"n_rows":29,"n_cols":13,"rows_kept":29}
["STARTEK E-Paper Display 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["1.3”","KD013QCFSN015","PDF","144x200","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","24.69*36.64*0.95","19.44*27.00","E-Paper Display"]
["1.54”","KD015QVFSN012","PDF","152x152","SPI","SSD1681","Free V.A","No TP","0℃~50℃","0 nit","31.80*37.32*1.14","27.51*27.51","Square TFT,E-Paper Display"]
["1.54”","KD015QVFSN015","PDF","200x200","SPI","SSD1681","Free V.A","No TP","0℃~40℃","0 nit","31.80*37.32*1.00","27.00*27.00","Square TFT,E-Paper Display"]
["2.13”","KD021QVFSN006","PDF","122x250","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","29.20*59.20*1.00","23.70*48.55","E-Paper Display"]
["2.13”","KD021QVFSN005","PDF","122x250","SPI","UC8251","Free V.A","No TP","0℃~50℃","0 nit","29.20*59.20*1.14","23.70*48.55","E-Paper Display"]
["2.7”","KD027QVFSN007","PDF","152x296","SPI","UC8251","Free V.A","No TP","0℃~50℃","0 nit","36.30*71.82*1.14","30.70*60.09","E-Paper Display"]
["2.7”","KD027QVFSN008","PDF","152x296","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","36.30*71.82*0.90","30.70*60.09","E-Paper Display"]
["2.9”","KD029QVFSN005","PDF","128x296","SPI","SSD1680","Free V.A","No TP","0℃~40℃","0 nit","36.70*79.00*1.20","29.06*66.90","E-Paper Display"]
["2.9”","KD029QVFSN006","PDF","128x296","SPI","TBD","Free V.A","No TP","0℃~35℃","0 nit","36.70*79.00*1.14","29.06*66.90","E-Paper Display"]
["3.5”","KD035QVFBN212","PDF","240x360","SPI&MCU","UC8253","Free V.A","No TP","-20℃~60℃","0 nit","54.41*84.70*1.14","49.67*74.51","E-Paper Display"]
["3.5”","KD035QVFSN268","PDF","240x360","SPI","TBD","Free V.A","No TP","0℃~40℃","0 nit","54.41*84.70*0.85","49.67*74.51","E-Paper Display"]
["3.7”","KD037WQFSN002","PDF","240x416","SPI","UC8253","Free V.A","No TP","0℃~50℃","0 nit","53.00*92.99*1.14","47.04*81.54","E-Paper Display"]
["3.7”","KD037WQFSN003","PDF","240x416","SPI","UC8253","Free V.A","No TP","0℃~40℃","0 nit","53.00*92.99*0.90","47.04*81.54","E-Paper Display"]
["4.0”","KD040WVFSN077","PDF","480x800","SPI","SD8385","Free V.A","No TP","0℃~40℃","0 nit","56.24*96.62*0.81","51.84*86.40","E-Paper Display"]
["5.8”","KD058VGFSN005","PDF","640x480","SPI","TBD","Free V.A","No TP","0℃~50℃","0 nit","125.40*99.50*1.26","118.78*88.22","E-Paper Display"]
["6.0”","KD060HDFSN009","PDF","758x1024","Parallel","TBD","Free V.A","No TP","0℃~50℃","0 nit","101.80*138.40*0.93","90.58*122.37","E-Paper Display"]
["7.3”","KD073WVFSN001","PDF","800x480","SPI","0110-53000018","Free V.A","No TP","15℃~35℃","0 nit","170.20*111.20*1.00","160.00*96.00","E-Paper Display"]
["7.3”","KD073WVFSN002","PDF","800x480","SPI","TBD","Free V.A","No TP","0℃~40℃","0 nit","170.20*111.20*0.85","160.00*96.00","E-Paper Display"]
["7.5”","KD075WVFSN001","PDF","800x480","SPI","JD79686","Free V.A","No TP","0℃~40℃","0 nit","170.20*111.20*1.25","163.20*97.92","E-Paper Display"]
["7.8”","KD078FHFBN003","PDF","1404x1872","MCU","HH7163 T-Con","Free V.A","No TP","0℃~50℃","0 nit","127.60*173.80*0.86","118.64*158.18","E-Paper Display"]
["7.84”","KD078FHFBN009","PDF","1404x1872","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","127.60*173.80*0.81","118.64*158.18","E-Paper Display"]
["10.3”","KD103HDFMN005","PDF","2240x1680","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","216.70*174.40*0.71","209.67*157.25","E-Paper Display"]
["13.3”","KD133QHFSN014","PDF","960x680","SPI","SSD1677","Free V.A","No TP","0℃~40℃","0 nit","286.32*212.26*1.20","275.52*195.16","E-Paper Display"]
["13.3”","KD133UXFMN026","PDF","2200x1650","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","287.00*215.50*0.86","270.60*202.95","E-Paper Display"]
["31.2”","KD312HDFMN001","PDF","720x1280","MCU","TBD","Free V.A","No TP","0℃~50℃","0 nit","697.20*402.80*1.30","691.20*388.80","E-Paper Display"]

{"sheet":"LTPS TFT","index":20,"n_rows":77,"n_cols":13,"rows_kept":77}
["STARTEK LTPS TFT 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
[0,"Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["0.95”","KD0095OLEDN010","PDF","120x240","SPI","RM69310","Free V.A","No TP","-20℃~70℃","450 nits","12.80*27.35*0.74","10.80*21.60","AMOLED Display,Bartype TFT,LTPS Display"]
["1.0”","KD010LQOSN001-C0000","PDF","340x340","QSPI","SH8601","Free V.A","CTP","-10℃~60℃","630 nits","29.25*30.00*0.68","26.35*26.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN001-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","650 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,Round TFT,LTPS Display"]
["1.4”","KD014VGOSN003-C001A","PDF","466x466","QSPI","CO5300","Free V.A","CTP","-20℃~70℃","800 nits","40.86*51.97*2.76","36.35*36.35","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Round TFT,LTPS Display"]
["1.4”","KD014HVOIN011-C0000","PDF","320x360","MIPI","FT2390","Free V.A","CTP","-20℃~60℃","450 nits","25.74*29.87*0.79","23.84*26.82","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016HVOMN002-C001A","PDF","320x360","MIPI&SPI","RM69092","Free V.A","CTP","-20℃~70℃","320 nits","31.32*36.05*2.05","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.6”","KD016HVOQN006-C000O","PDF","320x360","QSPI","RM69092","Free V.A","CTP","-20℃~70℃","450 nits","28.92*33.35*0.76","27.02*30.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.78”","KD017HVOSN005-C000","PDF","368x448","QSPI/SPI","CO5300","Free V.A","CTP","-20℃~60℃","450 nits","33.50*40.89*2.58","28.70*34.94","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["1.96”","KD019HVOSN001-C001A","PDF","410x502","QSPI","CO5300AF-46","Free V.A","CTP","-10℃~60℃","600 nits","35.37*42.40*2.76","31.37*38.40","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","34.79*43.14*0.78","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOSN001-C001A","PDF","410x502","QSPI","CO5300","Free V.A","CTP","-20℃~60℃","500 nits","36.70*44.21*2.55","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002-C002B","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","550 nits","37.35*45.15*2.31","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.06”","KD020HVOIN002","PDF","410x502","MIPI","CO5300","Free V.A","CTP","-20℃~60℃","600 nits","34.79*43.14*0.83","33.09*40.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["2.4”","KD024WVFLD101","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024EGOIN148-C0000","PDF","450x600","SPI/MCU/MIPI","ICNA3312","Free V.A","CTP","-20℃~80℃","850 nits","38.68*51.56*0.73","36.72*48.96","Capacitive Touch Display,AMOLED Display,Wide Temp TFT,High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101A","PDF","800x480","LVDS","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFLD101A-C001A","PDF","800x480","LVDS","HX8283-A","Free V.A","CTP","-20℃~70℃","990 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102A","PDF","800x480","RGB","HX8283-A","Free V.A","No TP","-20℃~70℃","1100 nits","58.00*41.30*2.58","52.32*31.39","High-brightness TFT,LTPS Display"]
["2.4”","KD024WVFPD102A-C001A","PDF","800x480","RGB","HX8283-A","Free V.A","CTP","-20℃~70℃","950 nits","66.00*49.30*4.61","52.32*31.39","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["2.4”","KD024EGOIN152-01","PDF","450x600","MCU/MIPI","RM690B0","Free V.A","No TP","-20℃~80℃","800 nits","38.72*51.56*1.00","36.72*48.96","AMOLED Display,High-brightness TFT,LTPS Display"]
["2.5”","KD025EGOIN002-C000","PDF","400x712","MIPI","RM690C0","Free V.A","CTP","-20℃~70℃","800 nits","32.90*58.56*2.00","31.10*55.36","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["2.7”","KD027WVOIN011","PDF","800x600","MIPI","RM69700","Free V.A","No TP","-40℃~85℃","400 nits","56.60*47.25*1.50","54.60*40.95","AMOLED Display,Wide Temp TFT,LTPS Display"]
["2.9”","KD029FHOIN010","PDF","1080x1200","MIPI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*0.65","50.11*55.68","AMOLED Display,LTPS Display"]
["2.9”","KD029FHOIN010-HDMI","PDF","1080x1200","HDMI","RM67295","Free V.A","No TP","-20℃~60℃","400 nits","52.91*62.58*11.00","50.11*55.68","AMOLED Display,LTPS Display,HDMI AMOLED"]
["3.7”","KD037WVOPD004","PDF","480x800","RGB","TL2796","Free V.A","No TP","-30℃~80℃","250 nits","53.94*90.00*1.50","48.24*80.40","AMOLED Display,Wide Temp TFT,LTPS Display"]
["3.9”","KD039FHOIN003-01-C0000","PDF","1080x1240","MIPI","SD5302","Free V.A","CTP","-20℃~70℃","500 nits","67.25*79.87*0.80","65.45*75.14","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.0”","KD040FHFLD058-C041A","PDF","1920x1080","LVDS","SC5010","Free V.A","CTP","-20℃~70℃","1000 nits","104.87*72.22*4.76","88.59*49.83","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["4.0”","KD040FHFLD058","PDF","1920x1080","LVDS","SC5010","Free V.A","No TP","-20℃~70℃","1100 nits","94.87*62.22*2.73","88.59*49.83","High-brightness TFT,LTPS Display"]
["4.0”","KD040UXOIN109-C073A","PDF","1080x1200","MIPI","VTDR6130A","Free V.A","CTP","-20℃~70℃","600 nits","72.93*80.53*1.12","68.43*76.03","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.1”","KD041HDOIN002-C000","PDF","2480x1860","MIPI","RM69A10","Free V.A","CTP","-20℃~70℃","280 nits","48.24*100.84*2.64","43.55*94.47","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["4.3”","KD043OLEDN001","PDF","568x1210","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","600 nits","49.13*103.55*0.75","47.37*100.91","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050FHFLD102","PDF","1920x1080","LVDS","SC5010B","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.76*2.77","110.59*62.21","High-brightness TFT,LTPS Display"]
["5.0”","KD050FHFID103","PDF","1920x1080","MIPI","SC5010E","Free V.A","No TP","-20℃~70℃","1000 nits","116.59*72.67*2.77","110.59*62.20","High-brightness TFT,LTPS Display"]
["5.0”","KD050HDOIN116-C000","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C116B","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","70.52*123.12*1.67","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C000-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","64.12*116.72*10.80","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050HDOIN116-C116B-SP005A-HDMI","PDF","720x1280","HDMI","TBD","Free V.A","CTP","-20℃~70℃","300 nits","70.52*123.12*12.37","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.0”","KD050FHFLD102-01-C085B","PDF","1920x1080","LVDS","SC5010B","Free V.A","CTP","-20℃~70℃","950 nits","126.99*83.05*4.47","110.59*62.21","Capacitive Touch Display,High-brightness TFT,LTPS Display"]
["5.0”","KD050HDOIN132-C001","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.0”","KD050HDOIN116-C000-a","PDF","720x1280","MIPI","RM67295","Free V.A","CTP","-20℃~70℃","500 nits","64.12*116.72*0.94","61.88*110.02","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHFID018-01-C017A-SP003A-HDMI","PDF","1080x1920","HDMI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*19.74","68.04*120.96","Capacitive Touch Display,HDMI TFT,LTPS Display"]
["5.5”","KD055FHFID018-C017A","PDF","1080x1920","MIPI","HX8399-A","Free V.A","CTP","-20℃~70℃","350 nits","79.04*137.67*2.60","68.04*120.96","Capacitive Touch Display,LTPS Display"]
["5.5”","KD055FHOIN031-C0000","PDF","1080x1920","MIPI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.82","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["5.5”","KD055FHOIN030-C001-SP005A-HDMI","PDF","1080x1920","HDMI","RM67199","Free V.A","CTP","-20℃~70℃","350 nits","69.74*126.60*10.80","67.82*120.58","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["5.5”","KD055FHOIN031-C0000-HDMI","PDF","1080x1920","HDMI","CH13721C","Free V.A","CTP","-20℃~60℃","500 nits","70.36*127.34*0.83","68.26*121.34","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.0”","KD060FPOIN011-C0000","PDF","1080x2160","MIPI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.0”","KD060FPOIN011-C0000-HDMI","PDF","1080x2160","HDMI","CH13721C","Free V.A","CTP","-20℃~70℃","500 nits","70.07*142.30*0.78","68.26*136.51","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.4”","KD064FPOIN001-C0000","PDF","1080x2340","MIPI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["6.4”","KD064FPOIN001-C0000-HDMI","PDF","1080x2340","HDMI","SD5207","Free V.A","CTP","-20℃~70℃","500 nits","69.84*150.42*0.80","68.04*147.42","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["6.5”","KD065FPOIN003","PDF","1080x2400","MIPI","RM692E5","Free V.A","No TP","-20℃~70℃","500 nits","71.45*156.64*0.29","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display"]
["6.5”","KD065FPOIN003-HDMI","PDF","1080x2400","HDMI","TBD","Free V.A","No TP","-20℃~70℃","450 nits","71.45*156.64*11.00","69.55*154.56","AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["6.67”","KD067FPOIN004-C0000","PDF","1080x2400","MIPI","VTDR6130","Free V.A","CTP","-20℃~70℃","500 nits","71.53*200.59*0.33","69.55*154.56","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display"]
["7.0”","KD070FHOIN128-C0000","PDF","1080x1920","MIPI","ICNA3512","Free V.A","CTP","-20℃~70℃","950 nits","89.13*160.91*1.01","87.13*154.91","Capacitive Touch Display,AMOLED Display,High-brightness TFT,LTPS Display"]
["7.0”","KD070FHOIN124-C142A","PDF","1080x1920","MIPI","GD7658A V110","Free V.A","CTP","-30℃~85℃","900 nits","99.04*174.56*2.22","86.94*154.56","Capacitive Touch Display,AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-C000-a","PDF","2480x1860","MIPI","RM69380","Free V.A","CTP","-40℃~80℃","600 nits","165.69*137.92*0.34","162.69*122.02","AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["8.0”","KD080WQOIN035-CP001A-HDMI","PDF","2480x1860","HDMI","RM69380","Free V.A","CTP","-20℃~70℃","600 nits","165.69*137.92*13.60","162.69*122.02","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,LTPS Display,HDMI AMOLED"]
["13.3”","KD133QXFEN020","PDF","1536x2048","eDP","TBD","Free V.A","No TP","0℃~50℃","300 nits","213.80*284.80*0.53","202.75*270.34","AMOLED Display,Flexible AMOLED,LTPS Display"]
["14.0”","KD140FHFLD003","PDF","1920x1080","eDP","TBD","Free V.A","No TP","-20℃~70℃","800 nits","317.52*186.73*4.80","308.16*173.34","High-brightness TFT,LTPS Display"]
["14.0”","KD140FHFLD003-C003A","PDF","1920x1080","eDP","TBD","Free V.A","CTP","-20℃~70℃","700 nits","337.49*206.76*7.58","308.16*173.34","Capacitive Touch Display,LTPS Display"]
["14.2”","KD142QHOEN001-C001A","PDF","2650x1392","eDP","TBD","Free V.A","CTP","-40℃~85℃","650 nits","343.63*186.63*6.44","319.33*167.74","Capacitive Touch Display,AMOLED Display,Flexible AMOLED,Wide Temp TFT,LTPS Display"]
["15.1”","KD151WQOEN001-C0000","PDF","2560x1600","eDP","RM98121","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*1.30","324.10*202.56","AMOLED Display,High-brightness TFT,Wide Temp TFT,LTPS Display"]
["15.1”","KD151WQOEN001-SP001A-HDMI","PDF","2560x1600","HDMI","TBD","Free V.A","No TP","-40℃~85℃","800 nits","328.90*210.46*5.80","324.10*202.56","AMOLED Display,Wide Temp TFT,LTPS Display,HDMI AMOLED"]
["15.6”","KD156UHOEN018","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.48*201.62*1.05","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN025","PDF","3840x2160","eDP","RM98110","Free V.A","No TP","-20℃~70℃","400 nits","348.22*201.62*1.10","344.22*193.62","AMOLED Display,LTPS Display"]
["15.6”","KD156UHOEN018-C014A","PDF","3840x2160","eDP","RM98110","Free V.A","CTP","-20℃~70℃","320 nits","357.22*208.27*3.35","344.22*193.62","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003","PDF","3840x2160","eDP","TBD","Free V.A","No TP","-20℃~70℃","400 nits","607.66*348.18*1.24","597.66*336.18","AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B","PDF","3840x2160","eDP","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*4.19","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display"]
["27.0”","KD270UDOEN003-C002B-HDMI","PDF","3840x2160","HDMI","TBD","Free V.A","CTP","-20℃~70℃","400 nits","613.00*361.50*13.60","597.66*336.18","Capacitive Touch Display,AMOLED Display,LTPS Display,HDMI AMOLED"]
["27.0”","KD270QHOVD026","PDF","2560x1440","V-By-One","TBD","Free V.A","No TP","0℃~45℃","1300 nits","600.62*346.42*0.78","586.75*330.05","AMOLED Display,High-brightness TFT,LTPS Display"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,Display Monitor,OLED Monitor"]
["31.5”","KD320UHOVD017","PDF","3840x2160","V-By-One","TBD","Free V.A","No TP","0℃~45℃","230 nits","709.68*407.43*0.80","696.58*391.82","AMOLED Display,LTPS Display"]

{"sheet":"Curved Monitor","index":21,"n_rows":23,"n_cols":13,"rows_kept":23}
["STARTEK Curved Monitor 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["23.8”","KD238FHFVA010-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","583.17*356.46*70.95","524.37*298.46","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["27.0”","KD270FHFVA014-C004A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","402.11*660.90*82.60","336.31*593.43","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA006-C005A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","464.82*764.72*97.06","394.82*694.61","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA008-C006A-C1600-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","462.00*762.51*100.03","394.80*693.89","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA011-C1800-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","719.70*420.60*118.70","698.40*392.85","Curved Monitor,Display Monitor"]
["34.0”","KD340UWFVA001-C1500-Monitor","PDF","3440x1440","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","808.70*362.40*126.42","797.22*333.72","Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA009-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.01*992.60*133.87","530.15*925.79","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA010-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.25*1005.29*164.61","530.75*927.01","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA011-C003A-C1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1003.64*606.45*136.13","925.90*529.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA012-C004A-J1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1016.87*606.45*136.03","933.40*530.75","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA013-C005A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1028.43*619.42*63.40","941.18*529.42","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA006-C001A-C1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1134.82*122.65","605.03*1053.83","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA007-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1142.15*150.91","605.03*1064.95","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA008-C003A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1168.03*702.00*76.70","1085.50*604.00","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA020-C1500-Monitor","PDF","3840x1080","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","1200.00*360.00*43.00","--","Curved Monitor,Display Monitor"]
["55.0”","KD550WSFVA005-C002A-J1500-Monitor","PDF","3840x2160","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","772.40*1291.82*207.07","698.20*1227.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA006-C003A-C1800-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","756.80*1270.02*167.40","681.40*1174.66","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA007-C004A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1302.12*780.40*78.70","1209.60*680.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA011-C005A-S1200-Monitor","PDF","3840x2160","HDMI/DP/RS232","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","1293.10*833.40*48.30","1227.40*698.20","Capacitive Touch Display,Curved Monitor,Display Monitor"]

{"sheet":"Display Monitor","index":22,"n_rows":78,"n_cols":13,"rows_kept":78}
["STARTEK Display Monitor 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["7.0”","KD070HDFLA116-CTP-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","-10℃~60℃","550 nits","169.20*104.00*38.26","154.21*85.92","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD051-01-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","700 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101HDFLD053-C064A-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","293.00*194.00*62.00","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD051-CTP-Monitor","PDF","1280x800","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","350 nits","255.26*173.90*41.80","217.96*136.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WSFLD028-C040A-Monitor","PDF","1024x600","HDMI","TBD","Free V.A","CTP","0℃~50℃","320 nits","258.10*166.10*43.23","222.72*125.28","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101HDFLA060-CTP-Monitor","PDF","800x1280","HDMI","TBD","Free V.A","CTP","-10℃~60℃","500 nits","259.96*177.96*29.40","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.1”","KD101WXFLD021A-C072A-Monitor","PDF","1280x800","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","258.25*176.05*26.68","216.96*135.60","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104WVTLA009-CTP-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","750 nits","261.60*208.80*43.00","213.20*160.40","Capacitive Touch Display,Display Monitor"]
["10.4”","KD104HDFLA0018-C009A-Monitor","PDF","1024x768","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","350 nits","283.00*225.20*64.00","211.20*158.48","Capacitive Touch Display,Display Monitor"]
["11.6”","KD116WSFEA003-CTP-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","1000 nits","298.22*186.10*44.00","257.32*145.18","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["12.1”","KD121HDFLA015-CTP-Monitor","PDF","1024x768","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~50℃","850 nits","294.50*233.00*44.00","247.00*185.50","Capacitive Touch Display,High-brightness TFT,Display Monitor"]
["12.8”","KD128FHFLD003-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~40℃","650 nits","325.09*201.11*44.00","284.59*160.61","Display Monitor"]
["13.3”","KD133FHFLA013-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","300 nits","325.00*205.00*35.00","296.00*164.00","Display Monitor"]
["13.3”","KD133FHFLA015-C010A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","332.40*206.40*56.80","293.76*165.24","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156WSFEA016-01-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","300 nits","398.00*248.00*46.50","343.54*192.83","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFLA021-C011A-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~60℃","250 nits","376.40*236.40*43.20","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["15.6”","KD156FHFED024-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","-10℃~60℃","300 nits","388.55*240.98*41.00","344.16*193.59","Capacitive Touch Display,Display Monitor"]
["19.0”","KD190SXFLA007-01-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","710 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["19.0”","KD190SXFLA007-CTP-Monitor","PDF","1280x1024","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","270 nits","429.60*357.00*43.00","376.30*301.10","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215WSFVA009F-Monitor","PDF","1920x1080","HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","510 nits","523.64*315.11*59.30","475.64*267.11","Display Monitor"]
["21.5”","KD215WSFVA009E-Monitor","PDF","1920x1080","HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","500 nits","523.64*315.11*59.30","475.64*267.11","Display Monitor"]
["21.5”","KD215WSFVA017-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~45℃","550 nits","493.26*284.13*35.59","478.67*260.28","Display Monitor"]
["21.5”","KD215WSFVA018-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~45℃","710 nits","493.26*284.13*35.59","478.67*260.28","Display Monitor"]
["21.5”","KD215WSFVA011-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","400 nits","510.00*306.60*56.20","475.64*268.11","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215WSFVA009-Monitor","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~50℃","750 nits","532.20*319.40*46.50","479.60*270.90","Display Monitor"]
["21.5”","KD215WSFVA017A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","492.70*283.90*44.40","478.66*260.28","Display Monitor"]
["21.5”","KD215FHFLA023-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["21.5”","KD215FHFLA023-C007A-Monitor-TR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","546.00*341.50*26.50","482.00*273.60","Capacitive Touch Display,Display Monitor"]
["23.6”","KD236WSFLD002-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~50℃","180 nits","559.00*335.00*56.20","521.47*293.10","Capacitive Touch Display,Display Monitor"]
["23.6”","KD236WSFLD002-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~50℃","180 nits","559.00*335.00*56.20","521.47*293.10","Display Monitor"]
["23.8”","KD238FHFVA010-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","583.17*356.46*70.95","524.37*298.46","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["23.8”","KD238FHFVA011-C006A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~45℃","300 nits","598.00*370.00*58.00","529.00*297.50","Display Monitor"]
["23.8”","KD238FHFVA012-C007A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~45℃","300 nits","598.00*370.00*58.00","529.00*297.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270WSFLA004-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","180 nits","644.40*382.60*59.40","597.60*336.15","Display Monitor"]
["27.0”","KD270WSFLA004-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","180 nits","644.40*382.60*59.40","597.60*336.15","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270WSFLA005-CTP-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","300 nits","645.40*383.20*62.50","598.00*336.50","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270FHFVA014-C004A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","402.11*660.90*82.60","336.31*593.43","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["27.0”","KD270FHFVA020-C009A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","No TP","0℃~45℃","300 nits","678.00*420.00*58.00","598.00*343.00","Display Monitor"]
["27.0”","KD270FHFVA021-C010A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","678.00*420.00*58.00","598.00*343.00","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA017-C006A-Monitor","PDF","3840x2160","HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["27.0”","KD270UHFVA018-C007A-Monitor","PDF","3840x2160","HDMI/DP","TBD","Free V.A","No TP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Display Monitor"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,Display Monitor,OLED Monitor"]
["27.0”","KD270UHFVA016-C005A-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","679.20*417.40*54.90","596.70*335.60","Capacitive Touch Display,Display Monitor"]
["31.5”","KD315WSFVA002-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","No TP","0℃~50℃","210 nits","739.00*435.00*59.30","698.60*390.10","Display Monitor"]
["31.5”","KD315WSFVA002-ITP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","Infrared Ray TP","0℃~50℃","250 nits","756.70*451.30*59.00","698.60*392.10","Display Monitor"]
["31.5”","KD315WSFVA002-CTP-Monitor","PDF","1920x1080","HDMI/VGA","TBD","Free V.A","CTP","0℃~50℃","300 nits","748.60*451.20*51.00","698.60*392.10","Capacitive Touch Display,Display Monitor"]
["31.5”","KD315WSFVA005-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","290 nits","789.40*483.85*73.00","697.40*391.85","Display Monitor"]
["31.5”","KD315WSFVA006-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","300 nits","781.50*476.00*46.00","698.40*391.30","Display Monitor"]
["31.5”","KD315WSFVA003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","718.80*421.70*58.70","698.40*392.85","Display Monitor"]
["31.5”","KD315WSFVA003A-01-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","718.80*421.70*58.70","698.40*392.85","Display Monitor"]
["32.0”","KD320FHFUA003-C003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","CTP","0℃~40℃","400 nits","745.50*440.50*66.50","698.00*393.00","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320FHFVA006-C005A-C1500-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","464.82*764.72*97.06","394.82*694.61","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA008-C006A-C1600-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","462.00*762.51*100.03","394.80*693.89","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA011-C1800-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","719.70*420.60*118.70","698.40*392.85","Curved Monitor,Display Monitor"]
["32.0”","KD320FHFVA009-C008A-Monitor-BR","PDF","1920x1080","HDMI/DP","TBD","Free V.A","CTP","0℃~45℃","300 nits","463.90*769.40*54.90","394.80*700.40","Capacitive Touch Display,Display Monitor"]
["32.0”","KD320UHFVA007-C007A-Monitor","PDF","3840x2160","HDMI/DP/USB","TBD","Free V.A","CTP","0℃~40℃","300 nits","789.00*485.00*58.20","697.30*392.20","Capacitive Touch Display,Display Monitor"]
["34.0”","KD340UWFVA001-C1500-Monitor","PDF","3440x1440","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","808.70*362.40*126.42","797.22*333.72","Curved Monitor,Display Monitor"]
["42.5”","KD425WSFVA003A-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","955.20*556.21*94.45","940.90*529.25","Display Monitor"]
["43.0”","KD430UHFVA009-C001A-C1650-Monitor","PDF","1920x1080","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.01*992.60*133.87","530.15*925.79","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA010-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","599.25*1005.29*164.61","530.75*927.01","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA011-C003A-C1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1003.64*606.45*136.13","925.90*529.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430UHFVA012-C004A-J1500-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1016.87*606.45*136.03","933.40*530.75","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["43.0”","KD430FHFVA014-C006A-Monitor-BR","PDF","1920x1080","VGA/HDMI/DP","TBD","Free V.A","CTP","0℃~40℃","300 nits","1007.70*595.40*53.60","943.10*529.80","Capacitive Touch Display,Display Monitor"]
["43.0”","KD430UHFVA013-C005A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1028.43*619.42*63.40","941.18*529.42","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA006-C001A-C1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1134.82*122.65","605.03*1053.83","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA007-C002A-J1650-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","680.73*1142.15*150.91","605.03*1064.95","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA008-C003A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1168.03*702.00*76.70","1085.50*604.00","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["49.0”","KD490UHFVA020-C1500-Monitor","PDF","3840x1080","HDMI/DP","RTD2775","Free V.A","No TP","0℃~40℃","300 nits","1200.00*360.00*43.00","--","Curved Monitor,Display Monitor"]
["55.0”","KD550WSFVA001-Monitor","PDF","1920x1080","HDMI","TBD","Free V.A","No TP","0℃~45℃","450 nits","1251.00*722.00*59.30","1210.60*677.10","Display Monitor"]
["55.0”","KD550WSFVA002A-Monitor","PDF","3840x2160","HDMI","TBD","Free V.A","No TP","0℃~45℃","500 nits","1225.70*705.60*82.30","1209.60*680.40","Display Monitor"]
["55.0”","KD550WSFVA005-C002A-J1500-Monitor","PDF","3840x2160","VGA/HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","772.40*1291.82*207.07","698.20*1227.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA006-C003A-C1800-Monitor","PDF","3840x2160","HDMI/VGA","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","756.80*1270.02*167.40","681.40*1174.66","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA007-C004A-J1500-Monitor","PDF","3840x2160","HDMI/DP","RTD2775","Free V.A","CTP","0℃~40℃","300 nits","1302.12*780.40*78.70","1209.60*680.40","Capacitive Touch Display,Curved Monitor,Display Monitor"]
["55.0”","KD550UHFVA011-C005A-S1200-Monitor","PDF","3840x2160","HDMI/DP/RS232","RTD2775","Free V.A","CTP","0℃~40℃","400 nits","1293.10*833.40*48.30","1227.40*698.20","Capacitive Touch Display,Curved Monitor,Display Monitor"]

{"sheet":"OLED Monitor","index":23,"n_rows":5,"n_cols":13,"rows_kept":5}
["STARTEK OLED Monitor 2026"]
["Notes：★The catalogue is updated twice a month."]
["Updated",null,{"$f":"TODAY()","v":"2026-02-10"}]
["Size","Part No.","Datasheet","Resolution","Interface","Driver","Viewing Angle","Touch","Temperature","Brightness","Dimension(mm)","Active Area(mm)","Feature"]
["27.0”","KD270QHOVD027-Monitor","PDF","2560x1440","HDMI/DP/Type-C/USB","TBD","Free V.A","No TP","0℃~45℃","1000 nits","604.42*350.62*57.85","590.42*333.72","AMOLED Display,High-brightness TFT,LTPS Display,OLED Monitor"]